{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["instructions","calculator","rims","hubs","Module1"],"not_rendered":{"charts":0,"images":4,"macros":1,"external_links":1,"defined_names":30,"comments":2,"pivot_tables":0},"unopened":[{"sheet":"Module1","index":4,"reason":"part_missing"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"instructions","index":0,"n_rows":27,"n_cols":1,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
["Spocalc"]
["Spocalc.xls is an Excel workbook I (Damon Rinard) made.  It has been updated to work with Excel 2016 my Matt Armbruster.  It works like any other Excel workbook.  There is no program beyond the built-in brains of Excel, just some formulas that automatically work on the numbers you enter to instantly give you the spoke lengths you need."]
[]
["Spocalc.xls contains four Excel worksheets: \"instructions\" (this sheet), \"calculator\", \"hubs\" and \"rims\".  Once you've opened spocalc.xlsm in Excel, you can look at any worksheet by clicking on its tab at the bottom of the screen.  Instructions on how to use the macros to enter hub and rim data are on the \"hubs\" and \"rims\" worksheets."]
[]
["The \"calculator\" worksheet is where you enter the rim and hub dimensions and view the results of the calculations. If you click on a cell containing the spoke length, you can view the formulas in the Formula Bar near the top of the worksheet."]
[]
["The \"rims\" worksheet is a list of dimensions you can use for rims, or you can measure your own rim and add it to the list if you want."]
[]
["The \"hubs\" worksheet is a list of hubs you can choose from, or again, you can measure your own hub and add it to the list if you want."]
[]
["Here's how to use the Spocalc:"]
["1. Make sure you enable the macros. (Often Excel prompts you to disable them in case they harbor a virus.) You can enable the macros when you open the file by clicking on the \"Enable Macros\" button when Excel asks."]
[]
["2. On the calculator sheet, click on the \"Choose\" buttons on the left and Spocalc will take you to the rims or hubs database."]
[]
["3. Select the name of the hub or rim you want by clicking on the cell containing its Name."]
[]
["4. Click on the appropriate \"Select\" button to send the data to the calculator worksheet."]
[]
[]
["This workbook as well as other versions are online at"]
["http://sheldonbrown.com/rinard/spocalc.htm"]
[]
["Please contact sheldonbrown.com if you have additons, corrections, questions or other feedback."]
[]
["Thank you Sheldon Brown, Doug Milliken, Greg Johnson, Larry Friedman, and Clark Rasmussen for your invaluable help in developing this spreadsheet -- Damon Rinard"]

{"sheet":"calculator","index":1,"n_rows":46,"n_cols":13,"rows_kept":46,"cut":false,"hidden":false,"merged":[[9,3,9,5],[24,3,24,5]]}
[null,"Spocalc-2022",null,"http://sheldonbrown.com/rinard/spocalc.htm"]
[null,"Today is",{"$f":"TODAY()","v":"2022-01-28"}]
[1,"Click on \"Choose\" buttons for hub and rim dimensions.  You can also edit or add to those dimensions."]
[2,"Enter \"N, total number of spokes\"."]
[3,"(Optional) Enter rim and hub dimensions manually by typing them in the yellow \"Input\" cells (column C)."]
[4,"(Optional) Enter \"X, number of cross\". You may enter a decimal value if desired."]
[5,"Spoke lengths for various cross patterns are immediately displayed in columns E and F."]
[6,"(Optional) Print this page by choosing Print from the File menu."]
[]
[null,"Front Wheel","Input Data","Output Data",null,null,"Reference information:",null,null,null,"Note:"]
[null,{"$f":"\"Hub: \" &C40","v":"Hub: AC APX"}]
[null,{"$f":"\"Rim: \"&C41","v":"Rim: Ambrosio aero (with washers)"}]
[null,"N, total number of spokes",28,"cross","left length","right length","left bracing angle","right bracing angle",null,null,"If paired hub spoke holes are 15 degrees apart, then:"]
[null,"ERD, effective rim diameter",604,0,{"$f":"SQRT((C$18/2*SIN(2*PI()*D14/(C$13/2)))^2+(C$14/2-((C$18/2)*COS(2*PI()*D14/(C$13/2))))^2+D$22^2)-C$20/2","v":281.74869280743906},{"$f":"SQRT((C$19/2*SIN(2*PI()*D14/(C13/2)))^2+(C$14/2-((C$19/2)*COS(2*PI()*D14/(C13/2))))^2+D$23^2)-C$20/2","v":281.74869280743906},{"$f":"CONCATENATE(ROUND(DEGREES(ASIN($D$22/E14))-3.5/2,1),\" heads out; \",ROUND(DEGREES(ASIN($D$22/E14))+3.5/2,1), \" heads in\")","v":"5.6 heads out; 9.1 heads in"},{"$f":"CONCATENATE(ROUND(DEGREES(ASIN($D$23/F14))-3.5/2,1),\" heads out; \",ROUND(DEGREES(ASIN($D$23/F14))+3.5/2,1), \" heads in\")","v":"5.6 heads out; 9.1 heads in"},"Tension L/R",null,"For 24 paired spokes laced 2x, enter 2.25 cross."]
[null,"OSB, offset spoke bed",0,1,283.98516799944656,{"$f":"SQRT((C$19/2*SIN(2*PI()*D15/(C13/2)))^2+(C$14/2-((C$19/2)*COS(2*PI()*D15/(C13/2))))^2+D$23^2)-C$20/2","v":283.98516799944656},{"$f":"DEGREES(ASIN($D$22/E15))","v":7.2828198891822113},{"$f":"DEGREES(ASIN($D$23/F15))","v":7.2828198891822113},{"$f":"SIN(RADIANS(G15))/SIN(RADIANS(H15))","v":1},null,"For 24 paired spokes laced 1x, enter 1.25 cross."]
[null,"WL, width from center to left flange",36,2,290.16023895746594,{"$f":"SQRT((C$19/2*SIN(2*PI()*D16/(C13/2)))^2+(C$14/2-((C$19/2)*COS(2*PI()*D16/(C13/2))))^2+D$23^2)-C$20/2","v":290.16023895746594},{"$f":"DEGREES(ASIN($D$22/E16))","v":7.1270166483951201},{"$f":"DEGREES(ASIN($D$23/F16))","v":7.1270166483951201},{"$f":"SIN(RADIANS(G16))/SIN(RADIANS(H16))","v":1},null,"For 20 paired spokes laced 2x, enter 2.29 cross."]
[null,"WR, width from center to right flange",36,3,298.85913498121408,{"$f":"SQRT((C$19/2*SIN(2*PI()*D17/(C13/2)))^2+(C$14/2-((C$19/2)*COS(2*PI()*D17/(C13/2))))^2+D$23^2)-C$20/2","v":298.85913498121408},{"$f":"DEGREES(ASIN($D$22/E17))","v":6.9185408708650886},{"$f":"DEGREES(ASIN($D$23/F17))","v":6.9185408708650886},{"$f":"SIN(RADIANS(G17))/SIN(RADIANS(H17))","v":1},null,"For 20 paired spokes laced 1x, enter 1.29 cross."]
[null,"dL, left flange diameter",42.5,4,308.22805799689519,{"$f":"SQRT((C$19/2*SIN(2*PI()*D18/(C13/2)))^2+(C$14/2-((C$19/2)*COS(2*PI()*D18/(C13/2))))^2+D$23^2)-C$20/2","v":308.22805799689519},{"$f":"DEGREES(ASIN($D$22/E18))","v":6.7072630766692898},{"$f":"DEGREES(ASIN($D$23/F18))","v":6.7072630766692898},{"$f":"SIN(RADIANS(G18))/SIN(RADIANS(H18))","v":1},null,"For 16 paired spokes laced 1x, enter 1.33 cross."]
[null,"dR, right flange diameter",42.5,{"$f":"C21","v":3},298.85913498121408,{"$f":"SQRT((C$19/2*SIN(2*PI()*D19/(C13/2)))^2+(C$14/2-((C$19/2)*COS(2*PI()*D19/(C13/2))))^2+D$23^2)-C$20/2","v":298.85913498121408},{"$f":"DEGREES(ASIN($D$22/E19))","v":6.9185408708650886},{"$f":"DEGREES(ASIN($D$23/F19))","v":6.9185408708650886},{"$f":"SIN(RADIANS(G19))/SIN(RADIANS(H19))","v":1}]
[null,"S, spoke hole diameter",2.6,null,null,null,null,null,null,null,"If paired hub spoke holes are 20 degrees apart, then:"]
[null,"X, cross number (decimal allowed)(optional)",3,null,null,null,null,null,null,null,"For 16 paired spokes laced 1x, enter 1.275 cross."]
[null,"WL_effective = W + OSB",null,{"$f":"C16+C15","v":36}]
[null,"WR_effective = W - OSB",null,{"$f":"C17-C15","v":36}]
[]
[null,"Rear Wheel","Input Data","Output Data",null,null,"Reference information:"]
[null,{"$f":"\"Hub: \"&C43","v":"Hub: AC APX"}]
[null,{"$f":"\"Rim: \"&C44","v":"Rim: Ambrosio Crono"}]
[null,"N, total number of spokes",36,"cross","left length","right length","left bracing angle","right bracing angle"]
[null,"ERD, effective rim diameter",615,0,{"$f":"SQRT((C$33/2*SIN(2*PI()*D29/(C$28/2)))^2+(C$29/2-((C$33/2)*COS(2*PI()*D29/(C$28/2))))^2+D$37^2)-C$35/2","v":284.35232363836985},{"$f":"SQRT((C$34/2*SIN(2*PI()*D29/(C$28/2)))^2+(C$29/2-((C$34/2)*COS(2*PI()*D29/(C$28/2))))^2+D$38^2)-C$35/2","v":282.90459179964},{"$f":"CONCATENATE(ROUND(DEGREES(ASIN($D$37/E29))-3.5/2,1),\" heads out; \",ROUND(DEGREES(ASIN($D$37/E29))+3.5/2,1), \" heads in\")","v":"5.3 heads out; 8.8 heads in"},{"$f":"CONCATENATE(ROUND(DEGREES(ASIN($D$38/F29))-3.5/2,1),\" heads out; \",ROUND(DEGREES(ASIN($D$38/F29))+3.5/2,1), \" heads in\")","v":"2.3 heads out; 5.8 heads in"},"Tension R/L",null,"Tension ratio calc","Input","Output"]
[null,"OSB, offset spoke bed",0,1,285.90617492874344,284.46631522487041,{"$f":"DEGREES(ASIN($D$37/E30))","v":7.0316603167495453},{"$f":"DEGREES(ASIN($D$38/F30))","v":4.0316258734563153},{"$f":"SIN(RADIANS(H30))/SIN(RADIANS(G30))","v":0.57432092433507054},null,"left bracing angle",6.5]
[null,"WL, width from center to left flange",35,2,290.33407554598944,288.91618497176182,{"$f":"DEGREES(ASIN($D$37/E31))","v":6.9238908586684005},{"$f":"DEGREES(ASIN($D$38/F31))","v":3.969430694807917},{"$f":"SIN(RADIANS(H31))/SIN(RADIANS(G31))","v":0.57423292517342006},null,"right bracing angle",4.5999999999999996]
[null,"WR, width from center to right flange",20,3,296.99054627996509,295.60444590810692,{"$f":"DEGREES(ASIN($D$37/E32))","v":6.7679709057805706},{"$f":"DEGREES(ASIN($D$38/F32))","v":3.8794803989573721},{"$f":"SIN(RADIANS(H32))/SIN(RADIANS(G32))","v":0.57410802150556306},null,"Tension L/R",null,{"$f":"SIN(RADIANS(L31))/SIN(RADIANS(L30))","v":0.70845094992873281}]
[null,"dL, left flange diameter",48,4,304.9583923709456,303.60851562007264,{"$f":"DEGREES(ASIN($D$37/E33))","v":6.5903450568386104},{"$f":"DEGREES(ASIN($D$38/F33))","v":3.7770547358780941},{"$f":"SIN(RADIANS(H33))/SIN(RADIANS(G33))","v":0.57396920551381947}]
[null,"dR, right flange diameter",48,{"$f":"C36","v":3},296.99054627996509,295.60444590810692,{"$f":"DEGREES(ASIN($D$37/E34))","v":6.7679709057805706},{"$f":"DEGREES(ASIN($D$38/F34))","v":3.8794803989573721},{"$f":"SIN(RADIANS(H34))/SIN(RADIANS(G34))","v":0.57410802150556306}]
[null,"S, spoke hole diameter",2.6]
[null,"X, cross number (decimal allowed)(optional)",3]
[null,"WL_effective = W - OSB",null,{"$f":"C31-C30","v":35}]
[null,"WR_effective = W + OSB",null,{"$f":"C32+C30","v":20}]
[]
[null,"Front hub is","AC APX"]
[null,"Front rim is","Ambrosio aero (with washers)"]
[]
[null,"Rear hub is","AC APX"]
[null,"Rear rim is","Ambrosio Crono"]
[]
[null,"Notes:"]

{"sheet":"rims","index":2,"n_rows":1007,"n_cols":7,"rows_kept":1007,"cut":false,"hidden":false,"merged":[]}
["ERD is the Effective Rim Diameter.  "]
["ERD is measured to the end of the spoke, usually flush with the head of the nipple.",null,null,null,null,null,"OSB = (W/2) - L"]
["OSB is the lateral spoke bed offset (from wheel center). Non-zero for asymmetric rims."]
["size is the nominal size of the wheel, and usually does not correspond to any particular dimension."]
["ISO is the diameter of the bead seat of the rim, in millimeters. "]
["(See http://www.sheldonbrown.com/tire_sizing.html for more on ISO dimension.)"]
[]
["ERD","OSB, mm","size","ISO, mm",null,"date","by"]
[604,0,"700C","tubular","Ambrosio aero (with washers)"]
[615,0,"700C","tubular","Ambrosio Crono"]
[601.5,0,"700C","tubular","Ambrosio Excellence","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[618,0,"700C","tubular","Ambrosio Formula 20 Crono - MEASURE TO BE SURE"]
[610,0,"700C","tubular","Ambrosio Crono F.20 - MEASURE TO BE SURE","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[618,0,"700C","tubular","Ambrosio Metamorphosis"]
[618,0,"700C","tubular","Ambrosio Montreal - MEASURE TO BE SURE!"]
[610.5,0,"700C","tubular","Ambrosio Montreal - MEASURE TO BE SURE!","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[617,0,"700C","tubular","Ambrosio Nemesis"]
[610.5,0,"700C","tubular","Ambrosio Nemesis 2000","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[618,0,"700C","tubular","Ambrosio Synthesis"]
[594,0,"700C","tubular","Ambrosio Thesis","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[605,0,"700C","tubular","Ambrosio Tour de France","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[567,0,"700C","tubular","American Classic carbon fiber V rim"]
[618,0,"700C","tubular","Araya 16B Gold"]
[618,0,"700C","tubular","Araya 16B Red"]
[618,0,"700C","tubular","Araya 16BGOLDNEW track, classic tub, 335g","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[609,0,"700C","tubular","Araya ADX-1"]
[607,0,"700C","tubular","Araya ADX-2"]
[611,0,"700C","tubular","Araya ADX-4"]
[611,0,"700C","tubular","Araya ADX-5"]
[606.29999999999995,0,"700C","tubular","Araya NEWADX-1S","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[619,0,"700C","tubular","Araya Pro Staff 340"]
[619,0,"700C","tubular","Araya Pro Staff 400"]
[618,0,"700C","tubular","Araya R-50, classic tub, 415g","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[581.4,0,"700C","tubular","Araya SA-230S Super Aero (30mm deep)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[618,0,"700C","tubular","Araya Tita-Ace"]
[{"$f":"592+3","v":595},0,"700C","tubular","Bontrager PN 220042 Race X-Lite alu","2002-03-07","DGR"]
[{"$f":"557+30","v":587},0,"700C","tubular","Bontrager PN 221065 Race X-Lite OCLV Carbon Aero","2002-02-18","dcg"]
[{"$f":"595+3","v":598},1.5,"700C","tubular","Bontrager PN 221636 Race X-Lite alu OSB","2002-03-07","DGR"]
[{"$f":"592+3","v":595},0,"700C","tubular","Bontrager PN 231573 Race X-Lite alu, new wider rim","2002-06-05","DGR"]
[{"$f":"595+3","v":598},1.5,"700C","tubular","Bontrager PN 231574 Race X-Lite alu OSB, new wider rim","2002-06-05","DGR"]
[616,0,"700C","tubular","Campagnolo Barcelona '92 (12mm tall)"]
[609,0,"700C","tubular","Campagnolo Barcelona '92 (15mm tall)","2006-12-02","Knoch, Andreas <A.Knoch@FAZ-INSTITUT.DE>"]
[617,0,"700C","tubular","Campagnolo Delta (box section)"]
[617,0,"700C","tubular","Campagnolo Lambda (box section)"]
[615,0,"700C","tubular","Campagnolo Los Angeles '84 "]
[617,0,"700C","tubular","Campagnolo Omega (box section)"]
[617,0,"700C","tubular","Campagnolo Record (box section)"]
[602,0,"700C","tubular","Campagnolo Seoul '88 "]
[617,0,"700C","tubular","Campagnolo Sigma (box section)"]
[616,0,"700C","tubular","Campagnolo strada "]
[603,0,"700C","tubular","Campagnolo V profile "]
[617,0,"700C","tubular","Campagnolo Victory (box section)"]
[617,0,"700C","tubular","Fiamme Ergal (Yellow Label)"]
[617,0,"700C","tubular","Fiamme Ergal-Iride"]
[615,0,"700C","tubular","Fiamme Hard Silver"]
[617,0,"700C","tubular","Fiamme Master"]
[617,0,"700C","tubular","Fiamme Red Label"]
[617,0,"700C","tubular","Fiamme Speedy (track)"]
[615,0,"700C","tubular","Fiamme Super Corsa"]
[617,0,"700C","tubular","FiR Alkor"]
[562,0,"700C","tubular","FiR Antara 2000"]
[617,0,"700C","tubular","FiR Isidis"]
[617,0,"700C","tubular","FiR Pulsar"]
[617,0,"700C","tubular","FiR Quasar"]
[617,0,"700C","tubular","FiR Sirus"]
[616,0,"700C","tubular","FiR ST120 (400g)"]
[616,0,"700C","tubular","FiR ST120L (340g)"]
[572,0,"700C","tubular","LEW Composite",null,"www.bicycleracewheels.com"]
[611,0,"700C","tubular","Matrix Iso "]
[615,0,"700C","tubular","Mavic Argent 10"]
[616,0,"700C","tubular","Mavic Argent 12 SSC"]
[615,0,"700C","tubular","Mavic Argent 7"]
[615,0,"700C","tubular","Mavic Argent 8"]
[616,0,"700C","tubular","Mavic Bleu SSC"]
[616,0,"700C","tubular","Mavic CX18"]
[{"$f":"584+3","v":587},0,"700C","tubular","Mavic CXP30 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[615,0,"700C","tubular","Mavic GEL280"]
[615,0,"700C","tubular","Mavic GL330"]
[{"$f":"609+3","v":612},0,"700C","tubular","Mavic GP4 new angular (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[615,0,"700C","tubular","Mavic GP4 old rounder"]
[604,0,"700C","tubular","Mavic Mach 2CD2 "]
[603,0,"700C","tubular","Mavic Mach2"]
[616,0,"700C","tubular","Mavic Montlhery Pro"]
[615,0,"700C","tubular","Mavic OR7"]
[{"$f":"612+3","v":615},0,"700C","tubular","Mavic Paris Roubaix SSC (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[617,0,"700C","tubular","Mavic Piste (track)"]
[613,0,"700C","tubular","Mavic Reflex -- MEASURE TO BE SURE!!!"]
[616,0,"700C","tubular","Mavic Reflex -- MEASURE TO BE SURE!!!"]
[613,0,"700C","tubular","Mavic Reflex -- MEASURE TO BE SURE!!!"]
[616,0,"700C","tubular","Mavic Reflex -- MEASURE TO BE SURE!!!"]
[613,0,"700C","tubular","Mavic Reflex -- MEASURE TO BE SURE!!!"]
[616,0,"700C","tubular","Mavic Reflex -- MEASURE TO BE SURE!!!"]
[617,0,"700C","tubular","Nisi AN-85"]
[617,0,"700C","tubular","Nisi Countach"]
[618,0,"700C","tubular","Nisi G-27"]
[618,0,"700C","tubular","Nisi Sludi Mod 290"]
[618,0,"700C","tubular","Nisi Sludi Mod 320"]
[617,0,"700C","tubular","Nisi Solidal"]
[603,0,"700C","tubular","Performance A19T "]
[608.1,0,"700C","tubular","Rolf Vector Pro, Araya made. For Greer internal nipples + 4mm washers","2002-03-03","DGR"]
[603.70000000000005,0,"700C","tubular","Rolf Vector Pro, Trek made. For Greer internal nipples, no washers","2002-03-03","DGR"]
[608,0,"700C","tubular","Saavedra aero"]
[618,0,"700C","tubular","Saturae:  All greay anodized models"]
[556,0,"700C","tubular","Sun Buzz Road (carbon, alu brake track)"]
[556,0,"700C","tubular","Sun Buzz Special Event (carbon, no brake track)"]
[613,0,"700C","tubular","Sun M17A (tubular)"]
[604,0,"700C","tubular","Sun M19A"]
[602,0,"700C","tubular","Sun M19AII (632 mm OD)"]
[614,0,"700C","tubular","Sun M20B"]
[602,0,"700C","tubular","Velocity Escape 19mm x 19mm"]
[582,0,"700C","tubular","Velocity Pro/Elite"]
[614,0,"700C","tubular","Wolber Aspin "]
[611,0,"700C","tubular","Wolber Profil 18 "]
[600,0,"700C","tubular","Wolber Profil 20 "]
[608,0,"700C","tubular","Wolber Profil A "]
[616,0,"700C","tubular","Wolber/Super Champion Arc-en-ciel"]
[616,0,"700C","tubular","Wolber/Super Champion Aspin"]
[616,0,"700C","tubular","Wolber/Super Champion Aubisque"]
[616,0,"700C","tubular","Wolber/Super Champion Competition"]
[616,0,"700C","tubular","Wolber/Super Champion Medaile d'Or"]
[614,0,"700C","tubular","Zipp 140 12mm deep box section aluminum tubular"]
[596,0,"700C","tubular","Zipp 250 24.8mm deep carbon tubular","2005-06-16","Zipp"]
[569,0,"700C","tubular","Zipp 280 38mm deep carbon tubular ","2005-06-17","Kuthan.Kan@egco.com"]
[566,0,"700C","tubular","Zipp 340 38mm deep carbon tubular"]
[530,0,"700C","tubular","Zipp 360 58mm deep carbon tubular","2005-06-17","Kuthan.Kan@egco.com"]
[484,0,"700C","tubular","Zipp 420 82mm deep carbon tubular","2005-06-17","Kuthan.Kan@egco.com"]
[530,0,"700C","tubular","Zipp 440 58mm deep carbon tubular"]
[532,0,"650C","tubular","Accel "]
[559,0,"650C","tubular","Ambrosio Crono F.20 - MEASURE TO BE SURE","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[560,0,"650C","tubular","Ambrosio Montreal - MEASURE TO BE SURE!","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[520,0,"650C","tubular","American Classic carbon fiber V rim"]
[558,0,"650C","tubular","Araya ADX-4"]
[553.29999999999995,0,"650C","tubular","Araya NEWADX-1S","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[563.4,0,"650C","tubular","Araya R-50","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[530,0,"650C","tubular","Araya SA-230S Super Aero (30mm deep)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[568,0,"650C","tubular","Campagnolo strada "]
[565,0,"650C","tubular","FiR Alkor",null,"Mark Hoskin, FiRUSA@aol.com"]
[511,0,"650C","tubular","FiR Antara 2000"]
[522,0,"650C","tubular","LEW Composite",null,"www.lew-usa.com"]
[577,0,"650C","tubular","Mavic CX18 "]
[576,0,"650C","tubular","Mavic GL330 "]
[563,0,"650C","tubular","Mavic Mach 2 "]
[557,0,"650C","tubular","Mavic Mach 2CD2 "]
[530.4,0,"650C","tubular","Rolf Vector Carbon, Lew made. For Greer internal nipples + 2.5mm washers","2002-05-06","DGR"]
[553,0,"650C","tubular","Rolf Vector Pro, Araya made. For Greer internal nipples + 4mm washers","2002-03-03","DGR"]
[553,0,"650C","tubular","Rolf Vector Pro, Trek made. For Greer internal nipples, no washers","2002-03-03","DGR"]
[558,0,"650C","tubular","Saavedra aero"]
[507,0,"650C","tubular","Sun Buzz Road (carbon, alu brake track)"]
[507,0,"650C","tubular","Sun Buzz Special Event (carbon, no brake track)"]
[560,0,"650C","tubular","Sun M17A (582 mm OD)"]
[552,0,"650C","tubular","Sun M19A, M19AII (582 mm OD)"]
[560,0,"650C","tubular","Sun M20B (582 mm OD)"]
[554,0,"650C","tubular","Velocity Escape 19mm x 19mm"]
[531,0,"650C","tubular","Velocity Pro/Elite"]
[558,0,"650C","tubular","Wolber Profil 18 "]
[550,0,"650C","tubular","Wolber Profil 20 "]
[521,0,"650C","tubular","Zipp 245 38mm deep carbon tubular","2005-11-05","Kuthan.Kan@egco.com"]
[520,0,"650C","tubular","Zipp 310 38mm deep carbon tubular"]
[484,0,"650C","tubular","Zipp 330 58mm deep carbon tubular","2005-11-05","Kuthan.Kan@egco.com"]
[482,0,"650C","tubular","Zipp 400 58mm deep carbon tubular"]
[{"$f":"24.5*25.4","v":622.29999999999995},0,"28\"","tubular","Wood, unknown make, vintage 1900 or so."]
[481,0,"24\"","tubular","Accel "]
[506,0,"24\"","tubular","Araya ADX-4"]
[503.2,0,"24\"","tubular","Araya NEWADX-1S","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[478.2,0,"24\"","tubular","Araya SA-230S Super Aero (30mm deep)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[517,0,"24\"","tubular","Mavic CX18 "]
[517,0,"24\"","tubular","Mavic GL330 "]
[504,0,"24\"","tubular","Mavic Mach 2 "]
[509,0,"24\"","tubular","Sun M17A (MEASURE TO BE SURE!)"]
[512,0,"24\"","tubular","Sun M17A (MEASURE TO BE SURE!)"]
[509,0,"24\"","tubular","Sun M17A (MEASURE TO BE SURE!)"]
[512,0,"24\"","tubular","Sun M17A (MEASURE TO BE SURE!)"]
[509,0,"24\"","tubular","Sun M17A (MEASURE TO BE SURE!)"]
[512,0,"24\"","tubular","Sun M17A (MEASURE TO BE SURE!)"]
[502,0,"24\"","tubular","Sun M19A "]
[503,0,"24\"","tubular","Sun M19AII (532 mm OD)"]
[511,0,"24\"","tubular","Wolber Profil 18 "]
[409,0,"20\"","tubular","Araya NEWADX-1S","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[411,0,"20\"","tubular","Sun M17A (MEASURE TO BE SURE!)"]
[441,0,"20\"","tubular","Sun M17A (MEASURE TO BE SURE!)"]
[411,0,"20\"","tubular","Sun M17A (MEASURE TO BE SURE!)"]
[441,0,"20\"","tubular","Sun M17A (MEASURE TO BE SURE!)"]
[411,0,"20\"","tubular","Sun M17A (MEASURE TO BE SURE!)"]
[441,0,"20\"","tubular","Sun M17A (MEASURE TO BE SURE!)"]
[402,0,"20\"","tubular","Sun M19A, M19AII (432 mm OD)"]
[352,0,"18\"","tubular","Sun M19A, M19AII (382 mm OD)"]
[298,0,"16\"","tubular","Sun M19A, M19AII (331 mm OD)"]
[611,0,"27\"",630,"Ambrosio Aero Elite (rim washers)"]
[620,0,"27\"",630,"Ambrosio Elite (single eyelets)"]
[623,0,"27\"",630,"Araya 16A(3)"]
[622,0,"27\"",630,"Araya 16A(5)"]
[618,0,"27\"",630,"Araya 20A"]
[617,0,"27\"",630,"Araya ADX-1W "]
[610,0,"27\"",630,"Araya ADX-2W"]
[616.4,0,"27\"",630,"Araya LP-60","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[622,0,"27\"",630,"Araya SP-30"]
[618,0,"27\"",630,"Araya SS-40"]
[621,0,"27\"",630,"Araya SS-45"]
[616.4,0,"27\"",630,"Araya TF-110","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[618.4,0,"27\"",630,"Araya W/O-2 steel","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[623,0,"27\"",630,"Dunlop Special Lightweight","2007-02-11","\"Sheldon Brown\" <CaptBike@sheldonbrown.com>"]
[609,0,"27\"",630,"Fiamme 71-Sport"]
[603,0,"27\"",630,"Fiamme 80-Elan"]
[{"$f":"610*630/622","v":617.84565916398719},0,"27\"",630,"Matrix Aurora "]
[605,0,"27\"",630,"Matrix ISO C"]
[609,0,"27\"",630,"Matrix ISO CII"]
[618,0,"27\"",630,"Matrix Titan"]
[622,0,"27\"",630,"Matrix Titan T (touring)"]
[620,0,"27\"",630,"Mavic E2, G40, Mod E"]
[618,0,"27\"",630,"Mavic MA single eyelets"]
[618,0,"27\"",630,"Mavic MA2"]
[618,0,"27\"",630,"Mavic MA40"]
[618,0,"27\"",630,"Mavic Mod 3"]
[618,0,"27\"",630,"Mavic Mod 4"]
[618,0,"27\"",630,"Performance TR22 "]
[617,0,"27\"",630,"Rigida 1320 "]
[{"$f":"618.2+3","v":621.20000000000005},0,"27\"",630,"Rigida AS 23 X (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[621,0,"27\"",630,"Rigida steel Superchromix 1.25 "]
[622,0,"27\"",630,"Specialized Saturae C20"]
[622,0,"27\"",630,"Specialized Saturae C22"]
[622,0,"27\"",630,"Specialized Saturae HC19"]
[619,0,"27\"",630,"Sun C16"]
[615,0,"27\"",630,"Sun CR16"]
[617,0,"27\"",630,"Sun CRE16"]
[617,0,"27\"",630,"Sun CRT16II"]
[619,0,"27\"",630,"Sun D253"]
[618,0,"27\"",630,"Sun L13"]
[620,0,"27\"",630,"Sun L17, L20"]
[618,0,"27\"",630,"Sun M13"]
[619,0,"27\"",630,"Sun M13II"]
[618,0,"27\"",630,"Sun M13L "]
[611,0,"27\"",630,"Sun M14A"]
[614,0,"27\"",630,"Sun M14A (old)"]
[620,0,"27\"",630,"Sun M17"]
[620,0,"27\"",630,"Sun M20"]
[619,0,"27\"",630,"Sun M20A"]
[619,0,"27\"",630,"Sun M25 "]
[623,0,"27\"",630,"Super Champ Competition"]
[619,0,"27\"",630,"Velocity Twin Hollow"]
[621,0,"27\"",630,"Weinmann 2115 "]
[624,0,"27\"",630,"Weinmann A129 "]
[620,0,"27\"",630,"Wolber M58, GTA , GTX "]
[620,0,"27\"",630,"Wolber/Super Champion Gentleman 81"]
[622,0,"27\"",630,"Wolber/Super Champion Gentleman GTA2"]
[622,0,"27\"",630,"Wolber/Super Champion Gentleman GTX"]
[622,0,"27\"",630,"Wolber/Super Champion Module 58"]
[622,0,"27\"",630,"Wolber/Super Champion Module 59"]
[622,0,"27\"",630,"Wolber/Super Champion T430 Alpine"]
[600,0,"700C",622,"Alesa 913 - MEASURE TO BE SURE!","2004-12-28","unknown"]
[600,0,"700C",622,"Alex DA22","2004-01-22","shane.halpin@london-fire.gov.uk"]
[606,0,"700C",622,"Alex DV15","2004-01-26","Dane Jackson <dane@unixbigots.org>"]
[{"$f":"580.8+3","v":583.79999999999995},0,"700C",622,"Alex G6000 22mm wide x 29mm deep, 686g","2003-09-15","DGR"]
[601,0,"700C",622,"Alex R390 (19.6mm wide, 19.1mm tall, double eyelets, 480g)","2003-04-18","\"Raul Cabrera\" <r-cabrera@tamu.edu>"]
[603,0,"700C",622,"Alex R390 19.6w x 19.1h, double eyelets (MEASURE TO BE SURE!)","2003-04-18","vheidner@charter.net"]
[605,0,"700C",622,"Ambrosio Aero Elite"]
[601,0,"700C",622,"Ambrosio Area 4 (Touring/Trekking)","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[607,0,"700C",622,"Ambrosio B.8 (Touring/Trekking)","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[601,0,"700C",622,"Ambrosio Balance 20w x 22h - MEASURE ERD TO BE SURE!","2004-09-09","morgan@hahaha.org"]
[594,0,"700C",622,"Ambrosio Balance 20w x 22h - MEASURE ERD TO BE SURE!","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[602.5,0,"700C",622,"Ambrosio C.C.28 (Touring/Trekking)","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[588,0,"700C",622,"Ambrosio Camel (Touring/Trekking)","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[614,0,"700C",622,"Ambrosio Elite"]
[613,0,"700C",622,"Ambrosio Elite City 22"]
[608,0,"700C",622,"Ambrosio Elite Prisma"]
[606,0,"700C",622,"Ambrosio Eurosport (Touring/Trekking)","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[606,0,"700C",622,"Ambrosio Evolution","2005-11-05","David.Kahn@tomy.co.uk"]
[606,0,"700C",622,"Ambrosio Excellence - MEASURE TO BE SURE"]
[601.5,0,"700C",622,"Ambrosio Excellence - MEASURE TO BE SURE","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[600,0,"700C",622,"Ambrosio Excellight S.S.C.","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[600.5,0,"700C",622,"Ambrosio Excursion","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[590,0,"700C",622,"Ambrosio FCS 28","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[598,0,"700C",622,"Ambrosio Keba (Touring/Trekking) - MEASURE TO BE SURE!","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[608.4,0,"700C",622,"Ambrosio Nexus","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[615,0,"700C",622,"Ambrosio Super Elite"]
[601,0,"700C",622,"Ambrosio The Frog (Touring/Trekking)","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[528,0,"700C",622,"American Classic carbon fiber V rim by Zipp"]
[590.5,0,"700C",622,"American Classic CR-350, new 24mm deep model","2003-07-25","American Classic"]
[598,0,"700C",622,"American Classic Design's \"CR350\"","2003-04-17","http://www.amclassic.com/Rims.html"]
[615,0,"700C",622,"Araya 15"]
[616,0,"700C",622,"Araya 16A(3)"]
[615,0,"700C",622,"Araya 16A(5)"]
[616,0,"700C",622,"Araya 18"]
[611,0,"700C",622,"Araya 20A"]
[607,0,"700C",622,"Araya ADX-1W"]
[602,0,"700C",622,"Araya ADX-2W"]
[600.29999999999995,0,"700C",622,"Araya ADX-510","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[611,0,"700C",622,"Araya CT19"]
[609,0,"700C",622,"Araya CTL185"]
[611,0,"700C",622,"Araya CTL-370"]
[609,0,"700C",622,"Araya CTL385 "]
[614,0,"700C",622,"Araya PX35"]
[610.4,0,"700C",622,"Araya PX-645 (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[606.29999999999995,0,"700C",622,"Araya RC-540","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[{"$f":"610.4+2","v":612.4},0,"700C",622,"Araya RT-520 (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[580,0,"700C",622,"Araya SA-530C Super Aero clincher (30mm deep)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[615,0,"700C",622,"Araya SP-20"]
[613,0,"700C",622,"Araya SP-30","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[611,0,"700C",622,"Araya SS-40"]
[614,0,"700C",622,"Araya SS-45"]
[610.4,0,"700C",622,"Araya TX-310F (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[611,0,"700C",622,"Araya TX350"]
[614,0,"700C",622,"Araya VX300 "]
[614,0,"700C",622,"Araya VX400"]
[{"$f":"592+3","v":595},0,"700C",622,"Bontrager PN 220421 Race X-Lite road ","2002-03-07","DGR"]
[{"$f":"595+3","v":598},{"$f":"0.06*25.4","v":1.5239999999999998},"700C",622,"Bontrager PN 220429 Race Lite road OSB","2002-03-07","DGR"]
[604.1,1.5,"700C",622,"Bontrager PN 220437 Select OSB","2002-08-30","DGR"]
[{"$f":"604+3","v":607},2.5,"700C",622,"Bontrager PN 220472 Race Tubeless 29\" OSB rim brake compatible ","2002-03-07","DGR"]
[580,0,"700C",622,"Bontrager PN 221715 Race Lite Tandem","2002-12-03","DGR"]
[{"$f":"604+3","v":607},2.5,"700C",622,"Bontrager PN 221850 Race Lite Tubeless 29\" OSB rim brake compatible","2002-03-07","DGR"]
[598,0,"700C",622,"Bontrager PN 231404 Race X-Light Aero aluminum clincher","2002-12-03","DGR"]
[593.64,0,"700C",622,"Bontrager PN 240064 RXXXL OCLV Carbon Tubular Front/Rear with SS washer (.82mm thick)","2003-04-17","DCG"]
[591.99,0,"700C",622,"Bontrager PN 240064 RXXXL OCLV Carbon Tubular Front/Rear with SS washer (.82mm thick)","2003-04-17","DCG"]
[{"$f":"593+3","v":596},0,"700C",622,"Bontrager PN 242752, R455 (04 Select Rd. extrusion)","2003-07-30","DCG"]
[{"$f":"604+3","v":607},2.5,"700C",622,"Bontrager PN 243628 Race Lite OSB 29\"","2004-03-08","DGR"]
[589.17999999999995,0,"700C",622,"Bontrager PN 250032 RXXXL OCLV Carbon Clincher Front w/SS washer (.82mm thick)","2004-03-05","DCG"]
[589.17999999999995,2,"700C",622,"Bontrager PN 250033 RXXXL OCLV Carbon Clincher OSB Rear w/SS washer (.82mm thick)","2004-03-05","DCG"]
[{"$f":"604+3","v":607},0,"700C",622,"Bontrager PN 981886 Clyde (24mm wide)","2002-03-07","DGR"]
[{"$f":"604+3","v":607},0,"700C",622,"Bontrager PN 992115, 994103 Fairlane symmetric","2002-03-07","DGR"]
[{"$f":"604+3","v":607},2.5,"700C",622,"Bontrager PN 992116, 994305 Fairlane OSB","2002-03-07","DGR"]
[590.5,0,"700C",622,"Bontrager RXL Carbon Clincher Front PROTOTYPE","2002-07-02","DCG"]
[593.5,1.5,"700C",622,"Bontrager RXL Carbon Clincher Rear OSB PROTOTYPE","2002-02-13","DCG"]
[586.15,0,"700C",622,"Bontrager RXL OCLV Carbon Tubular Front/Rear Prototype","2002-07-22","DGR"]
[611,0,"700C",622,"Campagnolo Amber "]
[575,0,"700C",622,"Campagnolo Atlanta '96 (about 30mm tall)"]
[614,0,"700C",622,"Campagnolo Delta XL, Omega XL, Lambda, Omicron box (very low profile)"]
[612,0,"700C",622,"Campagnolo Gamma box"]
[612,0,"700C",622,"Campagnolo Helsinki '52"]
[600,0,"700C",622,"Campagnolo Lambda \"V\" profile  (about 21mm tall)"]
[612,0,"700C",622,"Campagnolo Melbourne '56"]
[600,0,"700C",622,"Campagnolo Mexico '68 \"V\" profile (about 23mm tall)","2005-08-29","nick@nickpashley.com"]
[608,0,"700C",622,"Campagnolo Montreal '76 box style"]
[603,0,"700C",622,"Campagnolo Montreal '76, new style (beveled semi-aero)"]
[601,0,"700C",622,"Campagnolo Moskva '80 "]
[618,0,"700C",622,"Campagnolo Munchen '72"]
[600,0,"700C",622,"Campagnolo Omega \"V\" profile (about 21mm tall)"]
[608,0,"700C",622,"Campagnolo Omega 19 box style (about 19mm wide)"]
[613,0,"700C",622,"Campagnolo Omega Strada and Strada Hardox box style (about 20mm wide)"]
[612,0,"700C",622,"Campagnolo Roma '60"]
[614,0,"700C",622,"Campagnolo Strada "]
[609,0,"700C",622,"Campagnolo Tokyo '64 "]
[613,0,"700C",622,"Campagnolo Topaz "]
[614,0,"700C",622,"Campagnolo XL Strada "]
[600,0,"700C",622,"Campagnolo Ypsilon \"V\" profile (about 21mm tall)"]
[615,0,"700C",622,"Campagnolo Ypsilon box"]
[{"$f":"AVERAGE(597,596,596,597,596.5)","v":596.5},0,"700C",622,"da Vinci V22 http://www.davincitandems.com/","2002-07-15","DGR"]
[599,0,"700C",622,"DT Swiss RR 1.1","2005-11-05","http://www.dtswiss.com"]
[600,0,"700C",622,"DT Swiss TK 7.1","2005-11-05","http://www.dtswiss.com"]
[611,0,"700C",622,"Fiamme 80-Elan"]
[562,0,"700C",622,"FiR Antara 2000"]
[600,0,"700C",622,"FiR EA10 "]
[610,0,"700C",622,"FiR EA50"]
[610,0,"700C",622,"FiR EA60 "]
[608,0,"700C",622,"FiR EA61"]
[609,0,"700C",622,"FiR EA65 "]
[614,0,"700C",622,"FiR EL20"]
[614,0,"700C",622,"FiR EL45"]
[614,0,"700C",622,"FiR ES35"]
[614,0,"700C",622,"FiR EU90"]
[606,0,"700C",622,"FiR MT 232"]
[585,0,"700C",622,"FiR Net97"]
[591,0,"700C",622,"FiR Net97 (MEASURE TO BE SURE!)","2003-12-19","Bruce Lange <brucelange@comcast.net>"]
[585,0,"700C",622,"FiR Net97 (MEASURE TO BE SURE!)"]
[614,0,"700C",622,"FiR SC150 actual weight 380gms!"]
[605,0,"700C",622,"FiR SC170"]
[600,0,"700C",622,"FiR SC200"]
[582,0,"700C",622,"FiR SC350"]
[582,0,"700C",622,"FiR SRG30 (30mm deep aero rim, 500gms)"]
[604,0,"700C",622,"IRD Cadence","2006-12-02","http://www.interlocracing.com/rims.html"]
[604,1.5,"700C",622,"IRD Cadence VSR (virtual symmetry rim)","2006-12-02","http://www.interlocracing.com/rims.html"]
[576,0,"700C",622,"IRD Cadence Aero (30 mm deep)","2006-12-02","http://www.interlocracing.com/rims.html"]
[607,0,"700C",622,"IRD Clyde 24 mm wide","2006-12-02","http://www.interlocracing.com/rims.html"]
[{"$f":"610","v":610},0,"700C",622,"Matrix Aurora"]
[{"$f":"603+3","v":606},2,"700C",622,"Matrix Aurora OSB (offset spoke bed)","2005-01-24","bontrager.com tech support "]
[597,0,"700C",622,"Matrix ISO C"]
[601,0,"700C",622,"Matrix ISO CII"]
[603.9,1.5,"700C",622,"Matrix PN 970704 ISO 3","2002-03-09","DGR: measured from built wheel"]
[603.9,1.5,"700C",622,"Matrix PN 970704 ISO 3","2002-03-09","DGR: measured from built wheel"]
[603.9,1.5,"700C",622,"Matrix PN 970704 ISO 3","2002-03-09","DGR: measured from built wheel"]
[{"$f":"592+3","v":595},0,"700C",622,"Matrix PN 970704 ISO 3","2002-03-07","DGR"]
[{"$f":"592+3","v":595},0,"700C",622,"Matrix PN 970704 ISO 3","2002-03-07","DGR"]
[{"$f":"592+3","v":595},0,"700C",622,"Matrix PN 970704 ISO 3","2002-03-07","DGR"]
[611,0,"700C",622,"Matrix Titan"]
[611,0,"700C",622,"Matrix Titan S"]
[614,0,"700C",622,"Matrix Titan T (touring)"]
[611,0,"700C",622,"Matrix Titan-II"]
[611,0,"700C",622,"Mavic 192 "]
[605,0,"700C",622,"Mavic 195"]
[604,0,"700C",622,"Mavic A 119","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[602.5,0,"700C",622,"Mavic A 317 Disc","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[604.5,0,"700C",622,"Mavic A 319 D","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[602.5,0,"700C",622,"Mavic A 319 D 05","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[600.5,0,"700C",622,"Mavic A 719","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[601,0,"700C",622,"Mavic CXP10 ","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[600,0,"700C",622,"Mavic CXP10 "]
[{"$f":"598.5+3","v":601.5},0,"700C",622,"Mavic CXP11 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[{"$f":"594+3","v":597},0,"700C",622,"Mavic CXP12 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[{"$f":"584+3","v":587},0,"700C",622,"Mavic CXP14 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[{"$f":"598.5+3","v":601.5},0,"700C",622,"Mavic CXP21 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[598.5,0,"700C",622,"Mavic CXP22N","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[599.5,0,"700C",622,"Mavic CXP22S","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[{"$f":"595+3","v":598},0,"700C",622,"Mavic CXP23 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[{"$f":"584+3","v":587},0,"700C",622,"Mavic CXP30 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[{"$f":"595+3","v":598},0,"700C",622,"Mavic CXP33 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[614,0,"700C",622,"Mavic E2"]
[614,0,"700C",622,"Mavic G40"]
[612.5,0,"700C",622,"Mavic MA","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[{"$f":"610+3","v":613},0,"700C",622,"Mavic MA2 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[607.5,0,"700C",622,"Mavic MA3","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[607,0,"700C",622,"Mavic MA3"]
[613,0,"700C",622,"Mavic MA40 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[611,0,"700C",622,"Mavic Mod 3"]
[613,0,"700C",622,"Mavic Mod 3D Argent"]
[611,0,"700C",622,"Mavic Mod 4"]
[613,0,"700C",622,"Mavic Mod 50"]
[614,0,"700C",622,"Mavic Mod E"]
[602,0,"700C",622,"Mavic Open 20 ","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[601,0,"700C",622,"Mavic Open 20 "]
[603,0,"700C",622,"Mavic Open 20D ","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[602,0,"700C",622,"Mavic Open 20D "]
[608,0,"700C",622,"Mavic Open 4CD","2001-10-11","Martin Staines mstaines@superform-aluminium.com"]
[{"$f":"602+3","v":605},0,"700C",622,"Mavic Open Pro (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[{"$f":"604+3","v":607},0,"700C",622,"Mavic Open SUP (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[{"$f":"602+3","v":605},0,"700C",622,"Mavic Reflex (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[{"$f":"600+3","v":603},0,"700C",622,"Mavic T138 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[{"$f":"606+3","v":609},0,"700C",622,"Mavic T215 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[{"$f":"600+3","v":603},0,"700C",622,"Mavic T217 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[{"$f":"602.5+3","v":605.5},0,"700C",622,"Mavic T221 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[{"$f":"600+3","v":603},0,"700C",622,"Mavic T223 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[604.5,0,"700C",622,"Mavic T224","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[{"$f":"603.5+3","v":606.5},0,"700C",622,"Mavic T238 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[{"$f":"608+3","v":611},0,"700C",622,"Mavic T261 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[601.5,0,"700C",622,"Mavic T519","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[600.5,0,"700C",622,"Mavic T520","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[613,0,"700C",622,"Nashbar UC13"]
[612,0,"700C",622,"Nisi Mixer","2004-02-18","Jon Senior <jon@restlesslemon.co.uk>"]
[604,0,"700C",622,"NOTUBES ZTR 355 29'er","2006-12-02","http://www.notubes.com/support_wheelset.php"]
[417,0,"700C",622,"NOTUBES ZTR Olympic 29'er","2006-12-02","http://www.notubes.com/support_wheelset.php"]
[610,0,"700C",622,"Performance C19 "]
[612,0,"700C",622,"Performance C19SL "]
[610,0,"700C",622,"Rigida 1320 "]
[{"$f":"602+3","v":605},0,"700C",622,"Rigida ARIES (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"610.7+3","v":613.70000000000005},0,"700C",622,"Rigida AS 23 X (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"609+3","v":612},0,"700C",622,"Rigida AS 26 F (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[602,0,"700C",622,"Rigida CHP-6"]
[{"$f":"605+3","v":608},0,"700C",622,"Rigida CHRINA (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"578+3","v":581},0,"700C",622,"Rigida DP 18 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"581.34+3","v":584.34},0,"700C",622,"Rigida DP 2000 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"592.6+3","v":595.6},0,"700C",622,"Rigida DP 25 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"589.4+3","v":592.4},0,"700C",622,"Rigida DPX (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"605+3","v":608},0,"700C",622,"Rigida EXCEL (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[606,0,"700C",622,"Rigida HLC2000 "]
[{"$f":"607.7+3","v":610.70000000000005},0,"700C",622,"Rigida LIBRA (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"609.5+3","v":612.5},0,"700C",622,"Rigida M 19 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"609.5+3","v":612.5},0,"700C",622,"Rigida M 21 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"597.8+3","v":600.79999999999995},0,"700C",622,"Rigida NOVA (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"592.4","v":592.4},0,"700C",622,"Rigida OLYMPUS (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"607.7+3","v":610.70000000000005},0,"700C",622,"Rigida ORION/MENSA (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"601.8+3","v":604.79999999999995},0,"700C",622,"Rigida PHOENIX (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[612,0,"700C",622,"Rigida Score "]
[{"$f":"600+3","v":603},0,"700C",622,"Rigida SHC (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"600+3","v":603},0,"700C",622,"Rigida SHP (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"607.7+3","v":610.70000000000005},0,"700C",622,"Rigida SIRIUS (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"601.3+3","v":604.29999999999995},0,"700C",622,"Rigida TUB 25/ TUB 26 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"600+3","v":603},0,"700C",622,"Rigida VELA (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"589.4+3","v":592.4},0,"700C",622,"Rigida X PLORER (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"596.84+3","v":599.84},0,"700C",622,"Rigida ZAC 2000 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"604+3","v":607},0,"700C",622,"Rigida/Weinmann ZAC 19 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[587,0,"700C",622,"Rinard/Hollenbeck carbon clincher proto #1"]
[{"$f":"599+3","v":602},0,"700C",622,"Ritchey Aero Road Comp centered holes (ERD is nipple contact dia + 3mm for nipples)","2004-03-17","http://www.ritcheylogic.com/trpdfcharts/rims.pdf"]
[602,2.5,"700C",622,"Ritchey Aero Road Comp OCR (ERD is nipple contact dia + 3mm for nipples)","2004-03-17","http://www.ritcheylogic.com/trpdfcharts/rims.pdf"]
[602,0,"700C",622,"Ritchey Aero Road Pro centered holes (ERD is nipple contact dia + 3mm for nipples)","2004-03-17","http://www.ritcheylogic.com/trpdfcharts/rims.pdf"]
[602,2.5,"700C",622,"Ritchey Aero Road Pro OCR (ERD is nipple contact dia + 3mm for nipples)","2004-03-17","http://www.ritcheylogic.com/trpdfcharts/rims.pdf"]
[602,0,"700C",622,"Ritchey Aero Road WCS centered holes (ERD is nipple contact dia + 3mm for nipples)","2004-03-17","http://www.ritcheylogic.com/trpdfcharts/rims.pdf"]
[602,2.5,"700C",622,"Ritchey Aero Road WCS OCR (ERD is nipple contact dia + 3mm for nipples)","2004-03-17","http://www.ritcheylogic.com/trpdfcharts/rims.pdf"]
[610,0,"700C",622,"Ritchey Rock 450CE"]
[610,0,"700C",622,"Ritchey Rock 490"]
[610,0,"700C",622,"Ritchey Rock 490C"]
[{"$f":"602+3","v":605},0,"700C",622,"Ritchey Rock 700 Pro (ERD is Nipple Seat Dia + 3mm for nipples)"]
[596,0,"700C",622,"Ritchey Trekking Comp","2004-03-17","http://www.ritcheylogic.com/trpdfcharts/rims.pdf"]
[594,2.5,"700C",622,"Ritchey Trekking Comp OCR","2004-03-17","http://www.ritcheylogic.com/trpdfcharts/rims.pdf"]
[611,0,"700C",622,"Ritchey Vantage Comp"]
[612,0,"700C",622,"Ritchey Vantage Cross-Sport "]
[{"$f":"592+3","v":595},0,"700C",622,"Rolf Sestriere","2002-07-25","DGR"]
[{"$f":"592+3","v":595},0,"700C",622,"Rolf Vector","2002-03-07","DGR"]
[580,0,"700C",622,"Rolf Vector Comp, Trek made","2002-04-15","DGR"]
[604.1,0,"700C",622,"Rolf Vector Pro, Araya made. For Greer internal nipples + 4mm washers","2002-03-07","DGR"]
[598,0,"700C",622,"Rolf Vector Pro, Trek made. For Greer internal nipples, no washers","2002-03-07","DGR"]
[604,0,"700C",622,"Salsa Delgado Cross 22.5w x 18h","2004-06-10","http://www.salsacycles.com/comps_rims.html"]
[614,0,"700C",622,"Specialized C20"]
[614,0,"700C",622,"Specialized C22"]
[614,0,"700C",622,"Specialized HC19"]
[614,0,"700C",622,"Specialized HC20"]
[607,0,"700C",622,"Sun 0 degree XC"]
[603,0,"700C",622,"Sun Ascent"]
[612,0,"700C",622,"Sun AT18 "]
[528,0,"700C",622,"Sun Buzz Clincher (carbon, alu brake track)"]
[610,0,"700C",622,"Sun CR16"]
[607,0,"700C",622,"Sun CR17A"]
[612,0,"700C",622,"Sun CR18, single eyelets",null,"www.sunrims.com"]
[608,0,"700C",622,"Sun CR20 "]
[609,0,"700C",622,"Sun CRE16"]
[609,0,"700C",622,"Sun CRT16II"]
[611,0,"700C",622,"Sun L13"]
[612,0,"700C",622,"Sun L17"]
[612,0,"700C",622,"Sun L18"]
[612,0,"700C",622,"Sun L20"]
[612,0,"700C",622,"Sun L25"]
[610,0,"700C",622,"Sun M13"]
[610,0,"700C",622,"Sun M13II"]
[612,0,"700C",622,"Sun M13L "]
[603,0,"700C",622,"Sun M14A"]
[606,0,"700C",622,"Sun M14A (old)"]
[612,0,"700C",622,"Sun M17"]
[611,0,"700C",622,"Sun M20"]
[612,0,"700C",622,"Sun M20B "]
[612,0,"700C",622,"Sun M25"]
[612,0,"700C",622,"Sun M25 "]
[601,0,"700C",622,"Sun ME14A"]
[603,0,"700C",622,"Sun Rhyno "]
[612,0,"700C",622,"Sun Rhyno Lite (newer version)"]
[603,0,"700C",622,"Sun SST20"]
[592,0,"700C",622,"Sun Venus (medium deep aero)"]
[606,0,"700C",622,"Torelli Master",null,"Southerlands"]
[611,0,"700C",622,"Torelli Master, new style","2002-04-03","http://www.rivendellbicycles.com/Webalog/wheels/18094.html"]
[596,0,"700C",622,"Velocity Aero (20mm wide x 21mm deep)"]
[602,0,"700C",622,"Velocity Aerohead (20mm wide x 19mm deep, 2001)"]
[598,0,"700C",622,"Velocity Aerohead (20mm wide x 21mm deep, 2000 and earlier)"]
[598,4,"700C",622,"Velocity Aerohead OC (Off Center)","2003-07-29","velocity@velocityusa.com"]
[582,0,"700C",622,"Velocity Deep V (19mm wide x 30mm deep)"]
[596,0,"700C",622,"Velocity Dyad (24mm wide x 22mm deep)"]
[591,0,"700C",622,"Velocity Fusion (19mm wide x 25mm deep) Measured 596.4. MEASURE TO BE SURE!","2002-09-18","DGR"]
[612,0,"700C",622,"Velocity Glider (26mm wide x 14mm deep)"]
[607,0,"700C",622,"Velocity Razor (20mm wide x 16mm deep)"]
[611,0,"700C",622,"Velocity Twin Hollow (22mm wide x 14mm deep)"]
[585,0,"700C",622,"Veulta Airline 3 ","2002-02-28","DCG"]
[595.9,0,"700C",622,"Vuelta Airline 2 622x13","2001-07-17","Vuelta fax"]
[599.29999999999995,0,"700C",622,"Vuelta Stylus 622x13","2001-07-17","Vuelta fax"]
[607,0,"700C",622,"Vuelta Vision","2002-02-28","DCG"]
[619,0,"700C",622,"Weinmann A129 "]
[609,0,"700C",622,"Wheelsmith Rimfire "]
[602,0,"700C",622,"Wolber TX Profil aero"]
[613,0,"700C",622,"Wolber/Super Champion Gentleman 81"]
[614,0,"700C",622,"Wolber/Super Champion Gentleman GTA2"]
[614,0,"700C",622,"Wolber/Super Champion Gentleman GTX"]
[615,0,"700C",622,"Wolber/Super Champion Module 58"]
[615,0,"700C",622,"Wolber/Super Champion Module 59"]
[614,0,"700C",622,"Wolber/Super Champion T430 Alpine"]
[606,0,"700C",622,"WTB SpeedMaster 21x11.3 700c (32h, 21mm wide) ","2002-06-17","thaft@wtb.com"]
[605,0,"700C",622,"Zipp 110 17mm deep box section aluminum clincher"]
[584,0,"700C",622,"Zipp 310 30mm deep aluminum clincher "]
[567,0,"700C",622,"Zipp 415 40mm deep carbon/aluminum clincher","2005-11-05","Kuthan.Kan@egco.com"]
[477,0,"700C",622,"Zipp 520 82mm deep carbon/aluminum clincher","2005-11-05","Kuthan.Kan@egco.com"]
[529,0,"700C",622,"Zipp 505 58mm deep carbon/aluminum clincher","2005-11-05","Kuthan.Kan@egco.com"]
[528,0,"700C",622,"Zipp 530 58mm deep carbon/aluminum clincher"]
[{"$f":"578+3","v":581},0,"650A",590,"Rigida AS 23 X (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"494+3","v":497},0,"650A",590,"Rigida AS 26 F (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[582,0,"26x1 3/8",590,"Rigida steel 26x1 3/8"]
[576,0,"26x1 3/8",590,"Sun CR20 "]
[578,0,"26x1 3/8",590,"Sun L20"]
[570,0,"26x1 3/8",590,"Sun M14A"]
[579,0,"26x1 3/8",590,"Weinmann 2120 26x1 3/8"]
[572,0,"650B",584,"Mavic Module 3, Module 4 ArgentD"]
[{"$f":"570.5+3","v":573.5},0,"650B",584,"Rigida AS 26 F (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[574,0,"650B",584,"Wolber M58 "]
[543,0,"650C",622,"Ambrosio Balance 20w x 22h - MEASURE ERD TO BE SURE!","2006-11-20","http://groups.google.com/group/rec.bicycles.tech/msg/0909c0f61e83da38"]
[482,0,"650C",571,"American Classic carbon fiber V rim"]
[{"$f":"600.3+571-622","v":549.29999999999995},0,"650C",571,"Araya ADX-510 (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[547.20000000000005,0,"650C",571,"Araya RC-540","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[529,0,"650C",571,"Araya SA-530C Super Aero clincher (30mm deep)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[534,0,"650C",571,"Bontrager carbon aero, back-calculated from 221441 using 255, 257 spokes.","2002-12-19","DGR"]
[{"$f":"543+3","v":546},0,"650C",571,"Bontrager PN 220430 Race Lite road","2002-03-22","DGR"]
[{"$f":"544+3","v":547},0,"650C",571,"Bontrager PN 231265 Race Lite OSB road","2002-03-22","DGR"]
[{"$f":"525+2*(9+2)","v":547},0,"650C",571,"Bontrager PN 243756 RXL Aero Clincher","2003-06-05","DCG"]
[555,0,"650C",571,"Campagnolo Montreal '76 "]
[556,0,"650C",571,"Campagnolo Omega 19 "]
[511,0,"650C",571,"FiR Antara 2000"]
[525,0,"650C",571,"FiR SRG30 (30mm deep aero rim, 440gms)"]
[{"$f":"546+3","v":549},0,"650C",571,"Mavic CXP12 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[539.5,0,"650C",571,"Mavic CXP14 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[{"$f":"537+3","v":540},0,"650C",571,"Mavic CXP14 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples) MEASURE TO BE SURE!!","2001-12-28","Mavic OEM brochure"]
[{"$f":"533+3","v":536},0,"650C",571,"Mavic CXP14 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples) MEASURE TO BE SURE!!","2001-12-10","Mavic OEM brochure"]
[{"$f":"547+3","v":550},0,"650C",571,"Mavic CXP33 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples) ","2001-12-28","Mavic OEM brochure"]
[559,0,"650C",571,"Mavic MA40 "]
[554,0,"650C",571,"Mavic Open 4CD"]
[{"$f":"551+3","v":554},0,"650C",571,"Mavic Open Pro (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[{"$f":"527.7+3","v":530.70000000000005},0,"650C",571,"Rigida DP 18","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"548.7+3","v":551.70000000000005},0,"650C",571,"Rigida NOVA R (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[551.70000000000005,0,"650C",571,"Rolf Vector Pro, Araya rim, including 9mm Greer nipple + 4mm washer","2002-03-03","DGR"]
[546,0,"650C",571,"Rolf Vector Pro, Trek made. For Greer internal nipples, no washers","2006-07-07","DGR"]
[552,0,"650C",571,"Sun Ascent"]
[560,0,"650C",571,"Sun M13II"]
[561,0,"650C",571,"Sun M13L "]
[552,0,"650C",571,"Sun M14A"]
[549,0,"650C",571,"Sun ME14A"]
[540,0,"650C",571,"Sun Venus (medium deep aero)"]
[558,0,"650C",571,"Velocity Aerohead (20mm wide x 19mm deep, 2001) MEASURE TO BE SURE!","2006-12-02","DGR"]
[554,0,"650C",571,"Velocity Aerohead (20mm wide x 21mm deep)"]
[531,0,"650C",571,"Velocity Deep V (19mm wide x 30mm deep)"]
[556,0,"650C",571,"Velocity Razor (like Mavic Open Pro)"]
[518,0,"650C",571,"Zipp 370 40mm deep carbon/aluminum clincher","2005-11-05","Kuthan.Kan@egco.com"]
[477,0,"650C",571,"Zipp 460 58mm deep carbon/aluminum clincher","2005-11-05","Kuthan.Kan@egco.com"]
[482,0,"650C",571,"Zipp 500 58mm deep carbon/aluminum clincher"]
[553,0,"26\" MTB",559,"Alex DX32","2004-11-13","Arseniy Vasilyev <Trailmax@yandex.ru>"]
[{"$f":"537.1+1.5","v":538.6},0,"26\" MTB",559,"Araya Big Willie MG2000 (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[{"$f":"547.8+1.5","v":549.29999999999995},0,"26\" MTB",559,"Araya GP-710 (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[{"$f":"497.2+1.5","v":498.7},0,"26\" MTB",559,"Araya RB-17 (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[547,0,"26\" MTB",559,"Araya RM14"]
[547,0,"26\" MTB",559,"Araya RM17"]
[547,0,"26\" MTB",559,"Araya RM20"]
[547,0,"26\" MTB",559,"Araya RM25"]
[547,0,"26\" MTB",559,"Araya RM395"]
[547,0,"26\" MTB",559,"Araya RM400"]
[{"$f":"545.7+1.5","v":547.20000000000005},0,"26\" MTB",559,"Araya RM-915DH (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[{"$f":"538.1+1.5","v":539.6},0,"26\" MTB",559,"Araya RM-930DISC (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[{"$f":"547.8+1.5","v":549.29999999999995},0,"26\" MTB",559,"Araya TM-840F (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[547,0,"26\" MTB",559,"Araya VP20"]
[543,0,"26\" MTB",559,"Araya XA-1"]
[522,0,"26\" MTB",559,"Atomic Trailpimp","2003-10-06","barsiantony@hotmail.com"]
[545,0,"26\" MTB",559,"Avenir Duro 17 "]
[545,0,"26\" MTB",559,"Bontrager BCX Blue "]
[545,0,"26\" MTB",559,"Bontrager BCX Red"]
[553,0,"26\" MTB",559,"Bontrager BCX1, BCX2, BCX3 "]
[{"$f":"536+3","v":539},2.5,"26\" MTB",559,"Bontrager PN 201752 Mustang OSB Disc","2002-03-07","DGR"]
[{"$f":"539+3","v":542},0,"26\" MTB",559,"Bontrager PN 211931 Mustang tubeless","2002-03-07","DGR"]
[{"$f":"539+3","v":542},0,"26\" MTB",559,"Bontrager PN 220459 Race Mod Tubeless front","2002-03-07","DGR"]
[{"$f":"536+3","v":539},2.5,"26\" MTB",559,"Bontrager PN 220481 Race Mod Disc specific","2002-03-07","DGR"]
[543,2.5,"26\" MTB",559,"Bontrager PN 231248 Race X-Lite OSB","2002-06-14","DGR"]
[538,0,"26\" MTB",559,"Bontrager PN 231714 Race X-Lite symmetrical","2002-06-14","DGR"]
[{"$f":"539","v":539},0,"26\" MTB",559,"Bontrager PN 982951 Valiant symmetrical","2002-03-07","DGR"]
[{"$f":"542+3","v":545},0,"26\" MTB",559,"Bontrager PN 984037 Maverick symmetrical","2002-03-07","DGR"]
[545,2.5,"26\" MTB",559,"Bontrager PN 984038 Maverick OSB","2002-03-07","DGR"]
[545,2.5,"26\" MTB",559,"Bontrager PN 984039 Mustang OSB","2002-03-07","DGR"]
[545,0,"26\" MTB",559,"Bontrager PN 984042 Clyde","2002-03-07","DGR"]
[545,0,"26\" MTB",559,"Bontrager PN 984238 Mustang symmetrical","2002-03-07","DGR"]
[545,2.5,"26\" MTB",559,"Bontrager PN 984574 Valiant OSB","2002-03-07","DGR"]
[545,0,"26\" MTB",559,"Bontrager PN 992201Corvair symmetrical","2002-03-07","DGR"]
[545,2.5,"26\" MTB",559,"Bontrager PN 993524 Corvair OSB","2002-03-07","DGR"]
[545,2.5,"26\" MTB",559,"Bontrager RaceLite Asym rear"]
[{"$f":"539+3","v":542},0,"26\" MTB",559,"Bontrager RaceLite front"]
[537.5,2.5,"26\" MTB",559,"Bontrager TubeLess Disc, OSB, SSD=534.5+3mm for eyelettes","2002-03-18","DCG"]
[542,2.5,"26\" MTB",559,"Bontrager, PN 221723, Mustang OSB, Tubeless","2003-08-06","dcg"]
[539,0,"26\" MTB",559,"Bontrager, PN 231323, Mustang, Front, Tubeless, lightweight extrusion","2003-08-06","dcg"]
[537,2.5,"26\" MTB",559,"Bontrager, PN 231327, Mustang, Disc, Tubeless","2003-08-06","dcg"]
[549,0,"26\" MTB",559,"Bontrager/Mavic MA2, MA40 "]
[552,0,"26\" MTB",559,"Bontrager/Weinmann BCR1"]
[547,0,"26\" MTB",559,"Breezer Backdraft "]
[541,0,"26\" MTB",559,"Campagnolo Aconcagua"]
[553,0,"26\" MTB",559,"Campagnolo Alpha XL"]
[541,0,"26\" MTB",559,"Campagnolo Atek"]
[551,0,"26\" MTB",559,"Campagnolo Beta"]
[539,0,"26\" MTB",559,"Campagnolo Contax , 16mm"]
[546,0,"26\" MTB",559,"Campagnolo Everest"]
[519,0,"26\" MTB",559,"Campagnolo K2 "]
[548,0,"26\" MTB",559,"Campagnolo Kappa"]
[542,0,"26\" MTB",559,"Campagnolo Kilimangiaro"]
[542,0,"26\" MTB",559,"Campagnolo Mirox"]
[540,0,"26\" MTB",559,"Campagnolo Stheno"]
[540,0,"26\" MTB",559,"Campagnolo Thorr "]
[543,0,"26\" MTB",559,"Campagnolo Zark "]
[546,0,"26\" MTB",559,"Campagnolo Zeta"]
[537,0,"26\" MTB",559,"DT Swiss E 540 Enduro disc","2005-11-05","dtswiss.com"]
[539,0,"26\" MTB",559,"DT Swiss EX 5.1d (disc brakes)","2005-11-05","dtswiss.com"]
[535,0,"26\" MTB",559,"DT Swiss FR 6.1d (disc brakes)","2005-11-05","dtswiss.com"]
[538,0,"26\" MTB",559,"DT Swiss XR 4.1 (rim or disc brakes)","2005-11-05","dtswiss.com"]
[538,0,"26\" MTB",559,"DT Swiss XR 4.1d (disc brakes)","2005-11-05","dtswiss.com"]
[538,0,"26\" MTB",559,"DT Swiss XR 4.1 ceramic","2005-11-05","dtswiss.com"]
[539,0,"26\" MTB",559,"DT Swiss X 450 MTB non disc","2005-11-05","dtswiss.com"]
[540,0,"26\" MTB",559,"DT Swiss X 450 MTB disc","2005-11-05","dtswiss.com"]
[545,0,"26\" MTB",559,"FiR MS26, Downhill (same w/ machined sidewalls)"]
[543,0,"26\" MTB",559,"FiR MT 232"]
[535,0,"26\" MTB",559,"FiR W 400"]
[530,0,"26\" MTB",559,"IRD Tsunami","2006-12-02","http://www.interlocracing.com/rims.html"]
[528,0,"26\" MTB",559,"IRD Tsunami disk","2006-12-02","http://www.interlocracing.com/rims.html"]
[538,0,"26\" MTB",559,"K525"]
[{"$f":"2*256+AVERAGE(33,32.5,33,32.5,31.9,31.4,32.1,32.3)","v":544.33749999999998},0,"26\" MTB",559,"Matrix 750 (22mm w x 20.5mm deep)","2002-09-29","DGR"]
[535,0,"26\" MTB",559,"Matrix ISO C"]
[539,0,"26\" MTB",559,"Matrix ISO CII"]
[551,0,"26\" MTB",559,"Matrix Lobo"]
[547,0,"26\" MTB",559,"Matrix Mt. Titan "]
[546,0,"26\" MTB",559,"Matrix S T Comp "]
[541,0,"26\" MTB",559,"Matrix Single Track"]
[546,0,"26\" MTB",559,"Matrix Swami "]
[541,0,"26\" MTB",559,"Mavic 117"]
[{"$f":"541+3","v":544},0,"26\" MTB",559,"Mavic 121 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[{"$f":"536+3","v":539},0,"26\" MTB",559,"Mavic 217 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[540.5,0,"26\" MTB",559,"Mavic 217D","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[{"$f":"540+3","v":543},0,"26\" MTB",559,"Mavic 220 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[{"$f":"540.5+3","v":543.5},0,"26\" MTB",559,"Mavic 221 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[{"$f":"541.5+3","v":544.5},0,"26\" MTB",559,"Mavic 238 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-10","Mavic OEM brochure"]
[543,0,"26\" MTB",559,"Mavic 238N","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[534.5,0,"26\" MTB",559,"Mavic D3.1","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[{"$f":"534.5+3","v":537.5},0,"26\" MTB",559,"Mavic D321 Disc (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[{"$f":"532+3","v":535},0,"26\" MTB",559,"Mavic D521 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[540,0,"26\" MTB",559,"Mavic Energie M217"]
[540,0,"26\" MTB",559,"Mavic Energie M7"]
[536.5,0,"26\" MTB",559,"Mavic EX 325 Disc","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[534.5,0,"26\" MTB",559,"Mavic EX 721","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[537,0,"26\" MTB",559,"Mavic EX 729 Disc","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[534.5,0,"26\" MTB",559,"Mavic EX 823 Disc","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[530.5,0,"26\" MTB",559,"Mavic EX 823 Disc 05","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[538.5,0,"26\" MTB",559,"Mavic F 219 Disc","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[538.5,0,"26\" MTB",559,"Mavic F519","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[543,0,"26\" MTB",559,"Mavic F519"]
[546,0,"26\" MTB",559,"Mavic M230 "]
[548,0,"26\" MTB",559,"Mavic M231"]
[544,0,"26\" MTB",559,"Mavic M238"]
[548,0,"26\" MTB",559,"Mavic M261"]
[545,0,"26\" MTB",559,"Mavic M281 "]
[550,0,"26\" MTB",559,"Mavic MA40"]
[542,0,"26\" MTB",559,"Mavic Oxygen M6 "]
[550,0,"26\" MTB",559,"Mavic Rando M4"]
[548,0,"26\" MTB",559,"Mavic Rando M5"]
[540.20000000000005,0,"26\" MTB",559,"Mavic T519"]
[{"$f":"540+3","v":543},0,"26\" MTB",559,"Mavic X138 eyelets (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[{"$f":"540+3","v":543},0,"26\" MTB",559,"Mavic X138N no eyelets (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[548,0,"26\" MTB",559,"Mavic X139N no eyelets","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[{"$f":"540.5+3","v":543.5},0,"26\" MTB",559,"Mavic X221 eyelets (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[{"$f":"539.5+3","v":542.5},0,"26\" MTB",559,"Mavic X221N no eyelets (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[{"$f":"539.5+3","v":542.5},0,"26\" MTB",559,"Mavic X222 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[{"$f":"536+3","v":539},0,"26\" MTB",559,"Mavic X223 Disc (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[540.5,0,"26\" MTB",559,"Mavic X225","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[534.5,0,"26\" MTB",559,"Mavic X3.1","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[534.5,0,"26\" MTB",559,"Mavic X3.1 Disc","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[532,0,"26\" MTB",559,"Mavic X3.1 UST disc specific. 16 to 18mm nipples required.","2002-02-20","Mavic tech via charlieb@attbi.com"]
[{"$f":"538.5+3","v":541.5},0,"26\" MTB",559,"Mavic X317 Disc (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[{"$f":"537.5+3","v":540.5},0,"26\" MTB",559,"Mavic X517 (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[541,0,"26\" MTB",559,"Mavic X618","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[541,0,"26\" MTB",559,"Mavic XC 317 Disc","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[541,0,"26\" MTB",559,"Mavic XC 717 Disc","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[541,0,"26\" MTB",559,"Mavic XC717","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[542.5,0,"26\" MTB",559,"Mavic XM 117","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[548,0,"26\" MTB",559,"Mavic XM 117 Disc","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[538.5,0,"26\" MTB",559,"Mavic XM 317 Disc","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[538.5,0,"26\" MTB",559,"Mavic XM 321 Disc","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[540.5,0,"26\" MTB",559,"Mavic XM 517","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[538.5,0,"26\" MTB",559,"Mavic XM 719","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[534.5,0,"26\" MTB",559,"Mavic XM 819","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[534.5,0,"26\" MTB",559,"Mavic XM 819 Disc","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[540,0,"26\" MTB",559,"NOTUBES ZTR 355","2006-12-02","http://www.notubes.com/support_wheelset.php"]
[545,0,"26\" MTB",559,"NOTUBES ZTR Freeride","2006-12-02","http://www.notubes.com/support_wheelset.php"]
[536,0,"26\" MTB",559,"NOTUBES ZTR Olympic","2006-12-02","http://www.notubes.com/support_wheelset.php"]
[{"$f":"538+3","v":541},0,"26\" MTB",559,"Rigida ARIES (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)",null,"www.rigida.com/anglais/"]
[{"$f":"545.4+3","v":548.4},0,"26\" MTB",559,"Rigida AS 26 F (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"545.4+3","v":548.4},0,"26\" MTB",559,"Rigida AS 26 FL (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"536.85+3","v":539.85},0,"26\" MTB",559,"Rigida DH 30 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"518+3","v":521},0,"26\" MTB",559,"Rigida DP 2000 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"516.6+3","v":519.6},0,"26\" MTB",559,"Rigida DP 22 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)",null,"www.rigida.com/anglais/"]
[{"$f":"529+3","v":532},0,"26\" MTB",559,"Rigida DP 25 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"531+3","v":534},0,"26\" MTB",559,"Rigida GENIUS (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"541.1+3","v":544.1},0,"26\" MTB",559,"Rigida GRIFFIN (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"536.6+3","v":539.6},0,"26\" MTB",559,"Rigida GRIZZLY (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"544.4+3","v":547.4},0,"26\" MTB",559,"Rigida LIBRA (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"546+3","v":549},0,"26\" MTB",559,"Rigida M 19 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"546+3","v":549},0,"26\" MTB",559,"Rigida M 21 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"544.1+3","v":547.1},0,"26\" MTB",559,"Rigida MENSA (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"544.1+3","v":547.1},0,"26\" MTB",559,"Rigida NORMA (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"528.9+3","v":531.9},0,"26\" MTB",559,"Rigida OLYMPUS (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"544.4+3","v":547.4},0,"26\" MTB",559,"Rigida ORION (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"538+3","v":541},0,"26\" MTB",559,"Rigida PHOENIX (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"544.4+3","v":547.4},0,"26\" MTB",559,"Rigida SIRIUS (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"544+3","v":547},0,"26\" MTB",559,"Rigida SLP (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[549,0,"26\" MTB",559,"Rigida steel Superchromix 1.75 "]
[{"$f":"540.4+3","v":543.4},0,"26\" MTB",559,"Rigida TAURUS (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"537.1+3","v":540.1},0,"26\" MTB",559,"Rigida TAURUS 2000 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"536.9+3","v":539.9},0,"26\" MTB",559,"Rigida TUB 25 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"536.9+3","v":539.9},0,"26\" MTB",559,"Rigida TUB 26 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"540.2+3","v":543.20000000000005},0,"26\" MTB",559,"Rigida TUCANA (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"534.2+3","v":537.20000000000005},0,"26\" MTB",559,"Rigida TURBO (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"526.4+3","v":529.4},0,"26\" MTB",559,"Rigida X PLORER (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"540.8+3","v":543.79999999999995},0,"26\" MTB",559,"Rigida XC 420 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"533.5+3","v":536.5},0,"26\" MTB",559,"Rigida ZAC 2000+D574","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"541+3","v":544},0,"26\" MTB",559,"Rigida/Weinmann ZAC 19 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"543+3","v":546},2.5,"26\" MTB",559,"Ritchey Disc OCR (ERD is Nipple Seat Dia + 3mm for nipples)"]
[{"$f":"542+3","v":545},2.5,"26\" MTB",559,"Ritchey OCR Comp (ERD is Nipple Seat Dia + 3mm for nipples)"]
[{"$f":"542+3","v":545},2.5,"26\" MTB",559,"Ritchey OCR Pro (ERD is Nipple Seat Dia + 3mm for nipples)"]
[{"$f":"542+3","v":545},2.5,"26\" MTB",559,"Ritchey OCR WCS (ERD is Nipple Seat Dia + 3mm for nipples)"]
[546,0,"26\" MTB",559,"Ritchey Rock 395"]
[546,0,"26\" MTB",559,"Ritchey Rock 415"]
[546,0,"26\" MTB",559,"Ritchey Rock 440SC "]
[{"$f":"544+4","v":548},0,"26\" MTB",559,"Ritchey Rock Comp (ERD is Nipple Seat Dia + 3mm for nipples)"]
[{"$f":"544+4","v":548},0,"26\" MTB",559,"Ritchey Rock Pro (ERD is Nipple Seat Dia + 3mm for nipples)"]
[{"$f":"544+4","v":548},0,"26\" MTB",559,"Ritchey Rock WCS (ERD is Nipple Seat Dia + 3mm for nipples)"]
[548,0,"26\" MTB",559,"Ritchey Vantage Comp"]
[549,0,"26\" MTB",559,"Ritchey Vantage Cross-Sport "]
[544,0,"26\" MTB",559,"Ritchey Vantage Expert "]
[545,0,"26\" MTB",559,"Ritchey Vantage Pro "]
[548,0,"26\" MTB",559,"Ritchey Vantage Sport"]
[543,0,"26\" MTB",559,"Salsa Delgado 22.5mm wide","2005-11-05","http://www.salsacycles.com/comps_rims.html"]
[545,0,"26\" MTB",559,"Salsa Gordo 27mm wide","2005-11-05","http://www.salsacycles.com/comps_rims.html"]
[544,0,"26\" MTB",559,"Salsa Semi 24mm wide","2005-11-05","http://www.salsacycles.com/comps_rims.html"]
[554,8.8000000000000007,"26\" MTB",559,"Snow Cat ASYM (44mm wide) http://www.allweathersports.com/winter/snowcats.html","2002-03-17","charlieb@prodigy.net"]
[554,0,"26\" MTB",559,"Snow Cat SYM (44mm wide) http://www.allweathersports.com/winter/snowcats.html","2002-03-17","charlieb@prodigy.net"]
[547,0,"26\" MTB",559,"Specialized GX23"]
[546,0,"26\" MTB",559,"Specialized GX26"]
[555,0,"26\" MTB",559,"Specialized Saturne HX22"]
[544,0,"26\" MTB",559,"Specialized Saturne HX28"]
[548,0,"26\" MTB",559,"Specialized Saturne HX32"]
[555,0,"26\" MTB",559,"Specialized Saturne X22"]
[544,0,"26\" MTB",559,"Specialized Saturne X28"]
[548,0,"26\" MTB",559,"Specialized Saturne X32"]
[547,0,"26\" MTB",559,"Specialized X26"]
[546,0,"26\" MTB",559,"Specialized XL21"]
[546,0,"26\" MTB",559,"Specialized XL23 "]
[545,0,"26\" MTB",559,"Specialized Z21 "]
[544,0,"26\" MTB",559,"Sun 0 degree Lite"]
[544,0,"26\" MTB",559,"Sun 0 degree XC"]
[549,0,"26\" MTB",559,"Sun AT18 "]
[471,0,"26\" MTB",559,"Sun Buzz MTB"]
[547,0,"26\" MTB",559,"Sun C16"]
[547,0,"26\" MTB",559,"Sun C20"]
[549,0,"26\" MTB",559,"Sun C20 tandem "]
[547,0,"26\" MTB",559,"Sun CR16"]
[545,0,"26\" MTB",559,"Sun CR17A"]
[544,0,"26\" MTB",559,"Sun CR18, single eyelets",null,"www.sunrims.com"]
[548,0,"26\" MTB",559,"Sun CR18 Pinned, 22.5, 32",null,"http://www.sun-ringle.com/product-vault/mtb-rims/cr18-pinned/"]
[545,0,"26\" MTB",559,"Sun CR20 "]
[548,0,"26\" MTB",559,"Sun CRE16"]
[547,0,"26\" MTB",559,"Sun CRT16"]
[548,0,"26\" MTB",559,"Sun CRT16II"]
[545,0,"26\" MTB",559,"Sun CRT17A"]
[541,0,"26\" MTB",559,"Sun DoubleWide"]
[548,0,"26\" MTB",559,"Sun DS1-XC"]
[541,0,"26\" MTB",559,"Sun Estate, 34mm, 32",null,"http://www.sun-ringle.com/mtb/rims/estate/"]
[547,0,"26\" MTB",559,"Sun L18"]
[549,0,"26\" MTB",559,"Sun L20 Style I"]
[550,0,"26\" MTB",559,"Sun L25"]
[549,0,"26\" MTB",559,"Sun M13L "]
[539,0,"26\" MTB",559,"Sun M14A"]
[550,0,"26\" MTB",559,"Sun M25"]
[548,0,"26\" MTB",559,"Sun Mammoth BFR (Big Fat Rim)"]
[534,0,"26\" MTB",559,"Sun ME14A"]
[547,0,"26\" MTB",559,"Sun Phat Albert"]
[541,0,"26\" MTB",559,"Sun Rhyno "]
[553.4,0,"26\" MTB",559,"Sun Rhyno Lite (Damon measured Nov. 06 2002)","2002-11-06","DGR"]
[541,0,"26\" MTB",559,"Sun Rhyno Lite (newer version and XL-1.75 version)"]
[544,0,"26\" MTB",559,"Sun Rhyno Lite (XL version)"]
[548,0,"26\" MTB",559,"Sun Rhyno Lite MEASURE TO BE SURE!"]
[548,0,"26\" MTB",559,"Sun Rhyno Lite XL Welded, 29.2, 32-36",null,"http://www.sun-ringle.com/product-vault/mtb-rims/rhyno-lite-xl-welded/"]
[548,0,"26\" MTB",559,"Sun Rhyno Lite Pinned, 27.5, 32-36",null,"http://www.sun-ringle.com/product-vault/mtb-rims/rhyno-lite-pinned/"]
[541,0,"26\" MTB",559,"Sun SST20"]
[544,0,"26\" MTB",559,"Sun Sub IV"]
[542,0,"26\" MTB",559,"Synchros Lil' Snapper","2003-10-06","fox-muller@comcast.net"]
[547,0,"26\" MTB",559,"Tioga XC","2003-09-06","Kelly_Paasch@und.nodak.edu"]
[536,0,"26\" MTB",559,"Velocity Aero Heat AT (24mm wide x 22mm deep)"]
[531,0,"26\" MTB",559,"Velocity Cliff Hanger (28mm wide x 25mm deep)"]
[517,0,"26\" MTB",559,"Velocity Deep V (24mm wide x 32mm deep)"]
[538,0,"26\" MTB",559,"Velocity K525 (21mm wide x 21mm deep)"]
[542,0,"26\" MTB",559,"Velocity Mt. GoAT (25mm wide x 18mm deep)"]
[540,0,"26\" MTB",559,"Velocity Synergy (23mm wide x 20mm deep, symmetrical and asymmetrical)"]
[547,0,"26\" MTB",559,"Velocity Triple V (26mm wide x 17mm deep)"]
[529.29999999999995,0,"26\" MTB",559,"Vuelta Airline 1","2001-07-17","Vuelta fax"]
[540.9,0,"26\" MTB",559,"Vuelta Excalibur DiscDH 559x27","2001-07-17","Vuelta fax"]
[543.6,0,"26\" MTB",559,"Vuelta Excalibur DiscFR 559x21","2001-07-17","Vuelta fax"]
[543.5,0,"26\" MTB",559,"Vuelta Excalibur DiscXC 559x21","2001-07-17","Vuelta fax"]
[547.1,0,"26\" MTB",559,"Vuelta Strong, no eyelets","2001-07-17","Vuelta fax"]
[543.20000000000005,0,"26\" MTB",559,"Vuelta Vision 559x18","2001-07-17","Vuelta fax"]
[545,0,"26\" MTB",559,"Weinmann Mod 2719 "]
[null,0,"26\" MTB",559,"Weinmann AS7X, 30.0, 32-36-48",null,"http://www.weinmanntek.com/Products/CTB/AS7X.htm"]
[551,0,"26\" MTB",559,"Wheelsmith Cowpie "]
[546,0,"26\" MTB",559,"Wheelsmith Speedcow "]
[551,0,"26\" MTB",559,"Wolber AT15"]
[550,0,"26\" MTB",559,"Wolber AT18"]
[547,0,"26\" MTB",559,"Wolber AT20 "]
[548,0,"26\" MTB",559,"Wolber Canyon "]
[536,0,"26\" MTB",559,"WTB Dual Duty 30x11.8 (32h, 30mm wide)","2002-06-17","thaft@wtb.com"]
[541,0,"26\" MTB",559,"WTB LaserBeam 22x11.8 (32h, 22mm wide)","2002-06-17","thaft@wtb.com"]
[538,0,"26\" MTB",559,"WTB LaserBeam 25x11.3 (32h, 25mm wide)","2002-06-17","thaft@wtb.com"]
[540,0,"26\" MTB",559,"WTB LaserDisc DH 36x0 (32h, 36mm wide)","2002-06-17","thaft@wtb.com"]
[542,0,"26\" MTB",559,"WTB LaserDisc XC 24x0 (32h, 24mm wide)","2002-06-17","thaft@wtb.com"]
[548,0,"26\" MTB",559,"WTB PowerBeam "]
[545,0,"26\" MTB",559,"WTB PowerBeam (old)"]
[541,0,"26\" MTB",559,"WTB SpeedDisc XC 24x0 (32h, 24mm wide)","2002-06-17","thaft@wtb.com"]
[541,0,"26\" MTB",559,"WTB SpeedMaster 23x11.3 (32h, 23mm wide) ","2002-06-17","thaft@wtb.com"]
[552,0,"26\" MTB",559,"WTB SpeedMaster 25mm "]
[549,0,"26\" MTB",559,"WTB SpeedMaster II "]
[{"$f":"537+3","v":540},2.5,"26\"",559,"Bontrager PN 230855 Race Lite Disc Tubeless OSB","2004-03-08","DGR"]
[{"$f":"529.2+3","v":532.20000000000005},0,"600A",540,"Rigida AS 23 X (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"528.1+3","v":531.1},0,"24x1 3/8",540,"Rigida AS 23 X (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[528,0,"24x1 3/8",540,"Sun C20"]
[527,0,"24x1 3/8",540,"Sun CR16"]
[532,0,"24x1 3/8",540,"Sun CR18, single eyelets",null,"www.sunrims.com"]
[529,0,"24x1 3/8",540,"Sun CR20 "]
[530,0,"24x1 3/8",540,"Sun L17"]
[529,0,"24x1 3/8",540,"Sun L20"]
[530,0,"24x1 3/8",540,"Sun M13II"]
[528,0,"24x1 3/8",540,"Sun M13L "]
[522,0,"24x1 3/8",540,"Sun M14A"]
[530,0,"24x1 3/8",540,"Wolber GTA"]
[{"$f":"506.6+1.5","v":508.1},0,"24x1 1/8",520,"Araya 20A  (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[500,0,"24x1 1/8",520,"Mavic Open 4 CD "]
[507,0,"24x1 1/8",520,"Sun L25, M25"]
[509,0,"24x1 1/8",520,"Sun M13II"]
[510,0,"24x1 1/8",520,"Sun M13L "]
[502,0,"24x1 1/8",520,"Sun M14A"]
[507,0,"24x1 1/8",520,"Sun M25 "]
[496,0,"24x1 1/8",520,"Sun ME14A"]
[497,0,"24\" BMX",507,"Araya 7X "]
[{"$f":"497.2+1.5","v":498.7},0,"24\" BMX",507,"Araya RB-17 (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[499,0,"24\" BMX",507,"Araya RB-907X/Super7X (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[496,0,"24\" BMX",507,"Araya RM20 "]
[{"$f":"497.2+1.5","v":498.7},0,"24\" BMX",507,"Araya VP-20 (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[{"$f":"492+3","v":495},0,"24\" BMX",507,"Bontrager Mack","2002-10-16","DGR"]
[492.5,0,"24\" BMX",507,"Mavic XY","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[{"$f":"494+3","v":497},0,"24\" BMX",507,"Rigida AS 26 FL (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"484.4+3","v":487.4},0,"24\" BMX",507,"Rigida DH 30 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"494.8+3","v":497.8},0,"24\" BMX",507,"Rigida M 19 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"494.8+3","v":497.8},0,"24\" BMX",507,"Rigida M 21 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[494,0,"24\" BMX",507,"Sun CR16"]
[493,0,"24\" BMX",507,"Sun CR18, single eyelets",null,"www.sunrims.com"]
[493,0,"24\" BMX",507,"Sun CR20 "]
[493,0,"24\" BMX",507,"Sun CRE16, CRT16II"]
[492,0,"24\" BMX",507,"Sun DS1-XC"]
[507,0,"24\" BMX",507,"Sun ICI-1"]
[493,0,"24\" BMX",507,"Sun L18"]
[497,0,"24\" BMX",507,"Sun L20"]
[497,0,"24\" BMX",507,"Sun L25, M25"]
[491,0,"24\" BMX",507,"Sun M14A"]
[497,0,"24\" BMX",507,"Sun M25 "]
[492,0,"24\" BMX",507,"Sun Mammoth BFR (Big Fat Rim)"]
[493,0,"24\" BMX",507,"Sun Rhyno Lite"]
[486,0,"24\" BMX",507,"Sun Rhyno Lite (newer version)"]
[483,0,"24\" BMX",507,"Velocity Aero Heat AT"]
[464.5,0,"24\" BMX",507,"Velocity Deep V (24mm wide x 32mm deep)"]
[480,0,"24\" BMX",507,"Velocity TAIPAN"]
[495.5,0,"24\" BMX",507,"Velocity Triple V "]
[{"$f":"478+3","v":481},0,"550A",490,"Rigida AS 23 X (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[438.7,0,"20x1 1/8",451,"Araya 20A ","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[{"$f":"430+3","v":433},0,"20x1 1/8",451,"Rigida AS 26 FL (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[439,0,"20x1 1/8",451,"Sun CR16"]
[438,0,"20x1 1/8",451,"Sun CR18, single eyelets",null,"www.sunrims.com"]
[435,0,"20x1 1/8",451,"Sun CR20 "]
[438,0,"20x1 1/8",451,"Sun ICI-1"]
[441,0,"20x1 1/8",451,"Sun L17"]
[441,0,"20x1 1/8",451,"Sun L20"]
[440,0,"20x1 1/8",451,"Sun M13II"]
[441,0,"20x1 1/8",451,"Sun M13L "]
[432,0,"20x1 1/8",451,"Sun M14A"]
[440,0,"20x1 1/8",451,"Sun M17 "]
[426,0,"20x1 1/8",451,"Sun ME14A"]
[429,0,"20x1 1/8",451,"Velocity Aerohead (20mm wide x 21mm deep)"]
[{"$f":"428.3+3","v":431.3},0,"500A",440,"Rigida AS 23 X (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[436,0,"500A",440,"Weinmann"]
[392,0,"20\" BMX",406,"ACS Z "]
[378,0,"20\" BMX",406,"Alesa Explorer"]
[376.9,0,"20\" BMX",406,"Answer Aero Tech"]
[393,0,"20\" BMX",406,"Araya GP-710 (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[396.4,0,"20\" BMX",406,"Araya MP-707X (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[379,0,"20\" BMX",406,"Araya RB-17 (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[377.9,0,"20\" BMX",406,"Araya RB-907X/Super7X (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[382,0,"20\" BMX",406,"Araya RB-J1/HIMIKO (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[392.3,0,"20\" BMX",406,"Araya TB-807X/Ultra7X (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[{"$f":"390","v":390},0,"20\" BMX",406,"Bontrager Mack"]
[{"$f":"396+3","v":399},0,"20\" BMX",406,"Mavic Xx (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[{"$f":"389+3","v":392},0,"20\" BMX",406,"Mavic Xy (ERD is Mavic's Nipple Seat Dia + 3mm for nipples)","2001-12-28","Mavic OEM brochure"]
[387.5,0,"20\" BMX",406,"Mavic XZ","2004-11-13","http://www.tech-mavic.com/uk/calcul.htm#"]
[{"$f":"392.2+3","v":395.2},0,"20\" BMX",406,"Rigida AS 26 FL (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"392.85+3","v":395.85},0,"20\" BMX",406,"Rigida M 19 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"392.85+3","v":395.85},0,"20\" BMX",406,"Rigida M 21 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"373+3","v":376},0,"20\" BMX",406,"Rigida X PLORER (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[395,0,"20\" BMX",406,"Sun AT18 "]
[389,0,"20\" BMX",406,"Sun Big City"]
[393,0,"20\" BMX",406,"Sun CR16"]
[395,0,"20\" BMX",406,"Sun CR18, single eyelets",null,"www.sunrims.com"]
[392,0,"20\" BMX",406,"Sun CR20 "]
[390,0,"20\" BMX",406,"Sun CRE16, CRT16II"]
[395,0,"20\" BMX",406,"Sun L17"]
[390,0,"20\" BMX",406,"Sun L18"]
[395,0,"20\" BMX",406,"Sun L20"]
[395,0,"20\" BMX",406,"Sun L25, M25"]
[395,0,"20\" BMX",406,"Sun M20"]
[395,0,"20\" BMX",406,"Sun M25 "]
[394,0,"20\" BMX",406,"Sun Mammoth BFR (Big Fat Rim)"]
[392,0,"20\" BMX",406,"Sun Rhyno "]
[395,0,"20\" BMX",406,"Sun Rhyno Lite"]
[395,0,"20\" BMX",406,"Sun Rhyno Lite (MEAURE TO BE SURE!)","2004-07-15","Robert Perkins <rperkins1@nc.rr.com>"]
[393,0,"20\" BMX",406,"Sun Rhyno Lite (MEAURE TO BE SURE!)"]
[392,0,"20\" BMX",406,"Sun SST20"]
[383,0,"20\" BMX",406,"Velocity Aero Heat AT"]
[364,0,"20\" BMX",406,"Velocity Deep V (24mm wide x 32mm deep)"]
[380,0,"20\" BMX",406,"Velocity TAIPAN"]
[395,0,"20\" BMX",406,"Velocity Triple V "]
[376.9,0,"20\" BMX",406,"Vuelta Airline 1","2001-07-17","Vuelta fax"]
[400,0,"20\" BMX",406,"Weinmann A129 "]
[387,0,"20\" BMX",406,"Weinmann Zac19 ","2004-07-15","Robert Perkins <rperkins1@nc.rr.com>"]
[363.7,0,"17x1 1/4",369,"Moulton, Alex (factory rim)"]
[364,0,"17x1 1/4",369,"Sun M17 Moulton"]
[345,0,"16x1 3/8",349,"Alesa Alloy 219 Brompton standard rim","2004-05-21","Wolf, Michael <m.wolf@waterman-group.co.uk>"]
[330,0,"16x1 3/8",349,"Sun M14A"]
[{"$f":"326.3+3","v":329.3},0,"400A",340,"Rigida AS 26 FL (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[288,0,"16x1.75",305,"Alex DM24","2003-05-23","Brian McDaniel <bambooland@earthlink.net>"]
[262.8,0,"16x1.75",305,"Araya GP-710 (MEASURE TO BE SURE!)","2001-12-30","http://www.araya-kk.co.jp/rim/catalog/main.html"]
[{"$f":"291.95+3","v":294.95},0,"16x1.75",305,"Rigida M 19 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[{"$f":"291.95+3","v":294.95},0,"16x1.75",305,"Rigida M 21 (ERD is Rigida's Nipple Seat Dia + 3mm for nipples)","2001-12-29","www.rigida.com/anglais/"]
[547.6,0,"26\" MTB",559,"Alex, Zuma 3.0 (Cruiser) 26\" 32 or 36H, 15mm deep, 32mm wide, ETRTO 559X26mm","2010-05-28","MFA http://www.alexrims.com/"]
[491,0,"24\" BMX",507,"Alex, Zuma 3.0 (Cruiser) 24\" 32 or 36H, 15mm deep, 32mm wide","2010-05-28","MFA http://www.alexrims.com/"]
[533.79999999999995,0,"26\" MTB",559,"Alex, Zuma 1.0 (Cruiser) 26\" 32 or 36H, 15.2mm deep, 32.8mm wide, ETRTO 559X27mm, NO RIM BRAKE","2010-05-28","MFA http://www.alexrims.com/"]
[491.4,0,"24\" BMX",507,"Alex, Zuma 1.0 (Cruiser) 24\" 32 or 36H, 15.2mm deep, 32.8mm wide, NO RIM BRAKE, ETRTO 507X27mm","2010-05-28","MFA http://www.alexrims.com/"]
[null,0,"26\" MTB",559,"Alex Y303, 36 or 48 holes, silver/black, 15.5 x 30.5, ETRTO 559X24mm","2010-05-28","MFA http://www.alexrims.com/"]
[496.6,0,"24\" BMX",507,"Alex Y303, 36 or 48 holes, silver/black, 15.5 x 30.5, ETRTO 507X24mm","2010-05-28","MFA http://www.alexrims.com/"]
[393,0,"20\" BMX",406,"Alex Y303, 36 or 48 holes, silver/black, 15.5 x 30.5, ETRTO 406X24mm","2010-05-28","MFA http://www.alexrims.com/"]
[536,0,"26\" MTB",559,"Shining MT-66, 20mm deep, 28mm wide, ETRTO 559x23, 32,36,48","2012-05-22","MFA http://www.shining-cycle.com.tw/en/product/showinfo-183.html"]
[535.25,0,"26\" MTB",559,"Weinmann ZAC 280, 20mm deep, 28mm wide, ","2018-08-09","MFA http://www.weinmanntek.com/product/2/6/49"]
[544,0,"26\" MTB",559,"Shining BX-20, 16mm deep, 30mm wide, ETRTO 559x24, 28,32,36,48","2019-08-07","MFA http://www.shining-cycle.com.tw/en/"]
[545.75,0,"26\" MTB",559,"Weinmann AS7X, 15mm deep, 30mm wide, ETRTO 559x25, 28,32,36,48","2019-08-07","MFA http://www.weinmanntek.com/product/2/6/49"]
[545,0,"26\" MTB",559,"Weinmann DM30, 16mm deep, 29.5mm wide, ETRTO 559x25, 36","2020-12-18","MFA https://www.jbi.bike/site/product_details.php?part_number=47858"]
[534.6,0,"26\" MTB",559,"RemerX Dragon L-719, 20mm deep, 24mm wide, ERTRO 559x19, 36, 32","2022-01-28","MFA https://www.messingschlager.com/en/products/rim_t67/remerx-dragon-l-719-28-29-hollow-rim_a380275-S"]
[541.29999999999995,0,"26\" MTB",559,"RemerX RMX-2021 SCR, 20mm deep, 26mm wide, ERTRO 559x21, 36","2022-01-28","MFA https://www.messingschlager.com/en/products/rim_t67/remerx-rmx-2021-scr-disc_a380227-S"]

{"sheet":"hubs","index":3,"n_rows":850,"n_cols":11,"rows_kept":850,"cut":false,"hidden":false,"merged":[]}
["S is the Spoke hole diameter, usually 2.4mm."]
["d is the diameter of the circle through the centers of the spoke holes."]
["W is the hub width from the center of the wheel to the center of the flange."]
["F/R indicates whether the hub is for a front or rear wheel."]
["OLD is the Over Lock Nut dimension, or frame spacing."]
["cogs is the number of cogs the hub accepts."]
[]
[null,"Left Flange",null,"Right Flange"]
["S, mm","dL, mm","WL, mm","dR, mm","WR, mm","F/R","cogs","OLD, mm","Hub","date","by"]
[2.6,42.5,36,42.5,36,"F",null,100,"AC APX","2001-12-28","www.dtswiss.com"]
[2.6,48,35,48,20,"R",null,135,"AC APX","2001-12-29","www.dtswiss.com"]
[2.4,42,38.5,42,18.5,"R","6,7",126,"American Classic"]
[2.4,42,41,42,16,"R",8,130,"American Classic"]
[2.4,42,36.5,42,20.5,"R","6,7",130,"American Classic"]
[2.4,42,39,42,18,"R",8,135,"American Classic"]
[2.4,42,34,42,23,"R","6,7",135,"American Classic"]
[2.4,42,36.5,42,20.5,"R",8,140,"American Classic"]
[2.6,56.5,23,56.5,36,"F",null,100,"American Classic HD-140 disc","2001-12-29","www.amclassic.com"]
[2.6,66.2,29,66.2,19,"R","8,9",135,"American Classic HD-240 Ultra-Light, 135mm Disk","2001-12-29","www.amclassic.com"]
[2.6,47,36,47,36,"F",null,100,"American Classic HH-120 suspension","2003-04-17","www.amclassic.com"]
[2.6,30,33.5,30,33.5,"F",null,100,"American Classic Micro, newer wider version","2001-12-29","www.amclassic.com"]
[2.4,30,25,30,25,"F",null,100,"American Classic Speedster, older narrow version",null,"www.amclassic.com"]
[2.4,47,36,47,36,"F",null,100,"American Classic Suspension small flange",null,"www.amclassic.com"]
[2.6,42,34.5,42,34.5,"F",null,100,"American Classic track","2001-12-29","www.amclassic.com"]
[2.6,42,30.5,42,30.5,"R",1,121,"American Classic track","2001-12-29","www.amclassic.com"]
[2.4,66.2,31,66.2,17,"R","8,9",130,"American Classic Ultra-Light, 130mm",null,"www.amclassic.com"]
[2.4,66.2,29,66.2,19,"R","8,9",135,"American Classic Ultra-Light, 135mm",null,"www.amclassic.com"]
[2.4,42,29,42,19,"R","8,9",135,"American Classic Ultra-Light, CHECK DIAMETER!","2005-10-10","OKVELO@aol.com"]
[2.6,45,35,45,20,"R",null,135,"Ariel","2001-12-29","www.dtswiss.com"]
[2.6,45,32,45,19,"R",null,135,"Bees","2001-12-29","www.dtswiss.com"]
[2.4,62.2,20.2,45.3,38.200000000000003,"F",null,100,"BikeE 16 hole disc hub","2003-05-23","Brian McDaniel <bambooland@earthlink.net>"]
[2.5,38,34.1,38,34.1,"F",null,100,"Bontrager ATB PN 200128 Superstock ","2002-02-14","dcg"]
[2.5,45,33.299999999999997,45,20.3,"R",null,135,"Bontrager ATB PN 200129 Superstock ","2002-02-14","dcg"]
[2.5,38,34.950000000000003,38,35,"F",null,100,"Bontrager ATB PN 200171 Race by Formula (semi-sealed bearings)","2002-02-22","DGR"]
[2.5,45,38.700000000000003,45,20.3,"R",null,135,"Bontrager ATB PN 210240 Race ","2002-02-14","dcg"]
[2.5,58,23.25,45,35.25,"F",null,100,"Bontrager ATB PN 210248 Race Mod Disc by DT Swiss (Onyx)","2002-02-26","DGR"]
[2.5,58,33.75,58,20.350000000000001,"R",null,135,"Bontrager ATB PN 210249 Race Mod Disc by DT Swiss (Onyx)","2002-02-19","DGR"]
[2.5,58,22.4,58,32.5,"F",null,100,"Bontrager ATB PN 220028 Select Disc ","2002-02-13","dcg"]
[2.5,58,34.4,58,20.399999999999999,"R",null,135,"Bontrager ATB PN 220029 Select Disc ","2002-02-13","dcg"]
[2.5,42,32.75,42,32.75,"F",null,100,"Bontrager ATB PN 220196 Race by Formula (sealed bearings)","2002-02-22","DGR"]
[2.5,45,38.450000000000003,58,20.25,"R","8,9",135,"Bontrager ATB PN 220197 Race by Formula (sealed bearings)","2002-06-06","DGR"]
[2.5,58,16.7,45,27.2,"F",null,100,"Bontrager ATB PN 220200 Race Disc by Formula","2002-01-02","dcg"]
[2.5,58,33.85,58,20.25,"R",null,135,"Bontrager ATB PN 220201 Race Disc by Formula","2002-01-02","dcg"]
[2.5,38,34.049999999999997,38,34.049999999999997,"F",null,100,"Bontrager ATB PN 220628 Select ","2002-02-14","dcg"]
[2.5,45,33.25,45,20.25,"R",null,135,"Bontrager ATB PN 220629 Select ","2002-02-14","dcg"]
[2.5,44,39,53,20.5,"R",null,135,"Bontrager ATB PN 220864 Race Lite by DT","2002-01-07","DGR"]
[2.5,44,36.5,53,23,"R",null,130,"Bontrager ATB PN 220864 Race Lite by DT, 130mm","2002-03-12","DGR"]
[2.5,45,38.5,58,20.2,"R",null,135,"Bontrager ATB PN 220865 Race Modified by DT Swiss (Onyx)","2001-12-31","dcg"]
[2.5,40.5,37.4,40.5,37.4,"F",null,100,"Bontrager ATB PN 220866 Race Lite by DT","2002-02-14","dcg"]
[2.5,38,35,38,35,"F",null,100,"Bontrager ATB PN 220867 Race Modified by DT Swiss (Onyx) ","2001-12-31","dcg"]
[2.5,38,35,38,35,"F",null,100,"Bontrager ATB PN 230044 sealed bearings","2002-03-12","DGR"]
[2.5,45,36.25,58,22.25,"F",null,100,"Bontrager ATB PN 230515 sealed bearings disc","2002-11-13","DGR"]
[2.5,58,33.85,58,20.25,"R",null,135,"Bontrager ATB PN 230516 sealed bearings disc","2003-10-14","DGR"]
[2.5,58,22.4,46,35.35,"F",null,100,"Bontrager ATB PN 240141 Disc, Team","2003-07-22","dcg"]
[2.5,58,34,46,19.45,"R","9,10",135,"Bontrager ATB PN 240175 Disc, Team","2003-07-22","dcg"]
[2.5,47,{"$f":"21+3.5/2","v":22.75},40,{"$f":"31.66+3.5/2","v":33.409999999999997},"F",null,100,"Bontrager ATB PN 242146 Race X Lite centerlock","2004-03-08","DGR"]
[2.5,47,{"$f":"135/2-36.8-3.5/2","v":28.950000000000003},47,{"$f":"135/2-44.6+3.5/2","v":24.65},"R",null,135,"Bontrager ATB PN 242147 Race X Lite centerlock","2004-03-08","DGR"]
[2.6,45,{"$f":"58.9-20.3","v":38.599999999999994},58,{"$f":"135/2-40.5-5-3.5/2","v":20.25},"R","8,9",135,"Bontrager ATB PN 990704 Yellow or red seals","2002-04-12","DGR"]
[2.5,45,34.25,45,19.75,"R","8,9",135,"Bontrager ATB PN Prototype LB/4 \"XT class\"","2002-03-12","DGR"]
[2.5,40,37.6,40,37.6,"F",null,100,"Bontrager ATB Race X-Lite by Chris King"]
[2.5,44,{"$f":"135/2-31.5","v":36},53,{"$f":"135/2-46.3","v":21.200000000000003},"R","8,9",135,"Bontrager ATB Race X-Lite by Chris King","2002-01-09","DGR"]
[2.5,47,23,40,34.200000000000003,"F",null,100,"Bontrager PN 242146 Race X Lite disc","2003-05-23","DGR"]
[2.5,47,33,47,21.25,"R","8,9",135,"Bontrager PN 242146 Race X Lite disc","2003-05-23","DGR"]
[{"$f":"1.35*2","v":2.7},77.8,{"$f":"130/2-32.5","v":32.5},63,{"$f":"130/2-48","v":17},"R","8,9",130,"Bontrager Power-tap 16H hi/lo proto. Even spacing. Use 1x.","2002-05-28","DGR"]
[{"$f":"0.1*25.4","v":2.54},78,{"$f":"130/2-32","v":33},66,{"$f":"130/2-45","v":20},"R","8,9",130,"Bontrager Power-tap 16H hi/lo proto. Paired. Calc1.33x, build1x.","2002-08-31","DGR"]
[2.5,78,{"$f":"130/2-33","v":32},66,{"$f":"130/2-47.5","v":17.5},"R","8,9",130,"Bontrager Power-tap 24H hi/lo proto. Paired. Calc1.25x, build1x.","2002-08-31","DGR"]
[2.5,{"$f":"31.8-2.5","v":29.3},34.9,47,17.25,"R","8,9",130,"Bontrager Road 240097,8 proto","2003-02-24","DGR"]
[2.5,47,{"$f":"31.3-3.5/2","v":29.55},47,{"$f":"19.3-3.5/2","v":17.55},"R",null,130,"Bontrager Road PN 220212 Race X-Lite.","2002-12-26","DGR"]
[2.5,38,33.450000000000003,38,33.450000000000003,"F",null,100,"Bontrager Road PN 220213 Race Lite. Radial only.","2002-02-07","DGR"]
[2.5,47,{"$f":"31.7-3.5/2","v":29.95},47,{"$f":"19.8-3.5/2","v":18.05},"R",null,130,"Bontrager Road PN 220271 Race Lite.","2002-12-26","DGR"]
[2.5,47,30,47,17,"R","8,9",130,"Bontrager Road PN 220407 Select","2002-08-30","DGR"]
[2.5,38,{"$f":"68.1/2","v":34.049999999999997},38,{"$f":"68.1/2","v":34.049999999999997},"F",null,100,"Bontrager Road PN 220622 Select","2002-09-18","DGR"]
[2.5,38,34.200000000000003,38,34.200000000000003,"F",null,100,"Bontrager Road PN 220969 RXL Aero. Radial only.","2002-02-18","dcg"]
[2.5,47,{"$f":"32.15+1","v":33.15},47,{"$f":"18.3+1","v":19.3},"R","8,9",130,"Bontrager Road PN 220970 RXL Aero. Use 1.333 cross.","2002-01-25","DGR"]
[2.5,47,30.75,47,17.25,"R","8,9",130,"Bontrager Road PN 221088 Race Lite Campy. Use  2.25 cross","2002-02-27","DGR"]
[2.7,60,{"$f":"31.35-3.5/2","v":29.6},60,{"$f":"26.35-3.5/2","v":24.6},"R","8,9",145,"Bontrager Road PN 230036 Race Lite Tandem. Use 2.25 cross.","2002-12-03","DGR"]
[2.7,60,35.450000000000003,60,35.450000000000003,"F",null,100,"Bontrager Road PN 230037 Race Lite Tandem. Use 2.25 cross.","2002-02-24","DGR"]
[2.5,38,32.299999999999997,38,32.299999999999997,"F",null,100,"Bontrager Road PN 230046 Race Lite. Radial only.","2002-03-09","DGR"]
[2.5,38,34.049999999999997,38,34.049999999999997,"F",null,100,"Bontrager Road PN 230291 Formula RXL 28H standard spacing","2002-06-03","DCG"]
[{"$f":"1.35*2","v":2.7},77.8,30.02,{"$f":"38.9*2","v":77.8},17.64,"R","8,9",130,"Bontrager Road PN 230416 Power Tap 16H. Use 1x.","2002-05-28","DGR"]
[2.5,47,{"$f":"31.8-3.5/2","v":30.05},47,{"$f":"19.8-3.5/2","v":18.05},"R","8,9",130,"Bontrager Road PN 230849, RXL road","2003-06-10","DGR"]
[2.5,38,{"$f":"(100/2)-13.4-(3.5/2)","v":34.85},38,{"$f":"C82","v":34.85},"F","8,9",100,"Bontrager Road PN 230850, RXL Aero","2003-06-05","DCG"]
[2.5,47,{"$f":"32.7+1","v":33.700000000000003},47,{"$f":"18.8+1","v":19.8},"R","8,9",130,"Bontrager Road PN 230851 RXL Aero. Use 1.333 cross.","2002-12-03","DGR"]
[2.5,{"$f":"35.8-2.5","v":33.299999999999997},{"$f":"84.1/2+1","v":43.05},{"$f":"35.8-2.5","v":33.299999999999997},{"$f":"84.1/2+1","v":43.05},"F",null,100,"Bontrager Road PN 240001 prototype 122g","2002-05-20","DGR"]
[0,39,37.5,39,37.5,"F",null,100,"Bontrager Road PN 240036 Team climbing ft hub","2003-11-07","dcg"]
[2.5,30.56,36.5,47,{"$f":"19.8-(3.55/2)","v":18.025000000000002},"R","9,10",130,"Bontrager Road PN 240097 RXXXL from DT","2004-03-05","dcg"]
[2.5,{"$f":"31.8-2.5","v":29.3},34.9,47,17.25,"R","8,9",130,"Bontrager Road PN 240097,8 proto","2003-02-24","DGR"]
[2.5,47,30.25,47,17.75,"R","8,9",130,"Bontrager Road PN 240134 Race.","2003-07-07","DGR"]
[2.5,47,{"$f":"30.25-(145-130)/2","v":22.75},47,{"$f":"17.75+(145-130)/2","v":25.25},"R","8,9",145,"Bontrager Road PN 240134 Race. Converted to 145","2003-07-07","DGR"]
[0,28.8,39.700000000000003,28.8,39.700000000000003,"F",null,100,"Bontrager Road PN 240144 proto","2003-02-24","DGR"]
[2.5,29.1,38.07,{"$f":"B91","v":29.1},{"$f":"C91","v":38.07},"F",null,100,"Bontrager Road PN 240144 RXXXL from DT","2004-03-05","dcg"]
[2.5,47,33.700000000000003,47,19.5,"R","8,9",130,"Bontrager Road PN 240441 RXL Aero. Use 1.333 cross.","2003-06-10","DGR"]
[2.5,38,34.049999999999997,38,34.049999999999997,"F",null,100,"Bontrager Road PN 240603 Race Lite. Radial or cross ok.","2003-07-07","DGR"]
[0,29.1,38.299999999999997,29.1,38.299999999999997,"F","9,10",100,"Bontrager Road PN 242220 flangless RXXXL","2003-05-20","DCG"]
[2.5,30.6,37,47,16.75,"R","9,10",130,"Bontrager Road PN 242221 flangless RXXXL - for DS calcs","2003-05-20","DCG"]
[0,30.6,37,47,16.75,"F","9,10",100,"Bontrager Road PN 242221 flangless RXXXL - for NDS calcs","2003-05-20","DCG"]
[2.6,47,30.8,47,26.8,"R","9,10",145,"Bontrager Road PN 244144 tandem low flange by Formula","2005-02-20","DGR"]
[0,28.2,38.1,28.2,38.1,"F",null,100,"Bontrager Road PN xxxxxx prototype carbon shell","2003-04-17","DCG"]
[2.5,30.9,33.799999999999997,47,18,"R","9,10",130,"Bontrager Road PN xxxxxx prototype carbon shell","2003-04-17","DCG"]
[2.5,47,33.299999999999997,47,33.299999999999997,"R",1,120,"Bontrager Track PN 240007","2003-07-24","DGR"]
[2.5,38,34.049999999999997,38,34.049999999999997,"F",null,100,"Bontrager Track PN 240008","2003-07-24","DGR"]
[2.4,57.5,25,57.5,21.5,"R",null,135,"Brave Monster 48-hole BMX freehub 8/9 cogs shimano-compatible","2006-12-02","Per Eric Rosén <per@rosnix.net>"]
[2.4,42.5,36.5,42.5,36.5,"F",null,100,"Bullseye "]
[2.4,42.5,38,42.5,21.5,"R",6,126,"Bullseye 126mm 6speed"]
[2.4,42.5,40,42.5,20.5,"R",7,130,"Bullseye 130mm 7speed"]
[2.4,53,36.5,53,36.5,"F",null,100,"Bullseye tandem "]
[2.4,53,26,53,26,"R",null,140,"Bullseye tandem "]
[2.2999999999999998,39,34,39,34,"F",null,100,"Campagnolo 1980's, 90's Chorus, C-Record, Athena low flange"]
[2.4,38.5,34.1,38.5,34.1,"F",null,100,"Campagnolo 1999+ Athena, Veloce, Mirage","2002-03-01","www.campagnolo.com"]
[2.4,44,36.5,44,16.7,"R",9,130,"Campagnolo 1999+ Athena, Veloce, Mirage","2002-03-01","www.campagnolo.com"]
[2.7,40,33.6,40,33.6,"F",null,100,"Campagnolo 1999+ Avanti","2002-03-01","www.campagnolo.com"]
[2.4,44,36.5,44,16.7,"R",8,130,"Campagnolo 1999+ Avanti","2002-03-01","www.campagnolo.com"]
[2.4,44.5,36,44.5,17,"R",8,130,"Campagnolo 8-speed cassette","2002-03-01","www.campagnolo.com"]
[2.2999999999999998,67,33,67,24,"R",5,120,"Campagnolo all 120mm hi-flange models "]
[2.2999999999999998,67,36,67,21,"R",6,126,"Campagnolo all 126mm hi-flange models "]
[2.2999999999999998,67,34,67,34,"F",null,100,"Campagnolo all hi-flange models"]
[2.2999999999999998,44,37,44,20,"R",7,127,"Campagnolo Athena, Chorus, Nuovo Record low flange"]
[2.4,44.5,35.5,44.5,18,"R",8,135,"Campagnolo Centaur 8 spd cassette"]
[2.4,44.5,36,44.5,20.5,"R",7,130,"Campagnolo Centaur, Euclid"]
[2.4,39,35.4,39,35.4,"F",null,100,"Campagnolo Chorus, Daytona OS","2002-03-01","www.campagnolo.com"]
[2.2999999999999998,44.5,36,44.5,21,"R",6,126,"Campagnolo C-Record low flange"]
[2.2999999999999998,44,33,67,24,"R",5,120,"Campagnolo Hi-Lo"]
[2.2999999999999998,38.5,35,38.5,35,"F",null,100,"Campagnolo Nuovo Record low flange"]
[2.7,44,34,44,25,"R",5,120,"Campagnolo Record","2007-02-11","\"L Travers\" <lat7575@swbell.net>"]
[2.4,39,35.35,39,35.4,"F",null,100,"Campagnolo Record OS","2002-03-01","www.campagnolo.com"]
[2.4,44,36.76,46,16.8,"R","9,10",130,"Campagnolo Record, Chorus, Daytona OS","2002-03-01","www.campagnolo.com"]
[2.2999999999999998,65,31.5,65,31.5,"F",null,100,"Campagnolo tandem "]
[2.4,65,28,65,28,"R",8,140,"Campagnolo tandem cassette"]
[2.4,67,35,67,30,"R",1,120,"Campagnolo track hi-flange C Record "]
[2.2999999999999998,67,44,67,31,"R",1,null,"Campagnolo track hi-flange Nuovo Record "]
[2.2999999999999998,44,44.5,44,31.5,"R",1,120,"Campagnolo track low flange"]
[2.2999999999999998,43.5,39.9,43.5,14.45,"R",null,130,"Cannondale by DT Swiss","2001-12-29","www.dtswiss.com"]
[2.2999999999999998,43.5,37.4,43.5,19.95,"R",null,135,"Cannondale by DT Swiss","2001-12-29","www.dtswiss.com"]
[2.5,57,35,45,19.2,"R",null,135,"Cannondale disc","2001-12-29","www.dtswiss.com"]
[2.5,58,18.350000000000001,45,31.56,"F",null,"none","Cannondale Lefty disc","2002-02-14","charlieb@attbi.com"]
[2.6,52.6,37.5,52.6,16.600000000000001,"R","8,9",135,"Cannondale Moto120","2001-10-26","Cannondale Tech Support"]
[2.2999999999999998,40,34,40,34,"F",null,100,"Chris King BMX"]
[2.2999999999999998,44,36,53,21,"R",8,135,"Chris King cassette MTB","1905-06-23","www.chrisking.com"]
[2.2999999999999998,44,38.5,53,18.5,"R",8,130,"Chris King cassette road","1905-06-23","www.chrisking.com"]
[2.2999999999999998,44,33.5,53,23.5,"R",8,140,"Chris King Classic 140mm","1905-06-23","www.chrisking.com"]
[2.2999999999999998,40,34,40,34,"F",null,100,"Chris King Classic front narrow"]
[2.2999999999999998,40,37.5,40,37.5,"F",null,100,"Chris King Classic front wide"]
[2.2999999999999998,44,36,53,21,"R",8,135,"Chris King Classic mountain","1905-06-23","www.chrisking.com"]
[2.2999999999999998,44,38.5,53,18.5,"R",8,130,"Chris King Classic road/cross","1905-06-23","www.chrisking.com"]
[2.5,57.6,23.1,57.6,31.2,"F",null,110,"Chris King Disc 20mm"]
[2.5,57.6,22.5,57.6,30.4,"F",null,100,"Chris King Disc ISO","2002-03-05","http://www.chrisking.com/specs/disc_specs.html"]
[2.5,57.6,33.9,57.6,20.100000000000001,"R","8,9",135,"Chris King Disc ISO","2002-03-05","http://www.chrisking.com/specs/disc_specs.html"]
[2.5,53,33.700000000000003,53,33.700000000000003,"R",1,135,"Chris King Disc Single Speed","2002-08-06","Chris King manual"]
[2.5,53,34.200000000000003,53,32,"R",1,135,"Chris King Disc Single Speed","2004-11-13","http://www.chrisking.com/specs/hubs_all.html"]
[2.4,53,23,53,31.5,"F",null,100,"Chris King Disc Universal"]
[2.2999999999999998,53,34,53,21,"R","8,9",135,"Chris King Disc Universal 135mm","1905-06-23","www.chrisking.com"]
[2.2999999999999998,53,31.5,53,23.5,"R",8,140,"Chris King Disc Universal 140mm","1905-06-23","www.chrisking.com"]
[2.2999999999999998,53,29,53,26,"R",8,145,"Chris King Disc Universal 145mm","1905-06-23","www.chrisking.com"]
[2.2999999999999998,40,37.5,40,37.5,"F",null,100,"Chris King MTB"]
[2.2999999999999998,44,30,53,27,"R",1,110,"Chris King Rear BMX","1905-06-23","www.chrisking.com"]
[2.2999999999999998,53,34,53,21,"R",8,135,"Chris King Rear DiscGoTech","1905-06-23","www.chrisking.com"]
[2.2999999999999998,53,31.5,53,23.5,"R",8,140,"Chris King Rear DiscGoTech","1905-06-23","www.chrisking.com"]
[2.5,53,31.5,53,23.5,"R",8,140,"Chris King Rear DiscGoTech","1905-06-23","www.chrisking.com"]
[2.2999999999999998,40,34,40,34,"F",null,100,"Chris King Road"]
[2.2999999999999998,53,33.700000000000003,53,33.700000000000003,"F",null,100,"Chris King Single Speed"]
[2.2999999999999998,53,33.700000000000003,53,33.700000000000003,"R",1,135,"Chris King Single Speed","1905-06-23","www.chrisking.com"]
[2.2999999999999998,53,33.700000000000003,53,33.700000000000003,"F",null,100,"Chris King Tandem"]
[2.2999999999999998,53,29,53,26,"R","8,9",145,"Chris King Tandem","1905-06-23","www.chrisking.com"]
[2.2999999999999998,53,33.700000000000003,53,33.700000000000003,"R","8,9",160,"Chris King Tandem","1905-06-23","www.chrisking.com"]
[2.4,39,37,39,37,"F",null,100,"CODA "]
[2.6,58,37,58,20,"R","8,9",135,"Coda 900 disc","2001-10-26","Cannondale Tech Support"]
[2.6,58,20,44.5,35,"F",null,100,"Coda 901 disc"]
[2.5,52,18,40,38,"F",null,100,"Coda disc","2001-12-28","www.dtswiss.com"]
[2.5,52.7,36,52.7,19,"R",null,135,"Coda DT Hugi 98 disc","2001-12-29","www.dtswiss.com"]
[2.6,58,19,45,30,"F",null,100,"Coda Expert disc"]
[2.6,58,35,44.5,20,"R","8,9",135,"Coda Expert disc","2001-10-26","Cannondale Tech Support"]
[2.6,44.5,31,44.5,31,"F",null,100,"Coda Expert Non-disc","2001-10-26","Cannondale Tech Support"]
[2.6,44.5,35.5,44.5,18.5,"R","8,9",135,"Coda Expert non-disc","2001-10-26","Cannondale Tech Support"]
[2.6,44.5,38.5,44.5,14.5,"R","8,9",130,"Coda Expert road","2001-10-26","Cannondale Tech Support"]
[2.6,56,25,62,31,"F",null,100,"Coda Moto disc","2001-12-28","www.dtswiss.com"]
[2.6,63.5,31.75,53.975000000000001,26.974799999999998,"R",1,null,"CORBIN DUPLEX coaster brake hub model 8"]
[2.6,51,19,39.5,34,"F",null,100,"Corratec Carbon disc","2001-12-28","www.dtswiss.com"]
[2.6,51,30,42,17,"R",null,135,"Corratec Carbon disc","2001-12-29","www.dtswiss.com"]
[2.6,55,35,55,35,"F",null,100,"Corratec Jumper","2001-12-28","www.dtswiss.com"]
[2.6,55,35,45,20,"R",null,135,"Corratec Jumper","2001-12-29","www.dtswiss.com"]
[2.6,58,34.5,58,34.5,"R",null,165,"Danny's 12mm through axle","2001-12-29","www.dtswiss.com"]
[2.5,36,35,36,35,"F",null,100,"Decathlon by DT Swiss","2001-12-28","www.dtswiss.com"]
[2.5,45,37.700000000000003,45,16.7,"R",null,130,"Decathlon by DT Swiss","2001-12-29","www.dtswiss.com"]
[2.5,45,35.200000000000003,45,19.2,"R",null,135,"Decathlon by DT Swiss","2001-12-29","www.dtswiss.com"]
[2.6,38,35,38,35,"F",null,100,"Dengler","2001-12-28","www.dtswiss.com"]
[2.4,39,37.200000000000003,39,37.200000000000003,"F",null,100,"Dia-Compe Tsali "]
[2.4,41,36,41,36,"F",null,100,"DMR Revolver","2002-10-10","Scarlett"]
[2.5,58,23,52,34.700000000000003,"F",null,100,"DT Cerit","2001-12-28","www.dtswiss.com"]
[2.5,58,33.25,52,20,"R",null,135,"DT Cerit disc","2001-12-29","www.dtswiss.com"]
[2.4,36,34.950000000000003,36,34.950000000000003,"F",null,100,"DT Hugi 240","2001-12-28","www.dtswiss.com"]
[2.4,45,37.700000000000003,45,16.7,"R",null,130,"DT Hugi 240","2001-12-29","www.dtswiss.com"]
[2.4,45,35.200000000000003,45,19.2,"R",null,135,"DT Hugi 240","2001-12-29","www.dtswiss.com"]
[2.4,45,29.8,45,16.100000000000001,"R",null,130,"DT Hugi 240 Campy 9,10s","2001-12-29","www.dtswiss.com"]
[2.5,58,22,46,34.799999999999997,"F",null,100,"DT Hugi 240 disc","2001-12-28","www.dtswiss.com"]
[2.5,58,33.5,46,19.2,"R",null,135,"DT Hugi 240 disc","2001-12-29","www.dtswiss.com"]
[2.6,58,33.5,46.5,19.2,"R",null,135,"DT Hugi 240 FR","2001-12-29","www.dtswiss.com"]
[2.6,58.5,25.8,58.5,25.8,"R",null,150,"DT Hugi 240 FR 12mm through axle","2001-12-29","www.dtswiss.com"]
[2.6,58.5,33.299999999999997,58.5,33.299999999999997,"R",null,165,"DT Hugi 240 FR 12mm through axle","2001-12-29","www.dtswiss.com"]
[2.4,45,29.8,45,16.100000000000001,"R",null,130,"DT Hugi 240 road","2001-12-29","www.dtswiss.com"]
[2.2999999999999998,45.5,39.450000000000003,45.5,17.95,"R",null,130,"DT Hugi 95","2001-12-29","www.dtswiss.com"]
[2.2999999999999998,45.5,37.4,45.5,20.05,"R",null,135,"DT Hugi 95","2001-12-29","www.dtswiss.com"]
[2.2999999999999998,41,35,41,35,"F",null,100,"DT Hugi 95 MTB","2001-12-28","www.dtswiss.com"]
[2.2999999999999998,39,34.5,39,34.5,"F",null,100,"DT Hugi 95 road","2001-12-28","www.dtswiss.com"]
[2.2999999999999998,41,35,41,35,"F",null,100,"DT Hugi 98","2001-12-28","www.dtswiss.com"]
[2.2999999999999998,45.5,39.9,45.5,17.55,"R",null,130,"DT Hugi 98","2001-12-29","www.dtswiss.com"]
[2.2999999999999998,45.5,37.299999999999997,45.5,20.149999999999999,"R",null,135,"DT Hugi 98","2001-12-29","www.dtswiss.com"]
[2.2999999999999998,46,33.65,46,16.399999999999999,"R",null,130,"DT Hugi 98 Campy 9s","2001-12-29","www.dtswiss.com"]
[2.5,52.5,16.95,46,35.1,"F",null,100,"DT Hugi Formula","2001-12-28","www.dtswiss.com"]
[2.5,52.5,33.4,46,19.649999999999999,"R","8,9",135,"DT Hugi Formula disc","2001-12-29","www.dtswiss.com"]
[2.6,58,22,52,30.2,"F",null,100,"DT Hugi FR disc","2001-12-28","www.dtswiss.com"]
[2.6,58,22,52,30.2,"F",null,110,"DT Hugi FR disc","2001-12-28","www.dtswiss.com"]
[2.8,60,36.299999999999997,61,18.95,"R",null,135,"DT Hugi Gustav M 98","2001-12-29","www.dtswiss.com"]
[2.8,60,33,61,21,"R",null,140,"DT Hugi Gustav M 98","2001-12-29","www.dtswiss.com"]
[2.8,60,23.65,61,34.85,"F",null,100,"DT Hugi Gustav M 98 disc","2001-12-28","www.dtswiss.com"]
[2.8,60,26.6,61,29.7,"F",null,110,"DT Hugi Gustav M 98 disc DH","2001-12-28","www.dtswiss.com"]
[2.5,58,23.1,46,34.4,"F",null,100,"DT Hugi Hayes","2001-12-28","www.dtswiss.com"]
[2.5,58,22.8,58,31.5,"F",null,110,"DT Hugi Hayes DH","2001-12-28","www.dtswiss.com"]
[2.5,58,33.25,46,19.75,"R","8,9",135,"DT Hugi Hayes disc","2001-12-29","www.dtswiss.com"]
[2.5,58,39,47,19.649999999999999,"R",null,135,"DT Hugi Louise 99","2001-12-29","www.dtswiss.com"]
[2.5,58,23.9,47,35.6,"F",null,100,"DT Hugi Louise 99 disc","2001-12-28","www.dtswiss.com"]
[2.8,60,36.299999999999997,61,18.95,"R","8,9",135,"DT Hugi Magura Disc Gustav M"]
[2.5,58,39,47,19.649999999999999,"R","8,9",135,"DT Hugi Magura Disc Louise"]
[2.2999999999999998,45,35,45,20.149999999999999,"R",null,135,"DT Hugi MTB"]
[2.2999999999999998,46,33.65,46,16.399999999999999,"R",9,130,"DT Hugi road Campagnolo compatible"]
[2.2999999999999998,45,39.9,45,17.55,"R","8,9",130,"DT Hugi road Shimano compatible"]
[2.2999999999999998,41,35,41,35,"F",null,100,"DT Hugi Sport","2001-12-28","www.dtswiss.com"]
[2.2999999999999998,45.5,39.450000000000003,45.5,17.95,"R",null,130,"DT Hugi Sport","2001-12-29","www.dtswiss.com"]
[2.2999999999999998,45.5,37.4,45.5,20.05,"R",null,135,"DT Hugi Sport","2001-12-29","www.dtswiss.com"]
[2.8,60,34.5,60,34.5,"F",null,100,"DT Hugi Tandem","2001-12-28","www.dtswiss.com"]
[2.8,60,34.25,60,19.45,"R","8,9",135,"DT Hugi Tandem Arai","2001-12-29","www.dtswiss.com"]
[2.8,60,31.25,60,21.45,"R","8,9",140,"DT Hugi Tandem Arai","2001-12-29","www.dtswiss.com"]
[2.8,60,28.75,60,23.95,"R","8,9",145,"DT Hugi Tandem Arai","2001-12-29","www.dtswiss.com"]
[2.8,60,22.75,61,34.4,"F",null,100,"DT Hugi Tandem disc","2001-12-28","www.dtswiss.com"]
[2.8,60,31.25,60,21.45,"R","8,9",140,"DT Hugi Tandem disc","2001-12-29","www.dtswiss.com"]
[2.8,60,28.75,60,23.95,"R","8,9",145,"DT Hugi Tandem disc","2001-12-29","www.dtswiss.com"]
[2.5,58,23,48,34.700000000000003,"F",null,100,"DT Onyx disc","2001-12-28","www.dtswiss.com"]
[2.5,58,22.8,58,31.5,"F",null,110,"DT Onyx disc","2001-12-28","www.dtswiss.com"]
[2.5,58,33.25,47,20,"R",null,135,"DT Onyx disc","2001-12-29","www.dtswiss.com"]
[2.5,40,34.200000000000003,40,34.200000000000003,"F",null,100,"DT Onyx Light","2001-12-28","www.dtswiss.com"]
[2.5,40,35.35,40,35.35,"F",null,100,"DT Onyx Normal","2001-12-28","www.dtswiss.com"]
[2.5,46,32.1,46,17.5,"R",null,130,"DT Swiss Onyx","2001-12-29","www.dtswiss.com"]
[2.5,46,29.6,46,20,"R",null,135,"DT Swiss Onyx","2001-12-29","www.dtswiss.com"]
[2.5,41,35,41,35,"F",null,100,"Edco","2001-12-28","www.dtswiss.com"]
[2.5,45,34,45,19,"R",null,135,"Edco","2001-12-29","www.dtswiss.com"]
[2.5,178,20,178,20,"F",null,100,"EMAG hub motor","2006-12-02","Per Eric Rosén\" <per@rosnix.net> http://www.electro-mobile.se/navmotor.htm and measurments"]
[2.6,42,33,42,33,"F",null,100,"Fimoco","2001-12-28","www.dtswiss.com"]
[2.6,48,33,48,21,"R",null,135,"Formula","2001-12-29","www.dtswiss.com"]
[2.5,52.5,19.649999999999999,46,35.1,"F",null,100,"Formula by DT Swiss","2001-12-28","www.dtswiss.com"]
[2.5,52.5,33.4,46,19.649999999999999,"R",null,135,"Formula by DT Swiss","2001-12-29","www.dtswiss.com"]
[2.6,51,18,51,34,"F",null,100,"Formula by Edco","2001-12-28","www.dtswiss.com"]
[2.6,51,32,51,20,"R",null,135,"Formula by Edco","2001-12-29","www.dtswiss.com"]
[2.6,45,22,45,33,"F",null,110,"Formula DH","2001-12-28","www.dtswiss.com"]
[2.6,48,19,48,38,"F",null,100,"Formula disc","2001-12-28","www.dtswiss.com"]
[0,{"$f":"29+4","v":33},{"$f":"77/2","v":38.5},{"$f":"29+4","v":33},{"$f":"77/2","v":38.5},"F",null,100,"Formula Engineering SP92, road straight pull spokes.","2002-12-27","DGR"]
[2.4,35,34.5,35,34.5,"F",null,100,"FRM FL-R TEAM CA (road only)","2006-12-02","Franco <frmbike@libero.it> frmbike.com"]
[2.4,36,29,42,18,"R",null,130,"FRM FL-R TEAM CA (road only)","2006-12-02","Franco <frmbike@libero.it> frmbike.com"]
[2.4,59,28.3,59,28.3,"F",null,100,"FRM FL-M TEAM (MTB)","2006-12-02","Franco <frmbike@libero.it> frmbike.com"]
[2.4,59,39.4,59,17.2,"R",null,135,"FRM FL-M TEAM (MTB)","2006-12-02","Franco <frmbike@libero.it> frmbike.com"]
[2.4,59,22.9,59,33.700000000000003,"F",null,100,"FRM FL-M TEAM DISC (MTB)","2006-12-02","Franco <frmbike@libero.it> frmbike.com"]
[2.4,59,39.4,59,17.2,"R",null,135,"FRM FL-M TEAM DISC (MTB)","2006-12-02","Franco <frmbike@libero.it> frmbike.com"]
[2.4,59,22.9,59,33.700000000000003,"F",null,"-","FRM \"Lefty\" FL-M TEAM DISC (MTB)","2006-12-02","Franco <frmbike@libero.it> frmbike.com"]
[2.4,38,34.4,38,34.4,"F",null,100,"FRM FL-R PRO & FL-M PRO (road & MTB)","2006-12-02","Franco <frmbike@libero.it> frmbike.com"]
[2.4,38,37.700000000000003,45,18.600000000000001,"R",null,130,"FRM FL-R PRO (road only)","2006-12-02","Franco <frmbike@libero.it> frmbike.com"]
[2.4,38,56.3,45,21.1,"R",null,135,"FRM FL-M PRO (MTB)","2006-12-02","Franco <frmbike@libero.it> frmbike.com"]
[2.4,44,22.8,38,33.700000000000003,"F",null,100,"FRM FL-M PRO DISC","2006-12-02","Franco <frmbike@libero.it> frmbike.com"]
[2.4,45,33.9,45,20.399999999999999,"R",null,135,"FRM FL-M PRO DISC","2006-12-02","Franco <frmbike@libero.it> frmbike.com"]
[2.4,34,34.5,34,34.5,"F",null,100,"FRM Comp & Pro","2002-06-14","www.frmbike.com"]
[2.4,37.5,34,41,18.5,"R",null,130,"FRM Comp & Pro","2002-06-14","www.frmbike.com"]
[2.4,37.5,36.5,41,21,"R",null,135,"FRM Comp & Pro","2002-06-14","www.frmbike.com"]
[2.4,35,34.5,35,34.5,"F",null,100,"FRM Feather Front","2002-06-14","www.frmbike.com"]
[2.4,44,23,38,33.4,"F",null,100,"FRM FL Disc Comp & Pro","2002-06-14","www.frmbike.com"]
[2.4,45,34.4,45,21,"R",null,135,"FRM FL Disc Comp & Pro","2002-06-14","www.frmbike.com"]
[2.4,37.5,34,41,18.5,"R",null,130,"FRM Team SL Rear","2002-06-14","www.frmbike.com"]
[2.6,58,19,54,34,"F",null,100,"Giant disc","2001-12-28","www.dtswiss.com"]
[2.6,58,33,54,20,"R",null,135,"Giant disc","2001-12-29","www.dtswiss.com"]
[2.2999999999999998,40.200000000000003,35.1,40.200000000000003,35.1,"F",null,100,"Gipiemme Special (Campy low flange copy)"]
[2.2999999999999998,44.5,36.799999999999997,44.5,20.3,"R",7,127,"Gipiemme Special (Campy low flange copy)",null,"DGR"]
[2.2999999999999998,44.5,29.5,44.5,27.9,"R",1,120,"Gipiemme Special (respaced from road to track)",null,"DGR"]
[2.4,66,36,66,36,"R",1,135,"Goldtec Track Hub","2002-10-17","Scarlett"]
[2.6,45,34,45,18,"R",null,135,"Goldtec-Ti","2001-12-29","www.dtswiss.com"]
[2.6,38,36,38,36,"F",null,100,"GT","2001-12-28","www.dtswiss.com"]
[2.6,45,35,45,22,"R",null,135,"GT","2001-12-29","www.dtswiss.com"]
[2.6,60,34,60,20,"R",null,135,"Hadley 12mm through axle","2001-12-29","www.dtswiss.com"]
[2.6,56,30,56,30,"R",null,160,"Hadley Arai","2001-12-29","www.dtswiss.com"]
[2.6,60,22.6,60,31.4,"F",null,110,"Hadley H500 DH","2001-12-28","www.dtswiss.com"]
[2.6,60,33.5,60,33.5,"R",null,160,"Hadley Santa Cruz 14mm through axle","2001-12-29","www.dtswiss.com"]
[2.8,55,17,55,43,"F",null,null,"Hanebrink LT 8 disc","2001-12-28","www.dtswiss.com"]
[2.6,62,34.5,62,34.5,"F",null,100,"Harris Cyclery High-flange track hub","2007-02-11","\"Sheldon Brown\" <CaptBike@sheldonbrown.com>"]
[2.6,62,31,62,31,"R",null,120,"Harris Cyclery High-flange track hub","2007-02-11","\"Sheldon Brown\" <CaptBike@sheldonbrown.com>"]
[2.5,56,{"$f":"135/2-35","v":32.5},56,{"$f":"135/2-50","v":17.5},"R","8,9",135,"Hayes by EDCO","2002-11-06","DGR"]
[2.5,58,23,48,34.700000000000003,"F",null,100,"Hayes Elite disc","2001-12-28","www.dtswiss.com"]
[2.5,58,33.25,47,20,"R",null,135,"Hayes Elite disc","2001-12-29","www.dtswiss.com"]
[2.5,58,22.8,58,31.5,"F",null,110,"Hayes Elite disc DH","2001-12-28","www.dtswiss.com"]
[2.5,58,22,46,34.799999999999997,"F",null,100,"Hayes Superlight disc","2001-12-28","www.dtswiss.com"]
[2.5,58,33.5,46,19.2,"R",null,135,"Hayes Superlight disc","2001-12-29","www.dtswiss.com"]
[2.4,31.5,32,31.5,32,"F",null,100,"Hershey Naked "]
[2.4,31.5,34,31.5,34,"F",null,100,"Hershey Standard Ti "]
[2.4,44.5,34,44.5,34,"F",null,100,"Hershey Suspension "]
[2.4,36.5,33,48,21,"R",null,135,"Hershey Ti "]
[2.6,33,32,33,32,"F",null,100,"Heylight","2001-12-28","www.dtswiss.com"]
[2.6,45,33,44,20,"R",null,135,"Heylight","2001-12-29","www.dtswiss.com"]
[2.6,46,24,33,26,"F",null,100,"Heylight disc","2001-12-28","www.dtswiss.com"]
[2.6,46,39,44,19,"R",null,135,"Heylight disc","2001-12-29","www.dtswiss.com"]
[2.6,29,34,29,34,"F",null,100,"Heylight Mini","2001-12-28","www.dtswiss.com"]
[3,34.700000000000003,32.799999999999997,54,19,"R",8,130,"Hi-E cassette Hi-Lo flange, custom narrow spacing"]
[2.6,62,20,62,25,"F",null,100,"Hope Big'Un","2001-12-28","www.dtswiss.com"]
[2.6,62,25,62,20,"R",null,135,"Hope Big'Un","2001-12-29","www.dtswiss.com"]
[2.6,46,21,46,34,"F",null,100,"Hope Bulb","2001-12-28","www.dtswiss.com"]
[2.6,44,33,50,20,"R",null,135,"Hope Bulb","2001-12-29","www.dtswiss.com"]
[2.6,56,21,46.7,33,"F",null,100,"Hope Bulb IS2000","2001-12-28","www.dtswiss.com"]
[2.6,56,33,49,19,"R",null,135,"Hope Bulb IS2000","2001-12-29","www.dtswiss.com"]
[2.6,42,22,42,32,"F",null,100,"Hope disc","2001-12-28","www.dtswiss.com"]
[2.6,42,33,45,20,"R",null,135,"Hope disc","2001-12-29","www.dtswiss.com"]
[2.4,41,34.5,41,34.5,"F",null,100,"Hope Fatso "]
[2.6,56,20,45,34,"F",null,100,"Hope Sport disc","2001-12-28","www.dtswiss.com"]
[2.6,45,33,45,20,"R",null,135,"Hope Sport disc","2001-12-29","www.dtswiss.com"]
[2.4,25,34,25,34,"F",null,100,"Hope Super Ultralight "]
[2.4,43,32,43,32,"F",null,100,"Hope Suspension "]
[2.4,65,32.5,65,32.5,"F",null,100,"Hope tandem "]
[2.4,65,27.5,65,22.5,"R",null,140,"Hope tandem "]
[2.4,43,32,43,32,"F",null,100,"Hope Tech "]
[2.4,43,22.5,43,22.5,"F",null,100,"Hope Tech, narrower flanges"]
[2.4,34,34,34,34,"F",null,100,"Hope Tech, Ultralight"]
[2.6,43,22,41,32.5,"F",null,100,"Hope Ti-Glide disc","2001-12-28","www.dtswiss.com"]
[2.6,43,33,44.5,20,"R",null,135,"Hope Ti-Glide disc","2001-12-29","www.dtswiss.com"]
[2.4,45,37.5,45,20,"R",null,null,"Hugi "]
[2.4,36,34.950000000000003,36,34.950000000000003,"F",null,100,"Hugi 240"]
[2.5,52.5,16.95,46,35.1,"F",null,100,"Hugi Formula Disc"]
[2.5,58,23.7,46,35.1,"F",null,100,"Hugi Hayes Disc"]
[2.8,60,23.65,61,34.85,"F",null,100,"Hugi Magura Disc Gustav M"]
[2.8,60,26.6,61,29.7,"F",null,110,"Hugi Magura Disc Gustav M downhill"]
[2.5,58,23.9,47,35.6,"F",null,100,"Hugi Magura Disc Louise"]
[2.4,45,39.5,45,18,"R",8,130,"Hugi road "]
[2.4,45,37.5,45,20,"R",null,135,"Hugi road "]
[2.2999999999999998,55,37,55,22,"R",8,null,"Hugi tandem"]
[2.4,41,35,41,35,"F",null,100,"Hugi tandem "]
[2.4,55,33.5,55,24,"R",null,140,"Hugi tandem "]
[2.8,60,34.5,60,34.5,"F",null,100,"Hugi tandem large flange"]
[2.8,60,34.5,60,34.5,"F",null,100,"Hugi TD (tandem) 2001"]
[2.8,60,31.25,60,21.45,"R","8,9",140,"Hugi TD (tandem) 2001"]
[2.8,60,28.75,60,23.95,"R","8,9",145,"Hugi TD (tandem) 2001"]
[2.8,60,21.6,61,34.5,"F",null,100,"Hugi TD disc brake (tandem) 2001"]
[2.5,39,33,39,33,"F",null,100,"Hugi/Union Std.","2001-12-28","www.dtswiss.com"]
[2.5,41,35,41,35,"F",null,100,"Hugi/Union/Marwi Susp.","2001-12-28","www.dtswiss.com"]
[2.6,5538,21,55.8,33,"F",null,100,"Inferno disc","2001-12-28","www.dtswiss.com"]
[2.6,55.8,35,55.8,21,"R",null,135,"Inferno disc","2001-12-29","www.dtswiss.com"]
[2.6,60,24,60,31,"F",null,110,"Intense 20mm disc","2001-12-28","www.dtswiss.com"]
[2.6,62,34.5,62,34.5,"F",null,100,"IRO High-flange track hub","2006-12-02","http://www.irocycle.com/hubspec.html"]
[2.6,62,31,62,31,"R",null,120,"IRO High-flange track hub","2006-12-02","http://www.irocycle.com/hubspec.html"]
[2.6,40,36,40,36,"F",null,100,"IRO Single Speed hub","2006-12-02","http://www.irocycle.com/hubspec.html"]
[2.6,53,39,53,39,"R",null,135,"IRO Single Speed hub","2006-12-02","http://www.irocycle.com/hubspec.html"]
[2.6,58,38,58,34,"R",null,135,"IRO Single Speed disc brake hub","2006-12-02","http://www.irocycle.com/hubspec.html"]
[2.4,44,28.5,44,28.5,"F",null,100,"Joytech sealed med flange"]
[2.4,42.5,34.5,42.5,34.5,"F",null,100,"Kingsbery low flange "]
[2.4,42.5,34.5,42.5,23.5,"R",null,135,"Kingsbery low flange 135mm"]
[2.5,52,38.5,52,38.5,"R",1,135,"Kogswell double fixed mtb/singlespeed rear","2003-10-06","CaptBike@sheldonbrown.com"]
[2.5,40,36.1,40,36.1,"F",null,100,"Kogswell front","2003-10-06","CaptBike@sheldonbrown.com"]
[2.5,58.5,{"$f":"110/2-25","v":30},51,{"$f":"110/2-16-3.5/2","v":37.25},"F",null,110,"M bits","2003-10-11","DGR"]
[2.4,43,33,43,33,"F",null,100,"Machine Tech Hollowcore "]
[2.4,43,34,43,20.5,"R",null,135,"Machine Tech Power Claw "]
[2.5,62.5,30.4,62.5,20.8,"R",9,135,"Magura 1999 Louise disc"]
[2.5,58,23,48,34.700000000000003,"F",null,100,"Magura Comp 2000","2001-12-28","www.dtswiss.com"]
[2.5,58,33.25,47,20,"R",null,135,"Magura Comp 2000","2001-12-29","www.dtswiss.com"]
[2.5,58,22.8,58,31.5,"F",null,110,"Magura Comp 2000 DH","2001-12-28","www.dtswiss.com"]
[2.5,58,23,52,34.700000000000003,"F",null,100,"Magura Fun","2001-12-28","www.dtswiss.com"]
[2.5,58,33.25,52,20,"R",null,135,"Magura Fun","2001-12-29","www.dtswiss.com"]
[2.5,58,23.1,46,34.4,"F",null,100,"Magura Gustav M 2000","2001-12-28","www.dtswiss.com"]
[2.5,58,33.25,46,19.75,"R",null,135,"Magura Gustav M 2000","2001-12-29","www.dtswiss.com"]
[2.5,58,22.8,58,31.5,"F",null,110,"Magura Gustav M 2000 DH","2001-12-28","www.dtswiss.com"]
[2.8,60,23.65,61,34.85,"F",null,100,"Magura Gustav M 99","2001-12-28","www.dtswiss.com"]
[2.8,60,36.299999999999997,61,18.95,"R",null,135,"Magura Gustav M 99","2001-12-29","www.dtswiss.com"]
[2.8,60,26.6,61,29.7,"F",null,110,"Magura Gustav M 99 DH","2001-12-28","www.dtswiss.com"]
[2.5,58,22,46,34.799999999999997,"F",null,100,"Magura Pro 2000","2001-12-28","www.dtswiss.com"]
[2.5,58,33.5,46,19.2,"R",null,135,"Magura Pro 2000","2001-12-29","www.dtswiss.com"]
[2.8,62,31,62,20,"R",null,135,"Magura/SRAM louise 99","2001-12-29","www.dtswiss.com"]
[2.8,62,20,62,30,"F",null,100,"Magura/SRAM Louise 99 disc","2001-12-28","www.dtswiss.com"]
[2.4,67.5,35.9,67.5,20.9,"R",5,122.4,"Maillard Professional High Flange","2007-02-11","\"L Travers\" <lat7575@swbell.net>"]
[2.4,67.5,33,67.5,33,"F",null,99,"Maillard Professional High Flange","2007-02-11","\"L Travers\" <lat7575@swbell.net>"]
[2.6,40,40,40,40,"F",null,null,"Manitou through axle, non-disc","2001-12-28","www.dtswiss.com"]
[2.6,56,36,56,36,"F",null,null,"Marzocchi QR 20","2001-12-28","www.dtswiss.com"]
[2.6,58,22,58,31,"F",null,null,"Marzocchi QR 20 disc","2001-12-28","www.dtswiss.com"]
[3,61,19,61,33,"F",null,null,"Marzocchi QR 20+ disc","2001-12-28","www.dtswiss.com"]
[2.5,58,29.4,50,36.5,"F",null,110,"Maverick American hub","2004-10-27","http://www.maverickamerican.com/pdfs/maverick_hub_specs.pdf"]
[2.5,40,27,40,27,"F",null,100,"Mavic 500, 501, 520, 530, 531, 550, 571, 577"]
[2.4,44.5,30,44.5,18,"R",7,126,"Mavic 501 "]
[2.4,44.5,31.5,44.5,16.5,"R",8,130,"Mavic 501 "]
[2.4,44.5,37,44.5,19,"R",6,126,"Mavic 506 "]
[2.4,44.5,42.5,44.5,30.5,"R",1,120,"Mavic 520 track low flange"]
[2.4,44.5,29.5,44.5,18.5,"R",null,130,"Mavic 531 MTB "]
[2.4,44.5,27,44.5,21,"R",null,135,"Mavic 531 MTB "]
[2.4,45,37.700000000000003,45,19.2,"R",6,126,"Mavic 550"]
[2.4,45,36,45,26,"R",1,120,"Mavic 570"]
[2.4,53,32,53,16.5,"R",null,130,"Mavic 571 road "]
[2.4,53,35,53,19,"R",null,130,"Mavic 571, 572 "]
[2.4,53,31.5,53,17,"R",null,135,"Mavic 577 MTB "]
[0,27,36,27,36,"F",null,100,"Mavic Cosmic Carbone 2001 blk. STRAIGHT SPOKES","2001-12-30","DGR"]
[2.4,40,34,40,34,"F",null,100,"Mavic MR601"]
[2.4,46,34,48,17.399999999999999,"R","8,9",130,"Mavic MR601"]
[2.4,34,28,34,28,"F",null,80,"Mavic special small TT hub"]
[2.6,32,35,32,35,"F",null,100,"Maxx","2001-12-28","www.dtswiss.com"]
[2.5,59,45,59,30,"R",1,120,"Miche track","2001-12-29","www.dtswiss.com"]
[2.6,62,34,62,34,"F",null,100,"Nashbar Fixed-Fixed Flip-Flop front hub NF-GHF","2005-11-05","nashbar.com"]
[2.6,62,31,62,31,"R",1,120,"Nashbar Fixed-Fixed Flip-Flop rear hub NF-GHR","2005-11-05","nashbar.com"]
[2.8,60,21.5,60,33.9,"F",null,100,"NC 17 disc","2001-12-28","www.dtswiss.com"]
[2.8,60,31.7,60,18.2,"R",null,135,"NC 17 disc","2001-12-29","www.dtswiss.com"]
[2.8,60,21.5,60,33.9,"F",null,110,"NC 17 disc DH","2001-12-28","www.dtswiss.com"]
[2.8,60,19,60,36,"F",null,null,"Nicolai Nucleon NC 17 95mm 20mm through axle","2001-12-28","www.dtswiss.com"]
[2.4,63,33.700000000000003,63,33.700000000000003,"F",null,100,"Normandy high flange"]
[2.4,63,39,63,19,"R",5,120,"Normandy high flange","2002-12-03","Jim McKim"]
[2.4,63,42,63,16,"R","6,7",126,"Normandy high flange respaced to 126mm","2002-12-03","Jim McKim"]
[2.6,31,35.25,31,35.25,"F",null,100,"Nuke Proof"]
[2.4,32,45,43.1,20,"R",null,126,"Nuke Proof "]
[2.4,32,43,43.1,22,"R",null,130,"Nuke Proof "]
[2.4,32,41,43.1,25,"R",null,135,"Nuke Proof "]
[2.4,32,36.5,32,36.5,"F",null,"BMX","Nuke Proof "]
[2.4,47,42,47,19.5,"R",null,130,"Nuke Proof Bombshell cassette "]
[2.4,47,41,47,21,"R",null,135,"Nuke Proof Bombshell cassette "]
[2.4,47,38,47,38,"F",null,100,"Nuke Proof Bombshell, post '95"]
[2.4,42.2,34,42.2,34,"F",null,100,"Nuke Proof Bombshell, pre '95"]
[2.4,32,45,47.3,20,"R",null,126,"Nuke Proof XT cassette "]
[2.4,32,43,47.3,22,"R",null,130,"Nuke Proof XT cassette "]
[2.4,32,40,47.3,25,"R",null,135,"Nuke Proof XT cassette "]
[2.4,32,38.5,47.5,20,"R",null,130,"Nuke Proof XTR cassette "]
[2.4,32,38.5,47.3,21,"R",null,135,"Nuke Proof XTR cassette "]
[2.4,32,33,32,33,"F",null,100,"Nuke Proof, older models"]
[2.5,46,27,46,27,"R",null,120,"On-one 120mm Double Fixed","2006-12-02","Jon Senior <jon@restlesslemon.co.uk>"]
[2.4,44.5,32,44.5,32,"F",null,100,"Pace carbon sealed "]
[2.4,44.5,38,44.5,22.5,"R",null,135,"Pace carbon sealed "]
[2.4,43,36,43,36,"F",null,100,"Paul Components "]
[2.2999999999999998,55,35,55,22,"R",8,130,"Phil Wood Cassette"]
[2.4,57.5,27.8,57.5,27.8,"F",null,100,"Phil Wood Cross Country "]
[2.4,48.5,34.5,48.5,34.5,"F",null,100,"Phil Wood Field Serviceable "]
[2.4,48.5,37.6,48.5,19.399999999999999,"R",null,126,"Phil Wood Field Serviceable "]
[2.4,48.5,34.9,48.5,22.1,"R",null,130,"Phil Wood Field Serviceable "]
[2.4,48.5,32.4,48.5,24.6,"R",null,135,"Phil Wood Field Serviceable "]
[2.4,48.5,39,48.5,18,"R",null,140,"Phil Wood Field Serviceable "]
[2.4,48.5,38,69,19,"R",null,126,"Phil Wood Hi right hand flange"]
[2.4,48.5,36.6,69,20.399999999999999,"R",null,130,"Phil Wood Hi right hand flange"]
[2.4,48.5,34.5,48.5,34.5,"F",null,100,"Phil Wood medium original "]
[2.4,48.5,38,48.5,19,"R",null,126,"Phil Wood medium original "]
[2.4,48.5,31,48.5,26,"R",null,140,"Phil Wood medium original "]
[2.4,48.5,38,57.5,19,"R",null,126,"Phil Wood Mid "]
[2.4,48.5,36,57.5,21,"R",null,130,"Phil Wood Mid "]
[2.4,57.5,36.700000000000003,48.2,20.3,"R",6,125,"Phil Wood MTB 6speed "]
[2.4,57.5,34.200000000000003,48.2,22.8,"R",6,130,"Phil Wood MTB 6speed "]
[2.4,57.5,31.7,48.2,25.3,"R",6,135,"Phil Wood MTB 6speed "]
[2.4,57.5,37.5,48.2,19.5,"R",7,126,"Phil Wood MTB 7speed "]
[2.4,57.5,35.700000000000003,48.2,21.3,"R",7,130,"Phil Wood MTB 7speed "]
[2.4,57.5,33.200000000000003,48.2,23.8,"R",7,135,"Phil Wood MTB 7speed "]
[2.4,57.5,30.7,48.2,26.3,"R",7,140,"Phil Wood MTB 7speed "]
[2.4,57.5,39,48.2,18,"R",8,130,"Phil Wood MTB 8speed "]
[2.4,57.5,38.200000000000003,48.2,18.8,"R",8,135,"Phil Wood MTB 8speed "]
[2.4,58.5,35.700000000000003,49.2,21.3,"R",8,140,"Phil Wood MTB 8speed "]
[2.4,48.2,34.200000000000003,48.2,22.8,"R",5,120,"Phil Wood road 5speed "]
[2.4,48.2,31.7,48.2,25.3,"R",5,126,"Phil Wood road 5speed "]
[2.4,48.2,36.700000000000003,48.2,20.3,"R",6,126,"Phil Wood road 6speed "]
[2.4,48.2,34.200000000000003,48.2,22.8,"R",6,130,"Phil Wood road 6speed "]
[2.4,48.2,31.7,48.2,25.3,"R",6,135,"Phil Wood road 6speed "]
[2.4,48.2,37.200000000000003,48.2,19.8,"R",7,126,"Phil Wood road 7speed "]
[2.4,48.2,35.700000000000003,48.2,21.3,"R",7,130,"Phil Wood road 7speed "]
[2.4,48.2,33.200000000000003,48.2,23.8,"R",7,135,"Phil Wood road 7speed "]
[2.4,48.2,39,48.2,18,"R",8,130,"Phil Wood road 8speed "]
[2.4,48.2,38.200000000000003,48.2,18.8,"R",8,135,"Phil Wood road 8speed "]
[2.4,48.2,35.700000000000003,48.2,21.3,"R",8,140,"Phil Wood road 8speed "]
[2.4,42.5,35,42.5,35,"F",null,100,"Phil Wood small old "]
[2.4,42.5,38,48.5,19,"R",null,126,"Phil Wood small old "]
[2.4,42.5,36,48.5,21,"R",null,130,"Phil Wood small old "]
[2.4,42.5,33.5,48.5,23.5,"R",null,135,"Phil Wood small old "]
[2.4,57.5,35.299999999999997,57.5,35.299999999999997,"F",null,100,"Phil Wood Suspension "]
[2.4,48.5,37.5,48.5,37.5,"F",null,100,"Phil Wood Time Trial "]
[2.4,48.2,30,48.2,30,"R",1,120126130,"Phil Wood track double-sided, small flange","2003-05-07","www.philwood.com"]
[2.4,48.2,34.5,48.2,34.5,"F",null,100,"Phil Wood track front, small flange","2003-05-07","www.philwood.com"]
[2.4,48.5,44,48.5,30,"R",1,120126130,"Phil Wood track one-sided, small flange","2003-05-07","www.philwood.com"]
[2.6,66,{"$f":"120/2-17","v":43},66,{"$f":"120/2-31","v":29},"R",1,120,"Phil Wood track, large flange","2003-03-29","DGR"]
[2.4,41,29.5,41,29.5,"R",null,null,"Phil Wood wheelchair"]
[2.8,45,32,45,21,"R",null,135,"Point HR","2001-12-29","www.dtswiss.com"]
[2.4,78,36.200000000000003,66,16.7,"R","8,9",130,"Power-tap","2001-07-17","Adam at Graber"]
[2.4,78,{"$f":"135/2-37","v":30.5},66,{"$f":"135/2-48","v":19.5},"R","8,9",153,"Power-tap ATB","2002-08-02","DGR"]
[2.5,{"$f":"35*2","v":70},31.8,70,18,"R","8,9",130,"Power-tap SL","2004-12-07","DGR"]
[2.4,41.3,32.5,41.3,32.5,"F",null,100,"Pulstar 28 hole"]
[2.4,47.6,32.5,47.6,32.5,"F",null,100,"Pulstar 32 hole"]
[2.4,47.6,32,47.6,22,"R",7,null,"Pulstar 7-spd 32-hole "]
[2.4,50.8,32,50.8,22,"R",7,null,"Pulstar 7-spd 36-hole"]
[2.4,47.6,34,47.6,20,"R",8,null,"Pulstar 8-spd 32-hole "]
[2.4,50.8,34,50.8,20,"R",8,null,"Pulstar 8-spd 36-hole"]
[2.6,48,35,48,35,"F",null,100,"Pure Power","2001-12-28","www.dtswiss.com"]
[2.4,40,34,40,34,"F",null,100,"Real front"]
[2.4,37,37,54.5,21,"R","8,9",null,"Real rear, not for disc brake"]
[2.4,40,41.5,41,22.5,"R",6,130,"Ringlé 6-spd MTB "]
[2.4,40,38.5,41,25.5,"R",7,135,"Ringlé 7-spd MTB "]
[2.4,40,43,41,21,"R",7,126,"Ringlé 7-spd road "]
[2.4,40,39.5,41,20.5,"R",8,135,"Ringlé 8-spd MTB "]
[2.4,40,42,41,18,"R",8,130,"Ringlé 8-spd road "]
[2.4,40,34,40,34,"F",null,100,"Ringlé Bubba "]
[2.6,40,38.5,41,25.5,"R",null,135,"Ringlé Bubba HR freewheel","2001-12-29","www.dtswiss.com"]
[2.6,45,34,45,22,"R",null,135,"Ringlé Super Bubba","2001-12-29","www.dtswiss.com"]
[2.4,42,34,42,34,"F",null,100,"Ringlé Super Bubba "]
[2.6,46,34,46,34,"F",null,100,"Ringlé Super Duper Bubba ","2001-12-28","www.dtswiss.com"]
[2.6,52,34,52,21,"R",8,135,"Ringlé SuperDuper Eight MTB "]
[2.4,45,34,45,22,"R",8,135,"Ringlé SuperEight MTB "]
[2.4,45,36.5,45,19.5,"R",8,130,"Ringlé SuperEight road "]
[2.4,38,32,38,32,"F",null,100,"Ringlé/Sun \"Sun of Bubba\""]
[2.8,58,22,58,35,"F",null,100,"Ritchey disc Pro Skraxle","2001-12-28","www.dtswiss.com"]
[2.8,58,35,58,20,"R",null,135,"Ritchey Pro disc","2001-12-29","www.dtswiss.com"]
[2.4,38,38,38,38,"F",null,100,"Ritchey Z-hub MTB: WCS, Pro, Comp"]
[2.4,45,28.1,45,21.9,"R","8,9",130,"Ritchey Z-hub MTB: WCS, Pro, Comp"]
[2.4,45,28.6,45,21.3,"R","8,9",130,"Ritchey Z-hub road: Pro"]
[2.4,45,28.5,45,21.5,"R","8,9",130,"Ritchey Z-hub road: WCS"]
[2.4,38,36,38,36,"F",null,100,"Ritchey Z-hub road: WCS, Pro"]
[{"$f":"0.1*25.4","v":2.54},62,{"$f":"110/2-31","v":24},62,{"$f":"110/2-23","v":32},"F",null,110,"Rocky Mountain disc QR20","2002-10-16","DGR"]
[2.5,100,30,100,30,"R",null,null,"Rohloff Speed Hub 500/14","2001-12-29","www.dtswiss.com"]
[2.5,50,23.25,42,32.25,"F",null,100,"Rolf ATB PN 210246 Urraco disc. Use 2.25 cross.","2002-03-13","DGR"]
[2.5,50,{"$f":"100/2-14.5-10.5-3.5/2","v":23.25},42,32.25,"F",null,100,"Rolf ATB PN 210668 Dolomite disc. Use 2.25 cross.","2002-12-04","DGR"]
[2.2999999999999998,42,32.75,42,32.75,"F",null,100,"Rolf ATB PN 990034 Propel. Radial, heads out.","2002-02-07","DGR"]
[2.8,39,32.549999999999997,39,32.549999999999997,"F",null,100,"Rolf Road PN 200322 Vector Pro. Radial, heads out.","2002-02-13","DGR"]
[2.5,65,34.6,47,17.8,"R","8,9",130,"Rolf Road PN 200328 Vector Comp. Use 2.29 cross.","2002-04-15","DGR"]
[2.5,42,{"$f":"69.5/2-3.5","v":31.25},42,{"$f":"69.5/2-3.5","v":31.25},"R","8,9",130,"Rolf Road PN 200385 Vector Comp. Radial, heads out.","2002-04-15","DGR"]
[2.2999999999999998,65,34.575000000000003,47,17.75,"R","8,9",130,"Rolf Road PN 210948 Vector. Use 2.25 cross.","2002-02-14","DGR"]
[2.5,38,34.049999999999997,38,34.049999999999997,"F",null,100,"Rolf Road PN 992473 Vector. Radial, heads out.","2002-02-14","DGR"]
[2.5,65,33,47,17.5,"R","8,9",130,"Rolf Road Vector Pro. Use 1.333 cross.","2002-01-27","DGR"]
[2.5,66,39,48,33,"R",1,120,"Rolf Track Vector Pro. Use 1.333 cross.","2002-03-19","DGR"]
[2.6,67,31,67,25,"R",1,110,"Rollex Freecoaster BMX","2001-12-29","www.dtswiss.com"]
[2.8,61,35,61,20,"R",null,135,"Roox Jim Bob","2001-12-29","www.dtswiss.com"]
[2.8,61,25,61,30,"F",null,110,"Roox Jim Bob 99 DH","2001-12-28","www.dtswiss.com"]
[2.8,83,28.5,83,25.5,"R",null,135,"Rotwild Schweizer Loop Inter-4","2001-12-29","www.dtswiss.com"]
[2.4,38.5,28.5,38.5,28.5,"F",null,100,"Sachs 3000, 5000, New Success"]
[2.4,60,25.5,60,24.5,"R",1,118,"Sachs 3-speed coaster "]
[2.4,89,30.5,89,23.5,"R",1,118,"Sachs 3-speed drum brake "]
[2.4,58,26.5,58,24,"R",1,110,"Sachs 3-speed standard "]
[2.4,67,35,67,20,"R",7,135,"Sachs 3X7 Centera, Quarz "]
[2.8,67,34,67,20,"R",7,135,"Sachs 3x7 disc/non-disc","2001-12-29","www.dtswiss.com"]
[2.4,67,37,67,18,"R",7,130,"Sachs 3X7 Original "]
[2.4,58,35,58,20,"R",7,135,"Sachs 3X7 Traxx "]
[2.4,45,31.6,45,19.600000000000001,"R",7,135,"Sachs 7 speed cassette "]
[2.4,45,32.6,45,18.600000000000001,"R",8,135,"Sachs 8 speed cassette "]
[2.4,87,35,87,17,"R",6,null,"Sachs HT3020 drum brake "]
[2.8,105,37,131,23,"R",null,null,"Sachs Inter 12","2001-12-29","www.dtswiss.com"]
[2.4,90,36,90,19,"R",6,126,"Sachs Orbit Drum 6-speed "]
[2.4,90,37.200000000000003,90,17.8,"R",7,130,"Sachs Orbit Drum 7-speed "]
[2.4,67,39,54,18,"R",7,130,"Sachs Orbit MTB 7-speed "]
[2.4,67,38,54,19,"R",null,126,"Sachs Orbit standard 6-speed "]
[2.4,75,29.5,75,28.5,"R",null,122,"Sachs Pentasport coaster "]
[2.4,90,29.5,90,30.5,"R",null,126,"Sachs Pentasport drum "]
[2.4,75,29.6,75,29,"R",null,122,"Sachs Pentasport Std. "]
[2.8,62,35,62,19,"R",null,135,"Sachs Quartz disc","2001-12-29","www.dtswiss.com"]
[2.8,62,20,62,30,"F",null,100,"Sachs Quarz, Neos disc brake hubs"]
[2.4,39,29.6,39,29.6,"F",null,100,"Sachs Quarz, Neos, Centera "]
[2.4,75,35.5,75,33,"R",null,130,"Sachs Super 7 coaster "]
[2.4,75,35.700000000000003,75,34.799999999999997,"R",null,135,"Sachs Super 7 drum "]
[2.4,75,34.5,75,34,"R",null,130,"Sachs Super 7 standard "]
[2.4,45,34.1,45,17.100000000000001,"R",null,126,"Sachs threaded "]
[2.4,45,34.6,45,16.600000000000001,"R",8,130,"Sachs threaded "]
[2.4,39,34,39,34,"F",null,100,"Sachs Traxx "]
[2.4,87,26,87,26,"F",null,100,"Sachs VT3000 drum brake "]
[2.4,90,30,90,26,"F",null,100,"Sachs VT5000 drum brake "]
[2.4,90,37,90,19,"R",7,null,"Sachs VT5000 drum brake "]
[2.4,38,33,38,33,"F",null,100,"Sanshin low flange (like Specialized)"]
[2.4,44.5,35.5,44.5,20,"R",null,126,"Sanshin low flange (like Specialized)"]
[2.4,44.5,33.5,44.5,22,"R",null,130,"Sanshin low flange (like Specialized)"]
[2.4,43,33,43,33,"F",null,100,"Sanshin medium flange (like Specialized)"]
[2.4,46,28,46,22,"R",5,"older","Sanshin medium flange (like Specialized)"]
[2.4,46,33,46,18,"R","6,7","older","Sanshin medium flange (like Specialized)"]
[2.8,62.1,37.700000000000003,62.1,37.700000000000003,"n/a",null,"n/a","Schwinn unicycle hub"]
[2.4,38,{"$f":"74/2+(3.3/2)","v":38.65},38,{"$f":"74/2+(3.3/2)","v":38.65},"F",null,100,"Shimano 105  HB-5501","2003-11-11","dcg"]
[2.6,45,32.5,45,20.5,"R","8,9",130,"Shimano 105 FH-5500","2002-03-05","http://bike.shimano.com/road/105/ComponentTemplate.asp?partnumber=FH-5500"]
[2.6,45,37.299999999999997,45,20.7,"R",7,126,"Shimano 105SC FH-1055 7S"]
[2.6,38,36.299999999999997,38,36.299999999999997,"F",null,100,"Shimano 105SC HB-1055-F"]
[2.6,45,38.200000000000003,45,20.2,"R",7,126,"Shimano 200GS FH-HG20-QR"]
[2.6,45,36.200000000000003,45,22.2,"R",7,130,"Shimano 200GS FH-HG20-QR"]
[2.6,45,36.200000000000003,45,22.2,"R",7,130,"Shimano 400CX FH-C040"]
[2.6,38,36.299999999999997,38,36.299999999999997,"F",null,100,"Shimano 400CX HB-C400"]
[2.6,45,35,45,19,"R",6,126,"Shimano 600 FH-6400 6S","2002-12-03","Jim McKim"]
[2.6,45,37.299999999999997,45,20.7,"R",7,126,"Shimano 600 Ultegra FH-6401 7S"]
[2.6,45,37.1,45,20.9,"R",8,130,"Shimano 600 Ultegra FH-6402 8S"]
[2.6,38,36.299999999999997,38,36.299999999999997,"F",null,100,"Shimano 600 Ultegra HB-6400"]
[2.6,45,35.299999999999997,45,22.7,"R",7,130,"Shimano 700CX FH-C070"]
[2.6,38,36.299999999999997,38,36.299999999999997,"F",null,100,"Shimano 700CX HB-C700"]
[2.6,45,38.1,45,22.5,"R",7,130,"Shimano Acera FH-M290"]
[2.6,45,35.6,45,25,"R",7,135,"Shimano Acera FH-M290"]
[2.6,38,35.799999999999997,38,35.799999999999997,"F",null,100,"Shimano Acera HB-M290"]
[2.6,45,34.5,45,21.5,"R",8,135,"Shimano Alivio FH-MC18AZ","2002-02-28","DCG"]
[2.6,45,38.1,45,22.5,"R",7,130,"Shimano Alivio FH-R050"]
[2.6,45,35.6,45,25,"R",7,135,"Shimano Alivio FH-R050"]
[2.6,45,37.6,45,23,"R",6,126,"Shimano Altus C90 FH-CT90"]
[2.6,45,38.1,45,22.5,"R",6,130,"Shimano Altus C90 FH-CT90"]
[2.6,45,35.6,45,25,"R",7,130,"Shimano Altus C90 FH-CT90"]
[2.6,45,35.6,45,25,"R",7,135,"Shimano Altus C90 FH-CT90"]
[2.6,38,35.799999999999997,38,35.799999999999997,"F",null,"96 or 100","Shimano Altus C90 HB-CT90"]
[2.6,45,38.1,45,22.5,"R","6,7",130,"Shimano Deore DX cassette"]
[2.6,42,34.5,42,34.5,"F",null,100,"Shimano Deore HB-M510"]
[2.6,38,35.799999999999997,38,35.799999999999997,"F",null,100,"Shimano Deore HB-M530","2006-12-02","Knoesen, Scherrit : WM Gerrard <scherrit.knoesen@gerrard.com>"]
[2.6,45,37.9,45,22.7,"R",8,135,"Shimano Deore LX & STX-RC. FH-R080 "]
[2.6,45,37.6,45,23,"R",7,130,"Shimano Deore LX FH-563"]
[2.6,45,35.1,45,25.5,"R",7,135,"Shimano Deore LX FH-563"]
[2.6,45,37.9,45,22.7,"R",8,135,"Shimano Deore LX FH-565"]
[2.6,45,36.799999999999997,45,23.2,"R","8,9",135,"Shimano Deore LX FH-570"]
[2.6,38,35.799999999999997,38,35.799999999999997,"F",null,100,"Shimano Deore LX HB-M563, HB-M564, HB-M570"]
[2.6,45,36.799999999999997,45,23.2,"R",8,135,"Shimano Deore XT FH-M737"]
[2.6,61,32,61,18.5,"R",9,135,"Shimano Deore XT FH-M756L","2003-10-06","barsiantony@hotmail.com"]
[2.6,38,35.799999999999997,38,35.799999999999997,"F",null,100,"Shimano Deore XT HB-M737, HB-M738"]
[2.6,61,21.1,61,31.7,"F",null,100,"Shimano Deore XT HB-M756L","2003-10-06","barsiantony@hotmail.com"]
[2.4,44,{"$f":"(56.9/2)+7.9+(3.3/2)","v":38},44,{"$f":"(56.9/2)-7.9+(3.3/2)","v":22.199999999999996},"R","9,10",130,"Shimano Dura-Ace 10spd 7800","2003-07-30","dcg"]
[2.4,40,{"$f":"37+(3.3/2)","v":38.65},40,{"$f":"37+(3.3/2)","v":38.65},"F",null,100,"Shimano Dura-Ace 7800","2003-07-30","dcg"]
[2.4,44,36.799999999999997,44,23.2,"R",6,126,"Shimano Dura-Ace FH-7400 6S"]
[2.4,44,38.15,44,21.85,"R",7,126,"Shimano Dura-Ace FH-7400 7S"]
[2.4,44,36.9,44,21.1,"R",8,130,"Shimano Dura-Ace FH-7402, 7403 8S"]
[2.4,44,36.9,44,21.1,"R",9,130,"Shimano Dura-Ace FH-7700 9S"]
[2.4,38,37,38,37,"F",null,100,"Shimano Dura-Ace low flange, all"]
[2.4,44,28.95,44,29,"R",1,120,"Shimano Dura-Ace re-spaced to track","2002-03-09","DGR \"New Dura-Ace\" freewheel hub: 1986-ish?"]
[2.6,67,34,67,34,"F",null,100,"Shimano Dura-Ace track high flange"]
[2.6,67,41,67,30,"R",1,120,"Shimano Dura-Ace track high flange"]
[2.4,38,35.799999999999997,38,35.770000000000003,"F",null,100,"Shimano Dura-Ace track small flange","2002-03-03","DGR"]
[2.4,44,37.479999999999997,44,31.71,"R",1,120,"Shimano Dura-Ace track small flange","2002-03-03","DGR"]
[2.6,45,38.200000000000003,45,20.2,"R",7,126,"Shimano Exage FH-HG40, FH-HG50"]
[2.6,45,36.200000000000003,45,22.2,"R",7,130,"Shimano Exage FH-HG40, FH-HG50"]
[2.6,45,33.700000000000003,45,24.7,"R",7,135,"Shimano Exage FH-HG40, FH-HG50"]
[2.6,38,36.299999999999997,38,36.299999999999997,"F",null,100,"Shimano Exage HB-RM50-F, HB-RM50"]
[2.6,45,35.6,45,25,"R",8,135,"Shimano FH-RM40-8","2002-02-28","DCG"]
[2.5,80,28,80,28,"F",null,100,"Shimano HB-NX30 hubdynamo"]
[2.8,80,29,80,29,"F",null,100,"Shimano Inter-L hub dynamo ","2001-12-28","www.dtswiss.com"]
[2.8,52,25,52,33,"F",null,100,"Shimano Nexave","2001-12-28","www.dtswiss.com"]
[2.8,45,30,45,21,"R",null,135,"Shimano Nexave","2001-12-29","www.dtswiss.com"]
[2.6,87,29.225000000000001,87,25.375,"R",7,130,"Shimano Nexus SG-7R45 7SPD INTER-7 ROLLER BRAKE","2002-05-07","DCG"]
[2.6,84,31.15,84,23.45,"R",1,123.5,"Shimano Nexus 4S coaster brake SG-4C30"]
[2.6,84,27.7,84,33.549999999999997,"R",1,123.5,"Shimano Nexus 4S roller brake SG-4R31"]
[2.6,87,29.73,87,24.7,"R",1,127,"Shimano Nexus 7S coaster brake SG-7C21"]
[2.6,87,31.15,87,23.45,"R",1,130,"Shimano Nexus 7S roller brake SG-7R40"]
[2.6,52,26,52,33,"F",null,100,"Shimano Nexus HB-IM40 front, roller brake"]
[2.5,80,23.2,80,28.8,"F",null,100,"Shimano Nexus HB-NX70 Disc hubdynamo","2006-12-02","Shimano's web site"]
[2.6,92.6,29.3,92.6,24.9,"R",1,132,"Shimano Nexus Inter-8 8-speed internal","2003-10-06","CaptBike@sheldonbrown.com"]
[2.6,92.6,{"$f":"31.85-3.2/2","v":30.25},92.6,{"$f":"26.45-3.2/2","v":24.849999999999998},"R",1,null,"Shimano Nexus Inter-8 8-speed internal SG-8R20","2004-01-22","CaptBike@sheldonbrown.com"]
[2.6,92.6,32.9,92.6,21.3,"R",1,125,"Shimano Nexus Inter-8 8-speed internal without roller brake locknut","2003-10-06","CaptBike@sheldonbrown.com"]
[2.5,80,28.5,80,28.5,"F",null,100,"Shimano Nexus Inter-L HB-NX30 hub dynamo","2001-10-11","Martin Staines <mstaines@superform-aluminium.com>"]
[2.6,74,30,74,30,"F",null,100,"Shimano Nexus Sport DH-3N70 hub dynamo","2005-11-05","shimano.com"]
[2.6,74,{"$f":"52.3/2-3.85","v":22.299999999999997},74,{"$f":"52.3/2+3.85","v":30},"F",null,100,"Shimano Nexus Sport DH-3D70 hub dynamo (disc brake)","2005-11-05","shimano.com"]
[2.6,38,34.5,38,34.5,"F",null,100,"Shimano parallax "]
[2.6,45,37.5,45,20.7,"R",7,126,"Shimano RSX FH-A410"]
[2.6,45,36,45,22.2,"R",7,130,"Shimano RSX FH-A410"]
[2.6,45,{"$f":"135/2-34.17+2.5","v":35.83},45,{"$f":"135/2-46.16-2.5","v":18.840000000000003},"R","8,9",130,"Shimano RSX FH-A416","2002-09-29","DGR"]
[2.6,45,{"$f":"135/2-34.17","v":33.33},45,{"$f":"135/2-46.16","v":21.340000000000003},"R","8,9",135,"Shimano RSX FH-A416, respaced from 130mm to 135","2002-09-29","DGR"]
[2.6,38,36.299999999999997,38,36.299999999999997,"F",null,100,"Shimano RSX HB-A410"]
[2.6,45,37.299999999999997,45,20.7,"R",7,126,"Shimano RX100 FH-A550"]
[2.6,38,36.299999999999997,38,36.299999999999997,"F",null,100,"Shimano RX100 HB-A550-F"]
[2.6,45,36.799999999999997,45,20.2,"R",7,126,"Shimano Santé"]
[2.6,45,35.5,45,35.5,"F",null,100,"Shimano Santé "]
[2.6,45,38.1,45,22.5,"R",7,130,"Shimano STX FH-MC32"]
[2.6,45,35.6,45,25,"R",7,135,"Shimano STX FH-MC32"]
[2.6,45,38.1,45,22.5,"R",7,130,"Shimano STX FH-R050"]
[2.6,45,35.6,45,25,"R",7,135,"Shimano STX FH-R050"]
[2.6,38,35.799999999999997,38,35.799999999999997,"F",null,100,"Shimano STX HB-MC32"]
[2.6,45,38.1,45,22.5,"R",7,130,"Shimano STX-RC FH-MC33"]
[2.6,45,35.6,45,25,"R",7,135,"Shimano STX-RC FH-MC33"]
[2.6,38,35.799999999999997,38,35.799999999999997,"F",null,100,"Shimano STX-RC. HB-MC33-S, HB-MC33"]
[2.6,63,28,63,22,"R",8,145,"Shimano tandem FH-FH08"]
[2.6,63,35,63,35,"F",null,100,"Shimano tandem HB-HF08"]
[2.4,44,38,44,18,"R","8,9",130,"Shimano Ultegra 9 spd FH-6500","2003-08-03","dcg"]
[2.5,74,28.5,74,28.5,"F",null,100,"Shimano Ultegra DH-2N70 hub dynamo","2005-03-23","info@m-gineering.nl"]
[2.6,45,37.1,45,20.9,"R",9,130,"Shimano Ultegra FH-6500 9S"]
[2.6,38,36.299999999999997,38,36.299999999999997,"F",null,100,"Shimano Ultegra HB-6500"]
[2.4,38,{"$f":"37+(3.3/2)","v":38.65},38,{"$f":"37+(3.3/2)","v":38.65},"F",null,100,"Shimano Ultegra HB-6500A","2003-08-03","dcg"]
[2.6,61,22,61,33,"F",null,100,"Shimano XT Disc"]
[2.6,61,34,61,19,"R",9,135,"Shimano XT Disc"]
[2.6,45,{"$f":"(58.4/2)+6.15+(3.3/2)","v":37},45,{"$f":"(58.4/2)-6.15+(3.3/2)","v":24.699999999999996},"R","8,9",135,"Shimano XT Disc FH-M756","2003-08-06","dcg"]
[2.6,44,{"$f":"(60.6/2)-5.5+(3.3/2)","v":26.45},38,{"$f":"(60.6/2)+5.5+(3.3/2)","v":37.449999999999996},"F",null,100,"Shimano XT Disc HB-M765","2003-08-06","dcg"]
[2.6,45,34.5,45,21,"R","8,9",135,"Shimano XT FH-M750","2003-08-06","dcg"]
[2.6,45,37.549999999999997,45,21.75,"R","8,9",135,"Shimano XT FH-M760","2005-11-05","shimano.com"]
[2.6,38,35.5,38,35.5,"F",null,100,"Shimano XT HB-M751","2003-08-06","dcg"]
[2.6,38,35,38,35,"F",null,100,"Shimano XT HB-M753","2004-12-11","Thad Ross"]
[2.6,44,37,44,21,"R",9,135,"Shimano XT FH-M752","2004-12-11","Thad Ross"]
[2.6,38,34.15,38,34.15,"F",null,100,"Shimano XT HB-M760","2003-08-06","dcg"]
[2.6,38,35.799999999999997,38,35.799999999999997,"F",null,100,"Shimano XT-II, DX"]
[2.6,45,35.6,45,25,"R","6,7",135,"Shimano XT-II, DX"]
[2.6,45,36.799999999999997,45,23.2,"R","8,9",135,"Shimano XTR FH-M950","2002-11-21","www.shimano.com says 26.8; Kent says 36.8"]
[2.6,45,{"$f":"58.4/2+6.15","v":35.35},45,{"$f":"58.4/2-6.15","v":23.049999999999997},"R","8,9",135,"Shimano XTR FH-M965 Disc","2002-06-18","Shimano 2002/03 Products & Features book"]
[2.6,38,35.799999999999997,38,35.799999999999997,"F",null,100,"Shimano XTR HB-M950"]
[2.6,43.4,{"$f":"60.6/2-5.5","v":24.8},38,{"$f":"60.6/2+5.5","v":35.799999999999997},"F",null,100,"Shimano XTR HB-M965 Disc","2002-06-18","Shimano 2002/03 Products & Features book"]
[2.8,40,30,40,30,"F",null,100,"Shogun Little Sumo","2001-12-28","www.dtswiss.com"]
[2.6,46,33,46,33,"F",null,100,"Shogun Zero Carbon","2001-12-28","www.dtswiss.com"]
[2.5,70,30,70,30,"F",null,100,"SON 20-28\" hubdynamo (2000 model) "]
[2.5,70,21.5,70,30,"F",null,100,"SON 20-28\" hubdynamo-disc brake (2000 model)"]
[2.4,38,33,38,33,"F",null,100,"Specialized low flange "]
[2.4,44.5,35.5,44.5,20,"R",null,126,"Specialized low flange "]
[2.4,44.5,33.5,44.5,22,"R",null,130,"Specialized low flange "]
[2.4,43,33,43,33,"F",null,100,"Specialized medium flange "]
[2.4,46,28,46,22,"R",null,"old","Specialized medium flange "]
[2.4,46,33,46,18,"R",null,"older","Specialized medium flange "]
[2.2999999999999998,36,34.799999999999997,36,34.799999999999997,"F",null,100,"Specialized skraxle by DT","2001-12-28","www.dtswiss.com"]
[2.6,45,37,45,37,"F",null,100,"Specialized Stout","2001-12-28","www.dtswiss.com"]
[2.2999999999999998,36,34.799999999999997,36,34.799999999999997,"F",null,100,"Specialized Y2K by DT","2001-12-28","www.dtswiss.com"]
[2.4,45,37.700000000000003,45,16.7,"R",null,130,"Specialized Y2K by DT","2001-12-29","www.dtswiss.com"]
[2.4,45,35.200000000000003,45,19.2,"R",null,135,"Specialized Y2K by DT","2001-12-29","www.dtswiss.com"]
[2.5,38,38,54,18,"R",null,130,"Speed Tec","2001-12-29","www.dtswiss.com"]
[2.5,54,20,54,32,"F",null,100,"Speed Tec disc","2001-12-28","www.dtswiss.com"]
[2.5,54,34,54,18,"R",null,135,"Speed Tec disc","2001-12-29","www.dtswiss.com"]
[2.6,48,35,48,35,"F",null,100,"Spot Single Speed","2001-12-28","www.dtswiss.com"]
[2.6,48,42,48,41,"R",1,135,"Spot single speed","2001-12-29","www.dtswiss.com"]
[2.6,40,34.299999999999997,40,34.299999999999997,"F",null,100,"SR sealed bearing","2004-03-07","DGR"]
[2.5,39,29.6,39,29.6,"F",null,100,"SRAM 2001 non-disc hubs"]
[2.5,45,30.7,45,20.5,"R",9,135,"SRAM 2001 non-disc hubs"]
[3,75,29,75,29,"R",1,123,"SRAM 5 speed hub MH 5205 w/no brake"]
[3,75,39.5,75,28.5,"R",1,122,"SRAM 5 speed hub MH 5215 w/coaster brake"]
[3,90,29.5,90,30.5,"R",1,126,"SRAM 5 speed hub MH 5225 w/drum brake"]
[2.6,39,30,39,30,"F",null,100,"SRAM 9.0","2001-12-28","www.dtswiss.com"]
[2.5,45,22.95,45,27.75,"F",null,100,"SRAM 9.0SL disc"]
[2.5,45,30.7,45,20.5,"R",9,135,"SRAM 9.0SL, Disc"]
[2.6,67,33,67,18,"R","8,9",null,"SRAM Dual Drive 27/24","2001-12-29","www.dtswiss.com"]
[2.6,67,33,67,18,"R","8,9",null,"SRAM Dual Drive 27/24 disc brake","2001-12-29","www.dtswiss.com"]
[2.6,67,33,67,18,"R","8,9",null,"SRAM Dual Drive 27/24 I-brake","2001-12-29","www.dtswiss.com"]
[2.6,93.6,26.5,93.6,31.5,"R",1,135,"SRAM i-Motion 9 Gearhub (with back pedal brake)","2006-12-02","Sheldon Brown <CaptBike@sheldonbrown.com>"]
[2.5,45,27.4,45,23.8,"R",7,135,"SRAM Neos, Centera"]
[2.5,45,29.9,45,21.3,"R",7,130,"SRAM Neos, Centera, Traax"]
[2.5,45,30.4,45,20.8,"R",8,135,"SRAM Plasma, Quartz, Neos, Centera"]
[2.5,39,29.6,39,29.6,"F",null,100,"SRAM Plasma, Quartz, Neos, Centera, Traax"]
[2.5,62.5,30.4,62.5,20.8,"R",8,135,"SRAM Power Disc: Plasma, Quartz"]
[2.5,62.5,32.9,62.5,18.3,"R",8,130,"SRAM Power Disc: Quartz"]
[2.5,45,32.9,45,18.3,"R",8,130,"SRAM Quartz, Neos, Centera"]
[2.9,194,27.5,194,27.5,"R",null,null,"SRAM Sparc","2001-12-29","www.dtswiss.com"]
[2.6,105,37.9,132,20.7,"R",1,135,"SRAM Spectro 12 speed hub with coaster brake"]
[3,58,25.5,58,24.5,"R",1,117,"SRAM Spectro 3 speed hum MH 3115 w/no brake"]
[3,58,25.5,58,24.5,"R",1,118,"SRAM Spectro 3 speed hum MH 3125 w/coaster brake"]
[3,89,32.5,89,25.5,"R",1,118,"SRAM Spectro 3 speed hum MH 3125 w/drum brake"]
[2.6,67,35,67,20,"R",7,135,"SRAM Spectro 3x7: 3s hub with 7s cassette"]
[3,75,34.5,75,34,"R",1,132,"SRAM Spectro 7 speed hub MH 7205 w/no brake"]
[3,75,34,75,33,"R",1,130,"SRAM Spectro 7 speed hub MH 7215 w/coaster brake"]
[3,90,35.700000000000003,90,34.799999999999997,"R",1,135,"SRAM Spectro 7 speed hub MH 7225 w/drum brake"]
[2.5,45,30.8,45,20.399999999999999,"R",7,130,"SRAM Traax"]
[2.4,65,27,65,27,"R",1,null,"Sturmey-Archer 3 spd "]
[2.4,102.5,27,42.5,27,"F",null,100,"Sturmey-Archer dyno "]
[2.4,101,40,65,25.5,"R",null,null,"Sturmey-Archer dyno "]
[2.4,90,41.5,90,18.5,"R",null,null,"Sturmey-Archer Elite ST drum "]
[2.4,90,27,90,27,"F",null,100,"Sturmey-Archer hi brake "]
[2.4,82,40,82,20,"R",null,null,"Sturmey-Archer hi brake "]
[2.4,45,37.15,45,19.7,"R",null,135,"Sunn by DT Swiss","2001-12-29","www.dtswiss.com"]
[2.4,52,34,52,21,"R",8,135,"Sun-Ringlé 439/439 Lite"]
[2.4,54.5,35.5,54.5,20.5,"R",8,135,"Sun-Ringlé ABBAH / Lawwill DH (12mm thru axle)"]
[2.6,59.5,24.5,54.5,35.5,"F",null,110,"Sun-Ringlé ABBAH S.O.S. DH (20mm thru axle)","2001-12-28","www.dtswiss.com"]
[2.6,59.5,34.5,59.5,21,"R",8,135,"Sun-Ringlé ABBAH S.O.S. XC","2001-12-29","www.dtswiss.com"]
[2.6,59.5,21,45.5,35,"F",null,100,"Sun-Ringlé ABBAH S.O.S. XC (9mm axle ends)"]
[2.6,51,32.1,51,32.1,"F",null,"95?","Sun-Ringlé Atilla the Hub","2001-12-29","www.sun-ringle.com"]
[2.6,51,37.1,51,30.2,"R",1,110,"Sun-Ringlé Attila the hub (BMX)","2001-12-29","www.sun-ringle.com"]
[2.4,46,34,46,34,"F",null,100,"Sun-Ringlé SuperDuper Bubba "]
[2.4,44.5,32,44.5,22,"R",7,135,"Suntour 7 spd 135mm cass "]
[2.4,39,33,39,33,"F",null,100,"Suntour GPX"]
[2.4,67,33,67,33,"F",null,100,"Suntour high flange track "]
[2.4,67,36,67,30,"R",1,120,"Suntour high flange track "]
[2.4,44.5,35.5,44.5,20,"R",null,126,"Suntour low flange "]
[2.4,44.5,31.5,44.5,24,"R",null,135,"Suntour low flange "]
[2.4,44.5,31,44.5,20.5,"R",7,135,"Suntour micro drive 7 spd "]
[2.4,44.5,33.5,44.5,21.5,"R",8,135,"Suntour micro drive 8 spd "]
[2.5,36,34,36,34,"F",null,100,"Suntour Microlight","2001-12-28","www.dtswiss.com"]
[2.4,39,33,39,33,"F",null,100,"Suntour Sprint"]
[2.4,44,36,44,19,"R",7,126,"Suntour Sprint low flange"]
[2.4,44.5,36,44.5,19,"R",7,126,"Suntour Superbe low flange"]
[2.4,39,33,39,33,"F",null,100,"Suntour Superbe Pro"]
[2.4,44.5,37,44.5,17,"R",8,130,"Suntour Superbe Pro cassette"]
[2.4,39,33,39,33,"F",null,100,"Suntour XC-9000"]
[2.4,45,34,45,21,"R",7,130,"Suntour XC-9000, XCD6000, XCD9000"]
[2.4,36,33,36,33,"F",null,100,"Suntour XCD-6000"]
[2.4,58,22.5,58,32,"F",null,100,"Surly \"New\" disc","2004-11-13","http://www.surlybikes.com/spew8.html"]
[2.4,58,34,58,38.5,"R",1,135,"Surly \"New\" disc","2004-11-13","http://www.surlybikes.com/spew8.html"]
[2.4,54,38.4,54,38.4,"R",1,135,"Surly \"New\" single speed MTB hub","2004-11-13","http://www.surlybikes.com/spew8.html"]
[2.4,54,32.200000000000003,54,32.200000000000003,"F",null,100,"Surly \"New\" track hub","2004-11-13","http://www.surlybikes.com/spew8.html"]
[2.4,54,30.1,54,30.1,"R",1,120,"Surly \"New\" track hub","2004-11-13","http://www.surlybikes.com/spew8.html"]
[2.4,43,33,43,33,"F",null,100,"Surly 1x1","2004-11-13","http://www.surlybikes.com/spew8.html"]
[2.4,43,39,43,39,"R",1,135,"Surly 1x1 single speed","2004-11-13","http://www.surlybikes.com/spew8.html"]
[2.6,62,31,62,31,"F",null,100,"Suzue front high flange","2001-12-28","www.dtswiss.com"]
[2.4,62.5,31.3,62.5,31.3,"F",null,100,"Suzue Sil-SP","2004-02-18","Jon Senior <jon@restlesslemon.co.uk>"]
[2.4,62.5,27.3,62.5,27.3,"R",1,120,"Suzue Sil-SP","2004-02-18","Jon Senior <jon@restlesslemon.co.uk>"]
[2.5,63,27,63,27,"R",null,null,"Suzue Tandem"]
[2.6,63.9,30.55,63.9,30.55,"n/a",null,"n/a","Suzue unicycle hub"]
[2.4,59.8,22.1,39.799999999999997,34.299999999999997,"F",null,100,"Syncros disc brake "]
[2.4,39.799999999999997,34.299999999999997,39.799999999999997,34.299999999999997,"F",null,100,"Syncros Hardcore"]
[2.4,32,35,45,18,"R",8,130,"TNT 8-speed "]
[2.4,32,35,45,22,"R",8,135,"TNT 8-speed "]
[2.4,32,37.5,32,37.5,"F",null,100,"TNT standard"]
[2.4,42,39,42,39,"F",null,100,"TNT suspension"]
[2.4,45,33,45,19,"R",8,135,"TNT suspension 8-speed "]
[2.6,41,35,41,35,"F",null,100,"Tomo","2001-12-28","www.dtswiss.com"]
[2.4,61,23.6,45,31.9,"F",null,100,"TruVative Disc Sealex SL FH-DISCX-SL-00",null,"www.truvative.com"]
[2.4,61,34.1,61,19.2,"R","8,9",135,"TruVative Sealex SL Disc RH-DISCX-SL-00",null,"www.truvativ.com"]
[2.4,38,34,38,34,"F",null,100,"TruVative Sealex SL FH-SEAL-SL-00",null,"www.truvative.com"]
[2.4,45,32,61,19.5,"R","8,9",135,"TruVative Sealex SL RH-SEAL-SL-00",null,"www.truvativ.com"]
[2.4,38,34,38,34,"F",null,100,"TruVative Sealex XR FH-SEAL-XR-00",null,"www.truvative.com"]
[2.4,45,32,61,19.5,"R","8,9",135,"TruVative Sealex XR RH-SEAL-XR-00",null,"www.truvativ.com"]
[2.5,56,22,56,35,"F",null,100,"Tune King disc 2000","2001-12-28","www.dtswiss.com"]
[2.5,56,19,56,34,"F",null,110,"Tune King disc 99 DH","2001-12-28","www.dtswiss.com"]
[2.4,59,20,59,31,"F",null,100,"Tune King Gustav M 99","2001-12-28","www.dtswiss.com"]
[2.4,59,31,59,20,"R",null,135,"Tune King Gustav M 99","2001-12-29","www.dtswiss.com"]
[2.5,56,24,56,35,"F",null,100,"Tune King Louise 99","2001-12-28","www.dtswiss.com"]
[2.5,55.5,25,55.5,34,"F",null,110,"Tune King MK disc 99 DH","2001-12-28","www.dtswiss.com"]
[2.5,56,36,56,20,"R",null,135,"Tune Kong disc","2001-12-29","www.dtswiss.com"]
[2.5,56,31,56,20,"R",null,135,"Tune Kong Louise 99","2001-12-29","www.dtswiss.com"]
[2.4,41,39,54,17,"R",8,130,"Tune MAG180/200/215  183,205,225gr"]
[2.4,41,37,54,20,"R",8,135,"Tune MAG180/200/215  183,205,225gr"]
[2.2999999999999998,35.6,34,35.6,34,"F",null,100,"Tune MIG 66 74gr"]
[2.5,36,36,36,36,"F",null,100,"Tune MIG 75","2001-12-28","www.dtswiss.com"]
[2.4,78,36.200000000000003,66,16.7,"R","8,9",130,"Tune Power Tap Prologue"]
[2.5,51.6,42,51.6,42,"F",null,100,"Tune SandWitch","2001-12-28","www.dtswiss.com"]
[2.2999999999999998,32,34,32,34,"F",null,100,"Ultimate Machine Co. road"]
[2.2999999999999998,32,34,43.5,21,"R",8,130,"Ultimate Machine Co., small left flange"]
[2.2999999999999998,43.5,34,43.5,21,"R",8,130,"Ultimate Machine Co., two equal flange diameters"]
[2.6,81,28,81,28,"F",null,null,"Union/Marwi WingIII","2001-12-28","www.dtswiss.com"]
[2.4,44,32,44,32,"R",null,null,"Wheelring wheelchair"]
[2.4,38,40,38,40,"F",null,100,"Wheelsmith Bullet "]
[2.4,44,35,44,20,"R",null,130,"Wheelsmith Bullet cass. "]
[2.4,54,34.299999999999997,54,20.100000000000001,"R",8,130,"White Industries cassette"]
[2.5,{"$f":"41-4","v":37},{"$f":"130/2-29","v":36},{"$f":"58.5-4","v":54.5},{"$f":"130/2-46.28","v":18.72},"R",9,130,"White Industries LTA cassette","2004-12-26","DGR"]
[2.4,54,34.5,54,21.5,"R",null,135,"White Industries cassette"]
[2.6,74,21,74,32,"F",null,100,"White Industries disc","2001-12-28","www.dtswiss.com"]
[2.5,48,32,48,32,"R",1,"126, 130, 135","White Industries ENO eccentric flip-flop","2003-04-17","CaptBike@sheldonbrown.com"]
[2.6,67,36,67,21,"R",null,135,"White Industries Hayes disc","2001-12-29","www.dtswiss.com"]
[2.6,75,22,75,35,"F",null,110,"White Industries Hayes disc DH","2001-12-28","www.dtswiss.com"]
[2.2999999999999998,34,38,34,38,"F",null,100,"White Industries road"]
[2.4,34,35.5,34,35.5,"F",null,100,"White Industries Ti "]
[2.4,54,29.5,54,24.5,"R",6,126,"White Industries Ti "]
[2.4,54,37,54,19,"R",7,126,"White Industries Ti "]
[2.4,54,27,54,27,"R",6,130,"White Industries Ti "]
[2.4,54,32,54,22,"R",7,130,"White Industries Ti "]
[2.4,54,36,54,18,"R",8,130,"White Industries Ti "]
[2.4,54,29,54,25,"R",7,135,"White Industries Ti "]
[2.4,54,34,54,20,"R",8,135,"White Industries Ti "]
[2.4,40,35.5,40,35.5,"F",null,100,"White Industries Tracker "]
[2.4,59,27,59,27,"R",7,136,"Wilderness Trails"]
[2.4,59,24.5,59,29.5,"R",7,141,"Wilderness Trails"]
[2.4,47,36,47,36,"F",null,100,"Wilderness Trails classic narrow "]
[2.4,47,39,47,39,"F",null,100,"Wilderness Trails classic standard "]
[2.4,47,45,47,45,"F",null,100,"Wilderness Trails classic wide "]
[2.4,40,34.5,40,34.5,"F",null,100,"Wilderness Trails Momentum "]
[2.4,45,39,45,39,"F",null,100,"Wilderness Trails New Paradigm large flange"]
[2.4,42.5,39,42.5,39,"F",null,100,"Wilderness Trails New Paradigm small flange"]
[2.4,36,35,36,35,"F",null,100,"Winners lo flange "]
[2.4,41.5,36,41.5,20.5,"R",null,135,"Winners low flange "]
[2.5,58,16,58,35,"F",null,null,"Woodman Bill LFY for Cannondale Lefty fork","2002-03-04","woodmanusa@earthlink.net"]
[2.4,59,30,59,25,"R",7,131,"WTB classic WTB 7 "]
[2.4,59,28,59,27,"R",7,136,"WTB classic WTB 7 "]
[2.4,59,31.5,59,23.5,"R",8,136,"WTB classic WTB 8 "]
[2.4,59,27.5,59,27.5,"R",8,141,"WTB classic WTB 8 "]
[2.4,45,31,45,25,"R",7,135,"WTB New Paradigm 7-speed cassette "]
[2.4,45,38.5,45,27.5,"R",7,140,"WTB New Paradigm 7-speed cassette "]
[2.4,45,33,45,23,"R",8,136,"WTB New Paradigm 8-speed cassette "]
[2.4,45,35,45,21,"R",8,139,"WTB New Paradigm 8-speed cassette "]
[2.6,44,35.299999999999997,37,19.100000000000001,"R","8,9",130,"Xero Lite 16H","2004-02-08","DGR"]
[2.8,38,35,38,35,"F",null,100,"XS BMX","2001-12-28","www.dtswiss.com"]
[2.8,45,27,45,27,"R",1,110,"XS BMX","2001-12-29","www.dtswiss.com"]
[2.8,63,33,63,33,"F",null,100,"XS BMX high flange","2001-12-28","www.dtswiss.com"]
[2.8,63,29,63,29,"R",1,110,"XS BMX high flange","2001-12-29","www.dtswiss.com"]
[2.4,43,35,43,20,"R",8,130,"Zipp "]
[2.2999999999999998,43,36,43,36,"F",null,100,"Zipp 100"]
[2.2999999999999998,43,37,43,20,"R",8,130,"Zipp 217"]
[2.4,58,33.700000000000003,58,33.700000000000003,"F",1,{"$f":"100-12","v":88},"YuHub MA-01F custom freewheel unicycle hub design. 32/36h, 100c-c, 158 overall.","2019-06-24","MFA"]